{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":214,"macros":1,"external_links":0,"defined_names":2,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":1721,"n_cols":12,"rows_kept":1721,"cut":false,"hidden":false,"merged":[[93,3,93,6],[1706,4,1706,6],[1487,4,1487,6],[1498,4,1498,6],[1499,4,1499,6],[1500,4,1500,6],[1501,4,1501,6],[1502,4,1502,6],[1503,4,1503,6],[1482,4,1482,5],[1483,4,1483,5],[1484,4,1484,5],[1485,4,1485,5],[1486,4,1486,6],[1694,3,1694,6],[1127,2,1127,3],[1071,3,1071,6],[1072,3,1072,6],[1073,3,1073,6],[1074,3,1074,6],[1075,3,1075,6],[1084,3,1084,4],[1083,3,1083,4],[878,2,878,3],[950,3,953,3],[281,3,281,5],[655,2,655,4],[850,6,857,6],[857,3,857,5],[851,3,851,5],[945,3,945,6],[1080,1,1080,8],[1071,7,1079,7],[1081,3,1081,4],[1082,3,1082,4],[1082,7,1090,7],[1104,3,1104,4],[1076,3,1076,6],[1088,5,1088,6],[1091,3,1091,6],[1490,2,1490,3],[1484,2,1484,3],[1485,2,1485,3],[1486,2,1486,3],[1452,1,1452,8],[1393,1,1393,8],[1113,2,1113,3],[1113,4,1113,5],[1113,7,1118,7],[1114,2,1114,3],[1114,4,1114,5],[1488,2,1488,3],[1489,2,1489,3],[1149,2,1149,5],[1105,3,1105,4],[1119,2,1119,3],[1119,4,1119,5],[1144,4,1144,5],[1145,4,1145,5],[1120,4,1120,5],[1118,2,1118,3],[1118,4,1118,5],[1108,7,1109,7],[1111,1,1111,8],[1513,4,1513,6],[981,7,982,7],[988,3,988,4],[1109,3,1109,4],[1110,3,1110,4],[1112,2,1112,3],[1112,4,1112,5],[1144,6,1145,6],[1145,2,1145,3],[1146,2,1146,3],[1146,6,1147,6],[1144,2,1144,3],[1116,2,1116,3],[1116,4,1116,5],[1117,2,1117,3],[1117,4,1117,5],[987,1,987,8],[994,3,994,4],[1085,5,1085,6],[1086,5,1086,6],[1002,7,1005,7],[1003,3,1003,4],[1004,3,1004,4],[1005,3,1005,4],[989,3,989,4],[990,3,990,4],[1085,3,1085,4],[1086,3,1086,4],[1087,3,1087,4],[991,3,991,4],[995,3,995,4],[996,3,996,4],[962,1,962,8],[974,7,975,7],[967,2,967,4],[968,2,968,4],[968,5,968,6],[970,3,970,6],[954,4,957,4],[1000,1,1000,8],[6,11,7,11],[1526,4,1526,6],[1527,4,1527,6],[1528,4,1528,6],[1529,4,1529,6],[1530,4,1530,6],[1488,4,1488,6],[1489,4,1489,6],[1490,4,1490,6],[1477,2,1477,3],[1478,2,1478,3],[1479,2,1479,3],[1480,2,1480,3],[1481,2,1481,3],[1477,4,1477,5],[1478,4,1478,5],[1479,4,1479,5],[1480,4,1480,5],[1481,4,1481,5],[1482,2,1482,3],[1483,2,1483,3],[1487,2,1487,3],[1120,2,1120,3],[1129,2,1129,3],[716,3,716,4],[717,3,717,4],[718,3,718,4],[719,3,719,4],[720,3,720,4],[159,5,159,6],[160,4,161,4],[673,3,673,5],[656,2,656,4],[657,2,657,4],[664,3,664,4],[651,2,651,4],[253,2,254,2],[253,3,254,3],[253,4,254,4],[253,5,254,5],[439,2,440,2],[388,2,389,2],[388,3,389,3],[397,2,399,2],[400,2,401,2],[283,3,283,4],[444,1,444,8],[645,2,645,4],[646,2,646,4],[965,2,965,4],[943,3,943,6],[944,3,944,6],[936,4,936,6],[579,3,579,6],[532,1,533,1],[532,2,533,2],[572,3,572,6],[573,3,573,6],[574,3,574,6],[934,2,934,3],[902,6,906,6],[913,2,913,3],[742,1,742,8],[710,1,710,8],[674,1,674,8],[661,1,661,8],[633,1,633,8],[627,1,627,8],[938,2,938,3],[937,4,937,6],[938,4,938,6],[894,2,894,3],[935,2,935,3],[939,4,939,6],[940,4,940,6],[937,2,937,3],[675,3,675,4],[711,3,711,4],[712,3,712,4],[713,3,713,4],[714,3,714,4],[936,2,936,3],[934,4,934,6],[935,4,935,6],[580,1,580,8],[872,7,875,7],[858,3,858,6],[862,3,862,6],[863,7,870,7],[993,3,993,4],[261,5,267,5],[963,2,963,4],[964,2,964,4],[441,1,441,8],[875,3,875,5],[871,3,871,6],[872,3,872,5],[861,3,861,6],[863,3,863,6],[913,6,914,6],[445,2,445,3],[445,4,445,5],[446,2,446,3],[446,4,446,5],[446,7,448,7],[887,4,887,5],[888,4,888,5],[889,4,889,5],[876,1,876,8],[954,5,955,5],[954,6,955,6],[958,6,959,6],[966,2,966,4],[877,2,877,3],[877,4,877,6],[867,3,867,6],[868,3,868,6],[869,3,869,6],[870,3,870,6],[948,1,948,8],[932,1,932,8],[933,2,933,3],[893,2,893,3],[887,2,887,3],[950,7,953,7],[952,5,953,5],[952,6,953,6],[891,2,891,3],[892,2,892,3],[941,4,941,6],[942,4,942,6],[886,1,886,8],[873,3,873,5],[874,3,874,5],[921,1,921,8],[941,2,941,3],[942,2,942,3],[909,2,909,3],[910,2,910,3],[911,2,911,3],[912,2,912,3],[897,4,897,5],[898,4,898,5],[899,4,899,5],[896,2,896,3],[647,2,647,4],[652,2,652,4],[662,3,662,4],[649,2,649,4],[650,2,650,4],[729,3,729,4],[730,3,730,4],[731,3,731,4],[609,3,612,3],[653,2,653,4],[654,2,654,4],[659,2,659,4],[670,3,670,4],[671,3,671,4],[672,3,672,5],[253,7,254,7],[150,5,150,6],[155,5,155,6],[388,4,388,5],[388,7,389,7],[442,2,442,3],[443,2,443,3],[404,2,409,2],[410,2,415,2],[566,3,566,6],[448,4,448,5],[260,7,268,7],[275,3,275,5],[276,3,276,5],[278,3,278,5],[279,3,279,5],[280,3,280,5],[388,1,389,1],[852,3,852,5],[853,3,853,5],[854,3,854,5],[840,3,840,6],[816,6,817,6],[978,7,980,7],[974,3,974,6],[975,3,975,6],[976,3,976,6],[977,3,977,6],[978,3,978,6],[979,3,979,6],[980,3,980,6],[960,6,961,6],[958,7,961,7],[960,5,961,5],[950,5,951,5],[950,6,951,6],[971,7,973,7],[969,1,969,8],[973,3,973,6],[888,7,893,7],[888,2,888,3],[889,2,889,3],[890,4,890,5],[891,4,891,5],[900,1,900,8],[644,2,644,4],[971,3,971,6],[972,3,972,6],[956,6,957,6],[958,3,961,3],[958,4,961,4],[958,5,959,5],[394,2,396,2],[199,7,203,7],[206,7,221,7],[210,5,221,5],[223,7,239,7],[323,7,324,7],[325,7,330,7],[416,2,426,2],[427,2,429,2],[430,2,434,2],[333,2,334,2],[333,7,334,7],[663,3,663,4],[954,7,957,7],[956,5,957,5],[892,4,892,5],[939,2,939,3],[940,2,940,3],[946,3,946,6],[947,3,947,6],[602,7,608,7],[639,2,639,4],[640,2,640,4],[641,2,641,4],[642,2,642,4],[643,2,643,4],[356,3,357,3],[356,4,356,5],[356,7,357,7],[6,2,6,5],[6,7,6,8],[0,2,0,6],[1,2,1,6],[2,2,2,6],[3,2,3,8],[4,1,4,8],[5,1,5,2],[9,1,10,1],[9,2,10,2],[9,3,10,3],[7,2,7,8],[8,1,8,8],[9,8,10,8],[72,8,73,8],[71,1,71,8],[11,7,70,7],[68,3,68,6],[69,3,69,6],[70,3,70,6],[72,1,73,1],[72,2,73,2],[72,3,73,3],[72,6,73,6],[72,7,73,7],[9,7,10,7],[9,6,10,6],[5,3,5,5],[5,6,5,8],[74,6,75,6],[74,7,75,7],[76,2,76,3],[79,1,79,8],[94,1,94,8],[175,1,175,8],[192,1,192,8],[204,1,204,8],[274,1,274,8],[287,1,287,8],[282,1,282,8],[310,1,310,8],[332,1,332,8],[124,3,124,6],[125,3,125,6],[284,3,285,4],[95,2,96,2],[176,2,177,2],[176,3,177,3],[176,4,177,4],[176,7,177,7],[141,3,141,6],[142,3,142,6],[143,3,143,6],[144,3,144,6],[145,3,145,6],[177,5,177,6],[147,2,148,2],[147,3,148,3],[270,5,273,5],[270,7,273,7],[255,7,258,7],[77,2,77,3],[78,2,78,3],[335,7,354,7],[437,2,438,2],[147,4,148,4],[80,1,81,1],[80,2,81,2],[80,3,81,3],[80,4,81,4],[80,7,81,7],[164,5,164,6],[155,4,158,4],[149,5,149,6],[149,4,154,4],[149,7,161,7],[152,5,152,6],[227,5,239,5],[255,5,258,5],[277,3,277,5],[156,5,156,6],[157,5,157,6],[158,5,158,6],[193,1,194,1],[193,2,194,2],[193,3,194,3],[193,4,194,4],[193,6,194,6],[193,7,194,7],[253,1,254,1],[123,1,123,8],[146,1,146,8],[162,1,162,8],[80,8,81,8],[91,3,91,6],[92,3,92,6],[95,7,96,7],[95,8,96,8],[97,4,102,4],[97,7,117,7],[103,4,105,4],[106,4,108,4],[82,7,92,7],[253,8,254,8],[241,5,242,5],[244,5,252,5],[241,7,242,7],[244,7,252,7],[168,4,170,4],[186,5,187,6],[188,5,189,6],[126,3,126,6],[127,3,127,6],[128,3,128,6],[129,3,129,6],[130,3,130,6],[131,3,131,6],[132,3,132,6],[160,5,160,6],[161,5,161,6],[137,3,137,6],[147,5,148,6],[147,7,148,7],[147,8,148,8],[176,8,177,8],[95,1,96,1],[95,3,96,3],[95,4,96,4],[153,5,153,6],[154,5,154,6],[151,5,151,6],[109,4,111,4],[193,8,194,8],[195,6,196,6],[195,7,197,7],[193,5,194,5],[190,5,190,6],[191,5,191,6],[178,5,180,6],[178,7,191,7],[181,5,183,6],[184,5,185,6],[165,5,165,6],[166,5,166,6],[167,5,167,6],[168,5,168,6],[169,5,169,6],[170,5,170,6],[176,5,176,6],[133,3,133,6],[134,3,134,6],[135,3,135,6],[136,3,136,6],[163,4,167,4],[163,5,163,6],[176,1,177,1],[147,1,148,1],[286,3,286,4],[297,3,300,4],[299,7,300,7],[301,3,302,4],[301,7,303,7],[303,3,303,4],[304,3,305,4],[304,7,305,7],[306,3,306,4],[307,3,307,4],[307,7,308,7],[308,3,308,4],[309,3,309,4],[288,3,288,4],[284,7,286,7],[374,3,376,3],[375,2,376,2],[333,3,333,5],[333,6,334,6],[315,7,320,7],[321,7,322,7],[312,7,314,7],[293,3,294,4],[289,3,292,4],[295,3,296,4],[449,1,449,8],[537,7,564,7],[388,8,389,8],[356,1,357,1],[356,2,357,2],[569,3,569,6],[569,7,570,7],[570,3,570,6],[451,7,453,7],[456,7,465,7],[468,7,477,7],[482,1,482,8],[478,1,478,8],[466,1,466,8],[454,1,454,8],[532,3,533,3],[532,4,533,4],[532,5,533,5],[532,7,533,7],[356,8,357,8],[359,2,360,2],[365,2,367,2],[355,1,355,8],[387,1,387,8],[359,3,360,3],[365,3,367,3],[368,3,369,3],[333,8,334,8],[333,1,334,1],[416,5,418,5],[419,5,421,5],[422,5,423,5],[424,5,426,5],[435,2,436,2],[571,3,571,6],[571,7,573,7],[447,2,447,3],[575,3,575,6],[576,3,576,6],[577,3,577,6],[578,3,578,6],[583,3,584,3],[532,8,533,8],[480,7,481,7],[484,7,522,7],[525,7,530,7],[582,7,584,7],[447,4,447,5],[448,2,448,3],[565,1,565,8],[531,1,531,8],[523,1,523,8],[442,5,442,6],[658,2,658,4],[724,3,724,4],[725,3,725,4],[726,3,726,4],[727,3,727,4],[728,3,728,4],[668,3,668,4],[669,3,669,4],[660,2,660,4],[665,3,665,4],[666,3,666,4],[667,3,667,4],[712,7,726,7],[585,7,589,7],[590,3,594,3],[590,7,594,7],[595,3,598,3],[595,7,598,7],[599,3,601,3],[599,7,601,7],[602,3,608,3],[648,2,648,4],[609,7,612,7],[614,3,616,3],[614,7,616,7],[629,7,632,7],[634,2,634,4],[635,2,635,4],[636,2,636,4],[637,2,637,4],[638,2,638,4],[585,3,589,3],[801,7,807,7],[770,3,782,3],[770,6,782,6],[816,7,819,7],[818,6,819,6],[808,3,815,3],[808,6,815,6],[675,1,676,1],[675,7,676,7],[675,8,676,8],[677,7,709,7],[727,7,740,7],[721,3,721,4],[722,3,722,4],[723,3,723,4],[744,7,766,7],[757,6,758,6],[764,6,766,6],[675,5,675,6],[735,3,735,4],[736,3,736,4],[737,3,737,4],[808,7,815,7],[816,3,819,3],[732,3,732,4],[733,3,733,4],[767,6,769,6],[767,7,769,7],[801,6,807,6],[740,3,740,4],[739,3,739,4],[715,3,715,4],[864,3,864,6],[865,3,865,6],[859,3,859,6],[860,3,860,6],[866,3,866,6],[734,3,734,4],[893,4,893,5],[895,7,899,7],[895,2,895,3],[897,2,897,3],[898,2,898,3],[899,2,899,3],[894,4,894,5],[839,4,839,6],[801,3,807,3],[820,7,821,7],[822,7,823,7],[825,7,832,7],[850,7,857,7],[841,7,843,7],[738,3,738,4],[770,7,782,7],[783,3,791,3],[783,6,791,6],[783,7,791,7],[792,3,800,3],[792,6,800,6],[792,7,800,7],[859,7,861,7],[879,7,885,7],[890,2,890,3],[895,4,895,5],[896,4,896,5],[913,7,920,7],[914,2,914,3],[915,2,915,3],[915,6,917,6],[916,2,916,3],[917,2,917,3],[918,2,918,3],[918,6,919,6],[919,2,919,3],[920,2,920,3],[907,6,911,6],[908,2,908,3],[906,2,906,3],[907,2,907,3],[901,2,901,3],[902,2,902,3],[902,7,912,7],[903,2,903,3],[904,2,904,3],[905,2,905,3],[922,7,931,7],[923,2,923,3],[924,2,924,3],[925,2,925,3],[926,2,926,3],[927,2,927,3],[928,2,928,3],[929,2,929,3],[930,2,930,3],[931,2,931,3],[923,4,923,6],[922,4,922,6],[922,2,922,3],[1009,7,1010,7],[1010,3,1010,4],[1018,3,1018,4],[1019,3,1019,4],[981,3,981,6],[982,3,982,6],[983,3,983,6],[984,3,984,6],[985,3,985,6],[986,3,986,6],[1001,3,1001,4],[1002,3,1002,4],[1011,3,1011,4],[1011,6,1015,6],[992,3,992,4],[1008,3,1008,4],[1006,3,1006,4],[1006,7,1007,7],[1007,3,1007,4],[997,3,997,4],[999,3,999,4],[1023,7,1027,7],[1024,3,1024,4],[1025,3,1025,4],[1026,3,1026,4],[1027,3,1027,4],[1020,1,1020,8],[1011,7,1015,7],[1012,3,1012,4],[1013,3,1013,4],[1014,3,1014,4],[1015,3,1015,4],[1016,3,1016,4],[1016,6,1019,6],[1016,7,1019,7],[1017,3,1017,4],[998,3,998,4],[1009,3,1009,4],[1028,7,1040,7],[1029,3,1029,4],[1030,3,1030,4],[1031,3,1031,4],[1032,3,1032,4],[1033,3,1033,4],[1034,3,1034,4],[1035,3,1035,4],[1036,3,1036,5],[1037,3,1037,5],[1038,3,1038,5],[1039,3,1039,5],[1040,3,1040,5],[1028,3,1028,4],[1021,3,1021,4],[1023,3,1023,4],[1022,3,1022,4],[1041,7,1042,7],[1043,3,1043,6],[1043,7,1049,7],[1044,3,1044,6],[1045,3,1045,6],[1046,3,1046,6],[1047,3,1047,6],[1048,3,1048,6],[1050,7,1055,7],[1050,2,1050,6],[1052,2,1052,6],[1053,2,1053,6],[1054,2,1054,6],[1055,2,1055,6],[1056,7,1058,7],[1061,3,1061,4],[1041,3,1041,6],[1042,3,1042,6],[1049,3,1049,6],[1051,2,1051,6],[1062,7,1063,7],[1062,2,1063,2],[1065,3,1065,4],[1065,7,1070,7],[1067,3,1067,4],[1068,3,1068,4],[1069,3,1069,4],[1070,3,1070,4],[1056,2,1056,6],[1057,2,1057,6],[1058,2,1058,6],[1059,2,1059,6],[1062,3,1062,6],[1063,3,1063,6],[1060,1,1060,8],[1092,3,1092,4],[1092,7,1102,7],[1093,3,1093,4],[1094,3,1094,4],[1095,3,1095,4],[1096,3,1096,4],[1097,3,1097,4],[1098,3,1098,4],[1099,3,1099,4],[1100,3,1100,4],[1101,3,1101,4],[1102,3,1102,4],[1077,3,1077,6],[1078,3,1078,6],[1079,3,1079,6],[1083,5,1083,6],[1084,5,1084,6],[1087,5,1087,6],[1121,2,1121,3],[1121,4,1121,5],[1121,7,1125,7],[1122,2,1122,3],[1122,4,1122,5],[1123,2,1123,3],[1123,4,1123,5],[1124,2,1124,3],[1124,4,1124,5],[1125,2,1125,3],[1125,4,1125,5],[1105,7,1106,7],[1106,3,1106,4],[1103,1,1103,8],[1107,3,1107,4],[1108,3,1108,4],[1115,2,1115,3],[1115,4,1115,5],[1088,3,1088,4],[1089,3,1089,4],[1090,3,1090,4],[1126,2,1126,3],[1126,4,1126,5],[1127,7,1128,7],[1128,2,1128,3],[1128,4,1128,5],[1127,4,1127,5],[1130,2,1130,3],[1130,4,1130,5],[1132,6,1139,6],[1133,2,1133,3],[1133,4,1133,5],[1134,2,1134,3],[1134,4,1134,5],[1135,2,1135,3],[1136,2,1136,3],[1137,2,1137,3],[1138,2,1138,3],[1139,2,1139,3],[1129,4,1129,5],[1140,2,1140,3],[1140,6,1143,6],[1141,2,1141,3],[1141,4,1141,5],[1142,2,1142,3],[1143,2,1143,3],[1142,4,1142,5],[1143,4,1143,5],[1140,4,1140,5],[1138,4,1138,5],[1139,4,1139,5],[1136,4,1136,5],[1137,4,1137,5],[1135,4,1135,5],[1132,2,1132,3],[1131,2,1131,3],[1131,4,1131,5],[1132,4,1132,5],[1150,2,1150,5],[1152,2,1152,3],[1153,6,1154,6],[1153,2,1153,3],[1154,2,1154,3],[1154,4,1154,5],[1153,4,1153,5],[1152,4,1152,5],[1146,4,1146,5],[1215,7,1216,7],[1206,1,1206,6],[1207,2,1207,5],[1208,2,1208,5],[1209,2,1209,5],[1210,2,1210,5],[1211,2,1211,5],[1212,2,1212,5],[1213,2,1213,5],[1215,1,1216,1],[1215,2,1216,2],[1215,5,1216,6],[1147,4,1147,5],[1149,7,1150,7],[1147,2,1147,3],[1148,2,1148,5],[1156,4,1156,5],[1151,1,1151,8],[1202,4,1205,5],[1155,6,1156,6],[1155,2,1155,3],[1156,2,1156,3],[1157,2,1157,5],[1157,7,1158,7],[1158,2,1158,5],[1159,2,1159,5],[1171,5,1171,6],[1177,5,1177,6],[1178,7,1186,7],[1190,5,1196,6],[1197,1,1197,6],[1244,3,1245,3],[1246,5,1246,6],[1155,4,1155,5],[1214,1,1214,8],[1160,1,1160,8],[1198,7,1201,7],[1198,3,1198,6],[1199,3,1199,6],[1200,3,1200,6],[1201,3,1201,6],[1220,5,1222,6],[1178,5,1178,6],[1247,3,1269,3],[1247,7,1256,7],[1257,7,1261,7],[1264,7,1265,7],[1266,7,1269,7],[1270,3,1270,6],[1271,3,1271,4],[1250,5,1252,6],[1272,3,1272,4],[1273,3,1273,4],[1274,3,1274,4],[1275,3,1275,4],[1276,3,1276,4],[1277,3,1277,4],[1278,3,1278,4],[1279,3,1279,4],[1215,8,1216,8],[1280,3,1280,4],[1281,3,1281,4],[1282,3,1282,4],[1283,1,1283,6],[1284,2,1284,3],[1284,4,1284,5],[1285,2,1285,3],[1285,4,1285,5],[1288,4,1288,5],[1289,2,1289,3],[1289,4,1289,5],[1292,4,1292,5],[1293,4,1293,5],[1294,4,1294,5],[1295,4,1295,5],[1296,4,1296,5],[1297,4,1297,5],[1291,4,1291,5],[1287,1,1287,6],[1288,2,1288,3],[1290,1,1290,8],[1286,2,1286,3],[1286,4,1286,5],[1298,4,1298,5],[1304,4,1304,5],[1305,4,1305,5],[1306,4,1306,5],[1307,4,1307,5],[1308,4,1308,5],[1309,4,1309,5],[1310,4,1310,5],[1311,4,1311,5],[1312,4,1312,5],[1313,4,1313,5],[1322,4,1322,5],[1332,4,1332,5],[1341,4,1341,5],[1349,4,1349,5],[1362,4,1362,5],[1375,4,1375,5],[1299,4,1299,5],[1300,4,1300,5],[1301,4,1301,5],[1302,4,1302,5],[1303,4,1303,5],[1389,4,1389,5],[1394,3,1394,4],[1394,5,1394,6],[1395,3,1395,4],[1396,3,1396,4],[1397,3,1397,4],[1398,3,1398,4],[1399,3,1399,4],[1400,3,1400,4],[1401,3,1401,4]],"merged_total":1476,"flags":["merged_cut"]}
[1]
[1]
[1]
[1]
[1]
[1,"Заказчик →",null,null,null,null,{"$f":"TODAY()","v":"2024-07-26"}]
[1,null,null,null,null,null,null,null,null,null,null,"Сумма"]
[1]
[{"$f":"SUM(J12:J71)","v":0}," Полугерметичные  поршневые  компрессоры   Frascold   (Италия)    В комплекте  серии V, Z, W входит электронное реле давления масла.     Тип хладагента R134, 404, 407, 507, 22 "]
[{"$f":"A9","v":0},"№","Модель     ","Объемная про-ть м3/ч  50Гц","Электрические характеристики"," трубы Ø mm","Рабочий режим","Кол-во в упаковке","Ед. изм."]
[{"$f":"A9","v":0},null,null,null,"A / kW","Всас./Нагнет."]
[{"$f":"J12","v":0},1,"A1-6Y  ",5.47,"3,6 / 2,0 "," 16 / 12","7.5 /-45 C",1,"шт",null,null,{"$f":"J12*K12","v":0}]
[0,{"$f":"B12+1","v":2},"A1.5-7Y  ",6.91,"4,5 / 2,3"," 16 / 12","7.5 /-40 C",null,"шт",null,null,{"$f":"J13*K13","v":0}]
[0,{"$f":"B13+1","v":3},"В1.5-9.1Y  ",8.9600000000000009,"5,9 / 3,3"," 16 / 12","7.5 /-45 C",null,"шт",null,null,0]
[0,{"$f":"1+B14","v":4},"В1.5-10.1Y  ",9.8800000000000008,"5,5 / 3,1"," 16 / 12"," -5 /-45 C",null,"шт",null,null,0]
[0,5,"В2-10.1Y  ",9.8800000000000008,"6,7 / 3,6","19 / 16","7.5 /-40 C",null,"шт",null,null,0]
[0,6,"D2-11.1Y  ",11.26,"7,1 / 4,1"," 22 / 16","7.5 /-40 C",null,"шт",null,null,0]
[0,7,"D2-13.1Y  ",13.15,"7,1 / 4,1","22 / 16"," -5 /-45 C",null,"шт",null,null,0]
[0,8,"D3-13.1Y  ",13.15,"8,8 / 4,8","28 / 16","7.5 /-30 C",null,"шт",null,null,0]
[0,9,"D2-15.1Y  ",15.36,"8,4 / 4,7","22 / 16"," -5 /-45 C",null,"шт",null,null,0]
[0,10,"D3-15.1Y ",15.36,"10,1 / 5,7","28 / 16"," 5 /-30 C",null,"шт",null,null,0]
[0,11,"D4-16.1Y  ",16.399999999999999,"11,6 / 6,2","28 / 19","7.5 /-30 C",null,"шт",null,null,0]
[0,{"$f":"B22+1","v":12},"D3-18.1Y ",17.93,"10,0 / 5,5","28 / 16"," -10 /-45 C",null,"шт",null,null,0]
[0,13,"D4-18.1Y  ",17.93,"12,5 / 6,7","28 / 19"," 5 /-30 C",null,"шт",null,null,0]
[0,14,"D3-19.1Y  ",19.12,"9,8 / 5,4","28 / 16"," -15 /-45 C",null,"шт",null,null,0]
[0,15,"Q5-21.1Y  ",21.18,"11,6 / 6,6","28 / 19"," 7.5 /-30 C",null,"шт",null,null,0]
[0,16,"Q4-25.1Y  ",24.69," 11 / 7,0 ","28 / 19"," -5 /-45 C",null,"шт",null,null,0]
[0,17,"Q5-25.1Y  ",24.69,"12,7 / 8,5","28 / 22"," 5 /-40 C",null,"шт",null,null,0]
[0,18,"Q5-28.1Y  ",28.02,"14 / 8,2","35 / 22"," -5 /-45 C",null,"шт",null,null,0]
[0,{"$f":"1+B29","v":19},"Q7-28.1Y  ",28.02,"17,6 / 9,5","35 /  28"," 5 /-30 C",null,"шт",null,null,0]
[0,{"$f":"1+B30","v":20},"Q5-33.1Y  ",32.659999999999997,"14,4 / 8,3","35 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,{"$f":"B31+1","v":21},"Q7-33.1Y  ",32.659999999999997,"20 / 11,2","35 /  28"," 5 /-30 C",null,"шт",null,null,0]
[0,{"$f":"B32+1","v":22},"Q7-36.1Y  ",35.86,"19,4 / 10,8","35 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,{"$f":"B33+1","v":23},"Q9-36.1Y  ",35.86,"22,2 / 11,5","35 /  28"," 5 /-30 C",null,"шт",null,null,0]
[0,24,"Q9-39.1Y  ",38.57,"22,2 / 11,7","35 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,25,"Q10-39.1Y  ",38.57,"23,7 / 12,5","35 /  28"," 5 /-30 C",null,"шт",null,null,0]
[0,26,"S8-42Y  ",41.32,"20,3 / 11,8","35 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,{"$f":"1+B37","v":27},"S12-42Y  ",41.32,"22,4 / 12,9","35 /  28"," 5 /-30 C",null,"шт",null,null,0]
[0,28,"S10-52Y  ",51.5,"24,5 / 14,9","35 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,29,"S15-52Y  ",51.5,"32,4 / 17,8","42 /  28"," 7.5 /-30 C",null,"шт",null,null,0]
[0,30,"S15-56Y  ",56,"30,7 / 16,5","42 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,31,"S20-56Y  ",56,"38,4 / 19,6","42 /  28"," 7.5 /-30 C",null,"шт",null,null,0]
[0,32,"S20-63Y  ",63.2,"33,0 / 17,5","42 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,33,"S25-63Y  ",63.2,"39,5 / 21,0","42 /  28"," 7.5 /-30 C",null,"шт",null,null,0]
[0,34,"V15-71Y  ",70.77,"32,2 / 19,6","42 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,35,"V25-71Y  ",70.77,"43,5 / 23,6","54 / 35"," 7.5 /-40 C",null,"шт",null,null,0]
[0,36,"V20-84Y  ",83.81,"46,2 / 24,2","42 /  28"," -5 /-45 C",null,"шт",null,null,0]
[0,37,"V30-84Y  ",83.81,"49,2 / 28,4","54 / 35"," 7.5 /-40 C",null,"шт",null,null,0]
[0,{"$f":"1+B48","v":38},"V25-103Y  ",103.2,"52,3 / 28,8","54 / 35"," -10 /-45 C",null,"шт",null,null,0]
[0,39,"V35-103Y  ",103.2,"61,0 / 38,5","54 / 35"," 7.5 /-30 C",null,"шт",null,null,0]
[0,40,"V30-112Y  ",112.11,"56,0 / 33.0","54 / 35"," -10 /-45 C",null,"шт",null,null,0]
[0,41,"V35-112Y  ",112.11,"67,5 / 39.0","54 / 35"," 7.5 /-30 C",null,"шт",null,null,0]
[0,42,"V30-123Y  ",123.13,"60,5 / 35.0","54 / 35"," -10 /-45 C",null,"шт",null,null,0]
[0,43,"V40-123Y  ",123.13,"76,5 / 40.0","54 / 35"," 7.5 /-30 C",null,"шт",null,null,0]
[0,44,"Z25-106Y  ",106.16,"53,6 / 31,9","54 / 35"," -5 /-45 C",null,"шт",null,null,0]
[0,45,"Z35-106Y  ",106.16,"60,2 / 35,1","54 / 35"," 7.5 /-40 C",null,"шт",null,null,0]
[0,46,"Z30-126Y  ",125.72,"55,7 / 35,0","54 / 35"," -5 /-45 C",null,"шт",null,null,0]
[0,47,"Z40-126Y  ",125.72,"71,9 / 40,7","67 / 42"," 7.5 /-40 C",null,"шт",null,null,0]
[0,48,"Z40-140Y  ",139.68,"70,0 / 38,0","67 / 42"," -5 /-45 C",null,"шт",null,null,0]
[0,49,"Z50-140Y ",139.68,"79,5 / 46,0","67 / 42"," 7.5 /-40 C",null,"шт",null,null,0]
[0,50,"Z40-154Y  ",154.38,"77,9 / 37,9","67 / 42"," -5 /-45 C",null,"шт",null,null,0]
[0,51,"Z50-154Y  ",154.38,"90,4 / 52,1","67 / 42"," 7.5 /-40 C",null,"шт",null,null,0]
[0,52,"Z40-168Y  ",168.16,"77,9 / 37,9","67 / 42"," -5 /-45 C",null,"шт",null,null,0]
[0,53,"Z50-168Y  ",168.16,"90,4 / 51,0","67 / 42"," 7.5 /-40 C",null,"шт",null,null,0]
[0,54,"Z50-185Y  ",185,"90,4 / 51,0","67 / 42"," -5 /-45 C",null,"шт",null,null,0]
[0,55,"W70-206Y  ",205.8,"116,8 / 66,8","79 / 54"," 5 /-30 C",null,"шт",null,null,0]
[0,56,"W75-228Y  ",227.77,"128,4 / 74,2","79 / 54"," 5 /-30 C",null,"шт",null,null,0]
[0,{"$f":"B67+1","v":57},"W80-240Y  ",239.02,"135,7 / 65,4"," 79 / 54"," 5 /-30 C",null,"шт",null,null,0]
[0,{"$f":"B68+1","v":58},"RSH SK220310","контроль производительности для компрессоров серия Q",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B69+1","v":59},"RSH SK220360","контроль производительности для компрессоров серия S",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B70+1","v":60},"RSH SK220400","контроль производительности для компрессоров серия V-Z-W",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J72:J79)","v":0},"        Двухступенчатые полугерметичные поршневые компрессоры Frascold (Италия)                                                                                                                                                ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A72","v":0},"№","Модель     ","Объемная про-ть м3/ч  50Гц","Электрические характеристики"," трубы Ø mm","Рабочий режим","Кол-во в упаковке","Ед. изм.",null,null,0]
[{"$f":"A72","v":0},null,null,null,"A / kW","Всас./Нагнет.",null,null,null,null,null,0]
[{"$f":"J75","v":0},{"$f":"B71+1","v":61},"2Z30-102.51Y  ","102,9 / 51,5","53 / 30"," 42 / 35"," -25 /-70 C",1,"шт",null,null,0]
[0,{"$f":"B75+1","v":62},"2Z40-123.62Y  ","123,1 / 62","71,9 / 40,7"," 42 / 35",null,null,"шт",null,null,{"$f":"J76*K76","v":0}]
[0,{"$f":"B76+1","v":63},"Тэн картера  50W/230V  серии A-B-D",null,null,null,null,null,"шт",null,null,0]
[0,64,"Тэн картера  70W/230V  серии Q-S",null,null,null,null,null,"шт",null,null,0]
[0,65,"Тэн картера  150W/230V серии V-Z-W",null,null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J80:J94)","v":0},"        Винтовые среднетемпературные компрессоры Frascold (Италия)   R22, 134, 404, 407, 507.                                                                                                                                             ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A80","v":0},"№","Модель     ","HP    ","KW","Мощность ватт            R-404-507","Мощность ватт R-407","Кол-во в упаковке","Ед. изм.",null,null,0]
[{"$f":"A80","v":0},null,null,null,null,"-10/40","+2/50",null,null,null,null,0]
[0,{"$f":"B79+1","v":66},"FVR-H-60-160Y",60,"39.4",90035,null,1,"шт",null,null,0]
[0,{"$f":"B83+1","v":67},"FVR-H-90-270Y",90," 67.2",166029,null,null,"шт",null,null,0]
[0,{"$f":"B84+1","v":68},"CXH-02-80-230Y",80,60,127277,159728,null,"шт",null,null,0]
[0,{"$f":"B85+1","v":69},"CXH-02-90-264Y",90,67,146702,185168,null,"шт",null,null,0]
[0,{"$f":"B86+1","v":70},"CXH-02-100-298Y",100,75,165599,210007,null,"шт",null,null,0]
[0,{"$f":"1+B87","v":71},"CXH-02-120-340Y",120,90,192492,250320,null,"шт",null,null,0]
[0,72,"CXH-52-125-372Y",125,95,211309,272753,null,"шт",null,null,0]
[0,73,"FVR-L-70-230Y",70,null,null,null,null,"шт",null,null,0]
[0,74,"FVR-L-125-430Y",125,null,null,null,null,"шт",null,null,0]
[0,75,"TOOWP123","картридж масляного фильтра для серии FVRL NRL NRH",null,null,null,null,"шт",null,null,0]
[0,76,"TOOWP125","картридж масляного фильтра для серии FVRL NRL NRH",null,null,null,null,"шт",null,null,0]
[0,77,"BLR/362204-07","картридж масляного фильтра для Bitzer",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J95:J118)","v":0},"         Спиральные  компрессоры  INVOTECH ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A95","v":0},"№","Модель     ","Электрические параметры","Диаметр трубы Ø mm","R22 - R407",null,"Кол-во в упаковке","Ед. изм.",null,null,0]
[{"$f":"A95","v":0},null,null,null,null,null,null,null,null,null,null,0]
[0,{"$f":"B94+1","v":78},"YM34E2S-102  2HP  220v","2070w 9.4A"," 22 - 12mm ","22400 Btu/h",null,1,"шт",null,null,0]
[0,{"$f":"B98+1","v":79},"YM34E1S-100   2HP","2034w 3.5A",null,"22400 Btu/h",null,null,"шт",null,null,0]
[0,{"$f":"1+B99","v":80},"YM43E1S-100   2.5HP","2297w 4.8A",null,"25500 Btu/h",null,null,"шт",null,null,0]
[0,81,"YM49E1S-100   3HP","2547w 5.1A",null,"29300 Btu/h",null,null,"шт",null,null,0]
[0,82,"YM60E1S-100   3.5HP","3220w 6.5A",null,"35000 Btu/h",null,null,"шт",null,null,0]
[0,83,"YM70E1S-100   4HP","3530w 7.0A",null,"39200 Btu/h",null,null,"шт",null,null,0]
[0,84,"YM86E1S-100   5HP","4250w 8.0A","22 - 12mm       28 - 16mm","49400 Btu/h",null,null,"шт",null,null,0]
[0,85,"YM102E1S-100   6HP","5050w 9.4A",null,"57600 Btu/h",null,null,"шт",null,null,0]
[0,86,"YM115E1S-100   7HP","5600w 11.2A",null,"69000 Btu/h",null,null,"шт",null,null,0]
[0,87,"YM132E1S-100   8HP","6447w 12.1A"," 28-22mm","76100 Btu/h",null,null,"шт",null,null,0]
[0,88,"YM158E1S-100   9HP","7921w 13.6A",null,"87600 Btu/h",null,null,"шт",null,null,0]
[0,89,"YM182E1S-100   10HP","8928w 15.5A",null,"101200 Btu/h",null,null,"шт",null,null,0]
[0,90,"YM200E1S-100   12HP","9671w 16.3A","28-22mm           35-22mm","116900 Btu/h",null,null,"шт",null,null,0]
[0,91,"YM210E1S-100   13HP","10170w 16.9A",null,"121000 Btu/h",null,null,"шт",null,null,0]
[0,92,"YM240E1S-100   14HP","11600w 20.6A",null,"130000 Btu/h",null,null,"шт",null,null,0]
[0,{"$f":"1+B112","v":93},"YSM235E1G-100   13HP","11900w 21.5A"," 35-22mm","130000 Btu/h",null,null,"шт",null,null,0]
[0,{"$f":"1+B113","v":94},"YSM260E1G-100   15HP","13150w 23A",null,"150000 Btu/h",null,null,"шт",null,null,0]
[0,{"$f":"1+B114","v":95},"YM260E1S-100   15HP","12700w 22.8A"," 42-28mm","143600 Btu/h",null,null,"шт",null,null,0]
[0,{"$f":"1+B115","v":96},"YM280E1S-100   16HP","14100w 26.4A",null,"160000 Btu/h",null,null,"шт",null,null,0]
[0,{"$f":"1+B116","v":97},"YM350E1S-100   20HP","16650w 29.4A",null,"200000 Btu/h",null,null,"шт",null,null,0]
[0,98,"YM410E1S-100   25HP","19400w 34.5A",null,"250000 Btu/h",null,null,"шт",null,null,0]
[{"$f":"SUM(J119:J123)","v":0},"  серия YF Присоединение - резьба.  (с опцией смотрового стекла уровня масла),   Тип хладагента R404, R507  3F      Рабочий режим кипения на R404-507  от 0  до -40C.   ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A119","v":0},"№","Модель     ","Электрические параметры","Диаметр трубы Ø mm",null,null,"Кол-во в упаковке","Ед. изм.",null,null,0]
[{"$f":"A119","v":0},null,null,null,null,null,null,null,null,null,null,0]
[0,{"$f":"B118+1","v":99},"YF25E1S-100   3.5HP","2324w 5.0A","22-12mm",null,null,1,"шт",null,null,0]
[0,{"$f":"B122+1","v":100},"YF41E1S-100   6HP","3358w 7.0A",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J124:J146)","v":0},"Вентиль для компрессора и для рессивера",null,null,null,null,null,null,null,null,null,0]
[0,{"$f":"B123+1","v":101}," BLR/RV-1/2   (3/4)","для компрессоров серии YM  2-7HP нагнетание 12мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B125+1","v":102}," BLR/RV-5/8   (3/4)","для компрессоров серии YM  5-7HP нагнетание 16мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B126+1","v":103},"  BLR/RV-3/8   (1)","10mm",null,null,null,null,"шт",null,null,0]
[0,{"$f":"1+B127","v":104},"  BLR/RV-1/2   (1)","12mm",null,null,null,null,"шт",null,null,0]
[0,105,"  BLR/RV-5/8   (1)","16mm",null,null,null,null,"шт",null,null,0]
[0,106,"    VS09    5/8   (1 1/4)","для компрессоров серии 2-4HP всас  16mm",null,null,null,null,"шт",null,null,0]
[0,107,"   BLR/RV-3/4   (1 1/4)","для компрессоров серии 2-4HP всас,   8-HP нагнетание 19mm",null,null,null,null,"шт",null,null,0]
[0,108,"   BLR/RV-7/8   (1 1/4)","для компрессоров серии 2-7HP всас,   8-13HP нагнетание 22mm",null,null,null,null,"шт",null,null,0]
[0,109,"    VS025    1 1/8   (1 1/4)","для компрессоров серии 5-7HP всас,   12-13HP нагнетание 28mm",null,null,null,null,"шт",null,null,0]
[0,110,"   BLR/RV-1 1/8   (1 3/4)","для компрессоров серии 8-13HP всас, нагнетание 20-25HP  28mm",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B134+1","v":111},"  BLR/RV-1 3/8    (1 3/4)","для компрессоров серии 8-13HP всас  35mm",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B135+1","v":112},"RW-RV-503    1 5/8  (2 1/4)","   15-25HP всас 42мм",null,null,null,null,"шт",null,null,0]
[0,113,"RW-RV-504   2 1/8   (2 1/8)","   15-25HP всас 54мм",null,null,null,null,"шт",null,null,0]
[0,114,"RW-FRC09","1 1/4  12UN   5/8  адаптер",null,null,null,null,"шт",null,null,0]
[0,115,"RW-FRC15","1 1/4  12UN   1 1/8  адаптер",null,null,null,null,"шт",null,null,0]
[0,116,"RW-FRC19","1 3/4  12UN   1 3/8  адаптер",null,null,null,null,"шт",null,null,0]
[0,117,"RW-FRC25","2 1/4  12UN   2 1/8  адаптер",null,null,null,null,"шт",null,null,0]
[0,118,"RW-ARC29","1 1/4  12UN   7/8  адаптер переходник угловой",null,null,null,null,"шт",null,null,0]
[0,119,"RW-ARC37","1 3/4  12UN   1 3/8  адаптер переходник угловой",null,null,null,null,"шт",null,null,0]
[0,120,"Тэн картера  110-240v","462/500mm    Для  компрессоров  серии INVOTECH  2-13HP 35W",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B144+1","v":121},"Тэн картера  110-240v","537/575mm    Для  компрессоров  серии INVOTECH  2-13HP 55W",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B145+1","v":122},"Тэн картера  110-240v","912/950mm    Для  компрессоров  серии INVOTECH  20-25HP 90W",null,null,null,null,"шт",null,null,{"$f":"J146*K146","v":0}]
[{"$f":"SUM(J147:J162)","v":0},"Серия YH  R407, R22,  3F,  (наличие смотрового стекла, удобно для использования в уравнительной линии тандема и централи)       Рабочий режим кипения на R407C  от +10 до-25C.",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A147","v":0},"№","Модель     ","Электрические параметры","Диаметр трубы Ø mm","R407, R22",null,"Кол-во в упаковке","Ед. изм.",null,null,0]
[{"$f":"A147","v":0},null,null,null,null,null,null,null,null,null,null,0]
[{"$f":"J150","v":0},{"$f":"B146+1","v":123},"YH69T1G-100   2HP","2160w 4.8A","22-12mm       28 - 16mm присоединение под пайку","22400 Btu/h",null,1,"шт",null,null,0]
[0,{"$f":"B150+1","v":124},"YH89T1G-100   3HP","2680w 5.3A",null,"29300 Btu/h",null,null,"шт",null,null,0]
[0,125,"YH119T1G-100   4HP","3550w 7.1A",null,"39200 Btu/h",null,null,"шт",null,null,0]
[0,126,"YH150T1G-100   5HP","4410w 8.4A",null,"49400 Btu/h",null,null,"шт",null,null,0]
[0,127,"YH175T1G-100   6HP","5030w 9.1A",null,"57600 Btu/h",null,null,"шт",null,null,0]
[0,128,"YH200T1G-100   7HP","5970w 11.2A",null,"66800 Btu/h",null,null,"шт",null,null,0]
[0,129,"YH230T1S-100   8HP","6770w 12.9A","28-22mm            35-22mm присоединение под резьбу","76100 Btu/h",null,null,"шт",null,null,0]
[0,130,"YH266T1S-100   9HP","7780w 14.8A",null,"87600 Btu/h",null,null,"шт",null,null,0]
[0,{"$f":"1+B157","v":131},"YH307T1S-100   10HP","8910w 15.6A",null,"101200 Btu/h",null,null,"шт",null,null,0]
[0,132,"YH355T1S-100   12HP","10240w 17.8A",null,"116900 Btu/h",null,null,"шт",null,null,0]
[0,133,"YH450T1S-100   15HP","13156w 20.5A",null,"143600 Btu/h",null,null,"шт",null,null,0]
[0,134,"YH610T1S-100   20HP","17444w 31.5A"," 42-28mm  ","200000 Btu/h",null,null,"шт",null,null,0]
[0,135,"YH720T1S-100   25HP","20547w 36.7A",null,"250000 Btu/h",null,null,"шт",null,null,0]
[{"$f":"SUM(J163:J175)","v":0},"         Серия YH   R410A    3F     соединение под пайку",null,null,null,null,null,null,null,null,null,0]
[0,{"$f":"B162+1","v":136},"YH95C1G-100   3.5HP","3170w 5.8A","22 - 12mm          28 - 16mm ","32700 Btu/h  ",null,1,"шт",null,null,0]
[0,{"$f":"B164+1","v":137},"YH119C1G-100   4HP","3888w 7.4A",null,"40900 Btu/h  ",null,null,"шт",null,null,0]
[0,{"$f":"B165+1","v":138},"YH150C1G-100   5HP","4854w 8.6A",null,"51600 Btu/h  ",null,null,"шт",null,null,0]
[0,{"$f":"1+B166","v":139},"YH175C1G-100   6HP","5545w 9.7A",null,"59500 Btu/h  ",null,null,"шт",null,null,0]
[0,140,"YH200C1G-100   7HP","6200w 11.6A",null,"70000 Btu/h  ",null,null,"шт",null,null,0]
[0,{"$f":"1+B168","v":141},"YH230C1G-100   8HP","7210w 13.4A","28 - 22mm      35 - 22mm ","79200 Btu/h  ",null,null,"шт",null,null,0]
[0,142,"YH292C1G-100   10HP","9070w 15.8A",null,"100500 Btu/h  ",null,null,"шт",null,null,0]
[0,{"$f":"1+B170","v":143},"YH355C1G-100   12HP","10800w 18.2A",null,"119800 Btu/h  ",null,null,"шт",null,null,0]
[0,{"$f":"1+B171","v":144},"YH450C1S-105   15HP","13759w 24.1A","35-22mm","15000 Btu/h  ",null,null,"шт",null,null,0]
[0,145,"YH610C1S-100   20HP","18620w 33.6A","42-28mm","20000 Btu/h  ",null,null,"шт",null,null,0]
[0,146,"YH720C1S-100   25HP","21254w 38.5A",null,"25000 Btu/h  ",null,null,"шт",null,null,0]
[0,147,"YH880C1S-100   30HP","26800w 50A",null,"30000 Btu/h  ",null,null,"шт",null,null,0]
[{"$f":"SUM(J176:J192)","v":0},"         Герметичные  компрессоры  ANKANG  серия QR3 - QL3  3F   в комплекте с вентилями",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A176","v":0},"№","Модель     ","Объем цилиндра, см3","Электрические параметры"," трубы Ø mm",null,"Кол-во в упаковке","Ед. изм.",null,null,0]
[{"$f":"A176","v":0},null,null,null,null,"Всас./Нагнет.",null,null,null,null,null,0]
[0,{"$f":"B175+1","v":148},"QR-44    2HP   220v",44,"2300w 11.3A"," 16 / 12",null,1,"шт",null,null,0]
[0,{"$f":"B179+1","v":149},"QR3-44    2HP   ",44,"2300w 3.80A",null,null,null,"шт",null,null,0]
[0,150,"QR3-52    2.5HP   ",52,"2700w 4.70A",null,null,null,"шт",null,null,0]
[0,151,"QR3-58    3HP   ",58.2,"3080w 5.00A"," 22 / 16",null,null,"шт",null,null,0]
[0,152,"QR3-62    3HP   ",62.7,"3310w 5.40A",null,null,null,"шт",null,null,0]
[0,153,"QR3-74    3.5HP   ",74.2,"4250w 6.70A",null,null,null,"шт",null,null,0]
[0,154,"QR3-90    4HP   ",90.2,"4600w 7.30A"," 22 / 16",null,null,"шт",null,null,0]
[0,155,"QR3-112    5HP   ",112.5,"6100w 9.60A",null,null,null,"шт",null,null,0]
[0,156,"QR3-124    6HP   ",124.4,"6800w 10.60A"," 28 / 16",null,null,"шт",null,null,0]
[0,157,"QR3-134    7HP   ",134.80000000000001,"7400w 11.70A",null,null,null,"шт",null,null,0]
[0,158,"QL3-52    2.5HP   ",52,"1380w 2.50A","  16 / 12",null,null,"шт",null,null,0]
[0,159,"QL3-74    3.5HP   ",74.2,"2060w 3.20A",null,null,null,"шт",null,null,0]
[0,160,"QL3-112    5HP   ",112.5,"2830w 5.00A"," 22 / 16",null,null,"шт",null,null,0]
[0,161,"QL3-134    7HP   ",134.80000000000001,"3620w 6.30A"," 28 / 16",null,null,"шт",null,null,0]
[{"$f":"SUM(J193:J204)+A199","v":0}," Герметичные компрессоры CUBIGEL  220 - 240v  50Hz     R404, 507 ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"SUM(J194:J198)","v":0},"№","Модель   LBP -10 / -40c","НР","Электрические параметры","Обьемная        пр-ть см3/час","Мотор","Кол-во в упаковке","Ед. изм.",null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,0]
[0,{"$f":"B192+1","v":162},"MX 21 FB"," 3/4","700w - 3.5A",20.72,null,null,"шт",null,null,0]
[0,{"$f":"B196+1","v":163},"MS 26 FB   под вентиль 12мм"," 3/4","910w - 4.0A",25.93,null,null,"шт",null,null,0]
[0,{"$f":"B197+1","v":164},"MS 34 F3   под вентиль 16мм",1,"1120w - 2.2A",34.42,"3F",null,"шт",null,null,0]
[{"$f":"SUM(J199:J204)","v":0},{"$f":"B198+1","v":165},"Модель   HBP +10 / -25c",null,null,null,"CSR","Кол-во в упаковке","Ед. изм.",null,null,0]
[0,166,"MX 16 TB"," 3/4","1000w - 5.0A",16.03,null,null,"шт",null,null,0]
[0,167,"MX 18 TB"," 7/8","1200w - 6.0A",18.399999999999999,null,null,"шт",null,null,0]
[0,168,"MS 22 TB  под вентиль 12мм",1,"1300w - 7.0A",21.75,null,null,"шт",null,null,0]
[0,169,"MS 26 TB   под вентиль 16мм",1.375,"1625w - 7.9A",25.93,null,null,"шт",null,null,0]
[0,170,"CAJ4517Z",1.375,"1625w - 7.9A",25.95,null,null,"шт",null,null,0]
[{"$f":"SUM(J205:J274)","v":0}," Герметичные компрессоры  DONPER  220 - 240v  50Hz  ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"SUM(J206:J222)","v":0},"№","Модель   LBP  R600a","НР"," см3/час","Обмотка","Мощность, ватт   -23,3/54,4C","Кол-во в упаковке","Ед. изм.",null,null,{"$f":"J206*K206","v":0}]
[{"$f":"J207","v":0},{"$f":"B204+1","v":171},"L   QD75YG  S"," 1/6-",7.5,"AL",130,null,"шт",null,null,0]
[0,{"$f":"B207+1","v":172},"MX   QD91YG  S"," 1/5",9.1,"AL",158,null,"шт",null,null,0]
[0,{"$f":"B208+1","v":173},"MQ   QD142YG  S"," 1/3",14.2,"AL",240,null,"шт",null,null,0]
[0,174,"MQ   QD142YG  S"," 1/3",14.2,"Cu",240,null,"шт",null,null,0]
[0,{"$f":"B210+1","v":175},"D40CY1C    ",null,4,"AL   ",50,null,"шт",null,null,0]
[0,176,"D43CY1B    ",null,4.3,null,65,null,"шт",null,null,0]
[0,177,"D53CY1E    ",null,5.3,null,80,null,"шт",null,null,0]
[0,178,"D65CY1D    ",null,6,null,95,null,"шт",null,null,0]
[0,179,"A120CY1    ",null,7.2,null,118,null,"шт",null,null,0]
[0,180,"A145CY1A    ",null,8.8000000000000007,null,140,null,"шт",null,null,0]
[0,181,"S96CY1A    ",null,9.6,null,155,null,"шт",null,null,0]
[0,182,"S100CY1A    ",null,10,null,168,null,"шт",null,null,0]
[0,183,"S118CY1    ",null,11.8,null,193,null,"шт",null,null,0]
[0,184,"L126CY1    ",null,12.6,null,212,null,"шт",null,null,0]
[0,185,"L140CY1    ",null,14,null,235,null,"шт",null,null,0]
[0,186,"K270CY1    ",null,16.2,null,265,null,"шт",null,null,0]
[{"$f":"SUM(J223:J240)","v":0},"№","Модель   LBP  R134a","НР"," см3/час","Обмотка","Мощность, ватт   -23,3/54,4C","Кол-во в упаковке","Ед. изм.",null,null,0]
[0,{"$f":"B222+1","v":187},"L   QD25HG  S"," 1/12",2.5,"AL",55,1,"шт",null,null,0]
[0,{"$f":"B224+1","v":188},"L   QD35HG  S"," 1/11",3.5,"AL",75,null,"шт",null,null,0]
[0,189,"ML   ADW51  S"," 1/6",5.0999999999999996,"AL",125,null,"шт",null,null,0]
[0,190,"ML   ADW57  S"," 1/5-",5.7,"AL",135,null,"шт",null,null,0]
[0,191,"D25DZ1   ",null,2.5,"AL   ",55,null,"шт",null,null,0]
[0,{"$f":"B228+1","v":192},"DK30DZ1    ",null,3,null,70,null,"шт",null,null,0]
[0,193,"AG100DZ1    ",null,3.6,null,85,null,"шт",null,null,0]
[0,194,"AG130DZ1   ",null,4.3,null,110,null,"шт",null,null,0]
[0,195,"SK53CZ1   ",null,5.3,null,145,null,"шт",null,null,0]
[0,196,"S65CZ1    ",null,6.5,null,170,null,"шт",null,null,0]
[0,197,"S72CZ1   ",null,7.2,null,195,null,"шт",null,null,0]
[0,198,"S76CZ1    ",null,7.6,null,215,null,"шт",null,null,0]
[0,199,"L83CZ1    ",null,8.3000000000000007,null,230,null,"шт",null,null,0]
[0,200,"L96CZ1    ",null,9.5,null,270,null,"шт",null,null,0]
[0,201,"K325CZ1    ",null,11.4,null,325,null,"шт",null,null,0]
[0,202,"K375CZ1    ",null,12.7,null,375,null,"шт",null,null,0]
[0,203,"K400CZ1    ",null,14.3,null,400,null,"шт",null,null,0]
[{"$f":"SUM(J241:J243)","v":0},"№","Модель   HBP  R134a","НР"," см3/час","Обмотка","Мощность, ватт   7,2/54,4C","Кол-во в упаковке","Ед. изм.",null,null,0]
[0,{"$f":"B240+1","v":204},"L6170CZ   "," 1/4+",7.9,"Cu   ",850,1,"шт",null,null,0]
[0,{"$f":"B242+1","v":205},"K6210CZ   "," 3/8",11.4,null,1200,null,"шт",null,null,0]
[{"$f":"SUM(J244:J253)","v":0},"№","Модель   LBP  R404a","НР"," см3/час","Обмотка","Мощность, ватт   -23,3/54,4C","Кол-во в упаковке","Ед. изм.",null,null,0]
[0,{"$f":"B243+1","v":206},"LG68CK    "," 3/8",6.8,"Cu   ",350,1,"шт",null,null,0]
[0,{"$f":"B245+1","v":207},"NE2150CK    "," 1/2",12,null,600,null,"шт",null,null,0]
[0,208,"NE2170CK    "," 3/4",13.5,null,700,null,"шт",null,null,0]
[0,209,"NE2178CKA    ",1,16.7,null,880,null,"шт",null,null,0]
[0,210,"NE2180CK    ",1,18,null,910,null,"шт",null,null,0]
[0,211,"NV2192CK    ",1,21.2,null,930,null,"шт",null,null,0]
[0,212,"NV2195CK    "," 1-1/2",27.8,null,1100,null,"шт",null,null,0]
[0,213,"NCT2195CK    "," 1-1/2",31.2,null,1100,null,"шт",null,null,0]
[0,214,"NCT2212CK    "," 1-3/4",34.6,null,1400,null,"шт",null,null,0]
[{"$f":"SUM(J254:J259)","v":0},"№","Модель   HBP  R404a","НР"," см3/час","Обмотка","Мощность, ватт ","Кол-во в упаковке","Ед. изм.",null,null,0]
[null,null,null,null,null,null,"-5/45C  /  -10/45C",null,null,null,null,0]
[0,{"$f":"B253+1","v":215},"NE6210CK    "," 2/5",9,"Cu   ","700  /  500",1,"шт",null,null,0]
[0,{"$f":"B256+1","v":216},"NE6213CK    "," 3/5",12,null,"1100  /  900",null,"шт",null,null,0]
[0,{"$f":"B257+1","v":217},"NCT6228CK    "," 1-1/4",23.6,null,"2400  /  1800",null,"шт",null,null,0]
[0,218,"NCT6240CK    "," 1-3/4",34.4,null,"3600  /  2900",null,"шт",null,null,0]
[{"$f":"SUM(J260:J269)","v":0},"№","Модель   LBP  R290","НР"," см3/час","Обмотка","Мощность, ватт   -23,3/54,4C","Кол-во в упаковке","Ед. изм.",null,null,0]
[{"$f":"J261","v":0},{"$f":"B259+1","v":219},"ML   GQR55U   S"," 1/4",5.5,"AL",265,1,"шт",null,null,0]
[0,{"$f":"B261+1","v":220},"S53CU1   "," 1/3-",5.3,"AL   ",240,null,"шт",null,null,0]
[0,{"$f":"B262+1","v":221},"S68CU1   "," 3/8+",6.8,null,325,null,"шт",null,null,0]
[0,222,"S76CU1   "," 1/2",7.6,null,375,null,"шт",null,null,0]
[0,223,"L83CU1   "," 1/2+",8.3000000000000007,null,400,null,"шт",null,null,0]
[0,224,"L96CU1   "," 3/4-",9.5,null,450,null,"шт",null,null,0]
[0,225,"KK550CU1S   "," 3/4",11.6,null,550,null,"шт",null,null,0]
[0,{"$f":"B267+1","v":226},"KK650CU1   "," 1/2",13.3,null,650,null,"шт",null,null,0]
[0,{"$f":"B268+1","v":227},"NE2168CU   "," 3/4",16.7,"Cu   ",750,null,"шт",null,null,0]
[{"$f":"SUM(J270:J274)","v":0},"№","Модель   M/HBP  R290","НР"," см3/час",null,"Мощность, ватт   7,2/54,4C","Кол-во в упаковке","Ед. изм.",null,null,0]
[0,{"$f":"B269+1","v":228},"NE6214CU    "," 1/2+",12,null,1600,1,"шт",null,null,0]
[0,229,"NE6217CU 1    "," 3/5+",14.2,null,1900,null,"шт",null,null,{"$f":"J272*K272","v":0}]
[0,230,"NE6217CU    "," 3/5+",14.2,null,1900,null,"шт",null,null,0]
[0,231,"NE6220CU    ",1,16.7,null,2200,null,"шт",null,null,0]
[{"$f":"SUM(J275:J282)","v":0},"Ротационный компрессоры GMCC      ",null,null,null,null,null,null,null,null,null,0]
[0,{"$f":"B274+1","v":232},"HSM165 ","1.0HP  /  9000 Btu/h  /  R22            ",null,null,"30 μF",80,"шт",null,null,0]
[0,{"$f":"B276+1","v":233},"HSM215","1.5HP  /  12000 Btu/h  /  R22",null,null,"35 μF",80,"шт",null,null,0]
[0,234,"PH290","2.0HP  /  18000 Btu/h  /  R22",null,null,"35 μF",60,"шт",null,null,0]
[0,235,"PH420 ","2.5HP  /  24000 Btu/h  /  R22",null,null,"50 μF",48,"шт",null,null,0]
[0,236,"ASM130 ","1.5HP  /  12000 Btu/h  /  R410",null,null,null,80,"шт",null,null,0]
[0,237,"ASF185 ","2.0HP  /  18000 Btu/h  /  R410",null,null,null,60,"шт",null,null,0]
[0,238,"PA270 ","2.5HP  /  24000 Btu/h  /  R410",null,null,null,48,"шт",null,null,0]
[{"$f":"SUM(J283:J287)","v":0},"Масла фреоновые",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A283","v":0},"№","Марка","Характеристики",null,"Объем",null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B282+1","v":239},"EMKARATE  RL 32 H","Синтетическое                          R134-404-407-507-410",null,"5-л",null,4,"кан.",null,null,0]
[0,{"$f":"B285+1","v":240},"EMKARATE  RL 68 H",null,null,"5-л",null,null,"кан.",null,null,0]
[0,241,"EMKARATE RL 170 H   ","Винтовой",null,"5-л",null,null,"кан.",null,null,0]
[{"$f":"SUM(J288:J310)","v":0},"Масла фреоновые ERRECOM Италия",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A288","v":0},"№","Марка","Характеристики",null,"Объем",null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B287+1","v":242},"LR-POE 32-1L","Синтетическое                        R134-404-407-507-410",null,"1-л",null,12,"кан.",null,null,0]
[0,{"$f":"B290+1","v":243},"LR-POE 32-5L",null,null,"5-л",null,2,"кан.",null,null,0]
[0,{"$f":"B291+1","v":244},"LR-POE 68-1L",null,null,"1-л",null,12,"кан.",null,null,0]
[0,{"$f":"B292+1","v":245},"LR-POE 68-5L",null,null,"5-л",null,2,"кан.",null,null,0]
[0,{"$f":"B293+1","v":246},"LR-POE 100-5L","Для Винтовых R22 ",null,"5-л",null,2,"кан.",null,null,0]
[0,{"$f":"B294+1","v":247},"LR-POE 100-25L",null,null,"25-л",null,1,"кан.",null,null,0]
[0,{"$f":"B295+1","v":248},"LR-POE 170-5L","Для Винтовых ",null,"5-л",null,2,"кан.",null,null,0]
[0,249,"LR-POE 170-25L",null,null,"25-л",null,1,"кан.",null,null,0]
[0,250,"LUBRICANT 32-1L","Минеральное R12, R22",null,"1-л",null,12,"кан.",null,null,0]
[0,251,"LUBRICANT 32-5L",null,null,"5-л",null,null,"кан.",null,null,0]
[0,252,"LUBRICANT 68-5L",null,null,"5-л",null,2,"кан.",null,null,0]
[0,253,"LUBRICANT 100-5L",null,null,"5-л",null,null,"кан.",null,null,0]
[0,254,"PREMIUM PAG 46 - 1L","Смазки для автокондиционера",null,"1-л",null,12,"кан.",null,null,0]
[0,255,"PREMIUM PAG 100 - 1L",null,null,"1-л",null,null,"кан.",null,null,0]
[0,256,"PUMPS 68 - 1L","Вакуумные масла",null,"1-л",null,null,"кан.",null,null,0]
[0,257,"ALPHA FLUSH - 5L",null,null,"5-л",null,2,"кан.",null,null,0]
[0,258,"BELNET - 5L",null,null,"5-л",null,null,"кан.",null,null,0]
[0,259,"POWER CLEAN IN 600 ML","Очиститель для испарителей",null,"600-мл",null,12,"кан.",null,null,0]
[0,260,"NANO ALKALINE CLEANER 5L","Щелочный очиститель",null,"5-л",null,2,"кан.",null,null,0]
[0,261,"NANO ACID CLEANER 5L","Кислотный очиститель",null,"5-л",null,null,"кан.",null,null,0]
[0,262,"KILLER BACT FOAM - 400 ML","Пена для очистки",null,"400-мл",null,12,"кан.",null,null,0]
[{"$f":"SUM(J311:J332)","v":0},"Хладагенты (фреоны)",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A311","v":0},"№","Марка",null,null,null,"Вес нетто (кг)","Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B310+1","v":263},"R 134A      ARKEMA  ",null,null,null," 13.6",40,"бал",null,null,0]
[0,{"$f":"B313+1","v":264},"R 404A     ARKEMA  ",null,null,null," 10.9",null,"бал",null,null,0]
[0,{"$f":"B314+1","v":265},"R 410A        ARKEMA  ",null,null,null," 11.3",null,"бал",null,null,0]
[0,{"$f":"B315+1","v":266},"R 134a      SANMEI     ",null,null,null," 13.6",40,"бал",null,null,0]
[0,{"$f":"B316+1","v":267},"R 404A      SANMEI",null,null,null," 10.9",null,"бал",null,null,0]
[0,268,"R 507A      SANMEI",null,null,null," 11.3",null,"бал",null,null,0]
[0,269,"R 407C     SANMEI  ",null,null,null," 11.3",null,"бал",null,null,0]
[0,270,"R 410A      SANMEI",null,null,null," 11.3",null,"бал",null,null,0]
[0,{"$f":"B320+1","v":271},"R 32     SANMEI",null,null,null," 9.5",null,"бал",null,null,0]
[0,{"$f":"B321+1","v":272},"R 600A     KOMANS    ",null,null,null," 6.5",null,"бал",null,null,0]
[0,273,"R 290     Refrigerant    ",null,null,null," 5.0",null,"бал",null,null,0]
[{"$f":"J324","v":0},274,"R 1234 yf     KOMANS    ",null,null,null," 5.0",1,"бал",null,null,0]
[0,275,"R 1234 yf     KOMANS    ",null,null,null," 10.0",null,"бал",null,null,0]
[0,276,"R 134a   ",null,null,null," 1.0",12,"бал",null,null,0]
[0,277,"R 404A   ",null,null,null,"0.7",null,"бал",null,null,0]
[0,278,"R 410A  ",null,null,null,"0.8",null,"бал",null,null,0]
[0,279,"R 600A",null,null,null,"0.42",null,"бал",null,null,0]
[0,280,"R 290    ",null,null,null,"0.40",null,"бал",null,null,0]
[0,281,"МАПП ГАЗ",null,null,null,"0.454",null,"бал",null,null,0]
[0,282,"T-CA","Газовая горелка",null,null," 11.8",10,"шт.",null,null,{"$f":"J332*K332","v":0}]
[{"$f":"SUM(J333:J355)","v":0}," Конденсаторы без вентиляторов  KARYER ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A333","v":0},"№","Модель","Мощность квт. R404-507",null,null,"Диаметр вентилятора мм","Кол-во в упаковке","Ед. изм.",null,null,0]
[{"$f":"A333","v":0},null,null,"Δt=10K","Δt=12K","Δt=15K",null,null,null,null,null,0]
[0,{"$f":"B332+1","v":283},"6R 18T 450A 2.25P (авто)",5.0999999999999996,6.1,7.68,"53*20*45cm 1х350",1,"шт",null,null,0]
[0,{"$f":"B336+1","v":284},"HКТ-150FC3-B03   +",11,13.2,16.5,"1 х 500",null,"шт",null,null,0]
[0,285,"HКТ-150GC3-B03",12.5,15,18.8,"1 х 500",null,"шт",null,null,0]
[0,286,"HКТ-150CC1-B03   ",14.3,16.899999999999999,21.2,"1 х 500",null,"шт",null,null,0]
[0,287,"HКТ-150EC1-B03   ",17.100000000000001,20.6,25.7,"1 х 500",null,"шт",null,null,0]
[0,288,"HКТ-250BB1-B03",20.100000000000001,24.1,30.1,"2 х 500",null,"шт",null,null,0]
[0,289,"HКТ-250BC2-B03   ",23.4,28.1,35.200000000000003,"2 х 500",null,"шт",null,null,0]
[0,290,"HКТ-250GB1-B03   +",26.8,32.1,40.200000000000003,"2 х 500",null,"шт",null,null,0]
[0,291,"HКТ-250CC1-B03",29.6,35.5,44.4,"2 х 500",null,"шт",null,null,0]
[0,292,"HКТ-250HC2-B03",33.4,40.1,50.2,"2 х 500",null,"шт",null,null,0]
[0,293,"HКТ-250HD1-B03",40.1,48.1,60.1,"2 х 500",null,"шт",null,null,0]
[0,294,"HКТ-350GD1-B03",54.3,65.099999999999994,81.400000000000006,"3 х 500",null,"шт",null,null,0]
[0,295,"HКТ-2X250FD3-B03",48.5,58,71.8,"2x2 x 500",null,"шт",null,null,0]
[0,296,"HКТ-2X250IC2-B03",60.3,72.3,90.4,"2x2 x 500",null,"шт",null,null,0]
[0,297,"HКТ-2X250HD1-B03",73,87.6,109.4,"2x2 x 500",null,"шт",null,null,0]
[0,298,"HKT-2X350FC1-B03",86.8,104.1,130.19999999999999,"2x3 x 500",null,"шт",null,null,0]
[0,{"$f":"B351+1","v":299},"4R 35T 1987A  V     1450",102,128,153,"2 x 800",null,"шт",null,null,0]
[0,300,"5R 35T 1987A  V     1830",108,145,167,"2 x 800",null,"шт",null,null,0]
[0,301,"4R 35T 2957A  V   2030",139,170,217,"3 x 800",null,"шт",null,null,0]
[0,302,"5R 35T 2957A  V    2610",160,200,250,"3 x 800",null,"шт",null,null,0]
[{"$f":"SUM(J356:J387)","v":0},"Конденсатор Микроканальный (батарея) в корпусе с вентиляторами",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A356","v":0},"№","Модели корпуса","Размер корпуса (мм).  A-B-C","Параметры батареи",null,null,"Площадь    ","Ед. изм.",null,null,0]
[{"$f":"A356","v":0},null,null,null,"Модель микроканаль-ной батареи ","Размер батареи (мм).  A-B-C",null,null,null,null,null,0]
[0,{"$f":"B355+1","v":303},"Корпус с диффузором 1х250мм YDWF68L25P4-250   ","870х350х430","DA01             31"," 340-300-16",null,"1.5m2","компл.",null,null,0]
[0,{"$f":"B359+1","v":304},"Корпус с диффузором 1х300мм YDWF68L35P4-300-PA","870х350х431","SD10                                  31"," 330-284-16",null,"1.5m2","компл.",null,null,0]
[0,{"$f":"B360+1","v":305},null,null,"SD11                             38"," 385-331-16",null,"2.4m2","компл.",null,null,0]
[0,306,"Корпус с диффузором 1х350мм YDWF74L34P4-350-PA","600х500х1000 H","SD12                                50"," 460-415-16",null,"3.5m2","компл.",null,null,0]
[0,307,"Корпус с диффузором 1х500мм YDWF102L70P4-500-PA",null,"SD31 L                    255"," 1500-600-16",null,"14.4m2","компл.",null,null,0]
[0,308,"Корпус с диффузором 2х500мм YDWF102L70P4-500-PA","1800х600х1300","SD18                                347"," 1074-1196-25.4",null,"32m2","компл.",null,null,0]
[0,309,"Корпус с диффузором 1x800мм YSWF138L100P6-800-PA","1200х1100х2200 H","SD18 U            694"," 1074-1196-25.4",null,"32m2","компл.",null,null,0]
[0,310,"Корпус с диффузором 2x800мм YSWF138L100P6-800-PA","2100х1100х2200 H","SD37 U            844"," 1944-1065-20.6",null,"42m2","компл.",null,null,0]
[0,311,null,null,"SD39  U           954","2220-1064-20.6",null,"48m2","компл.",null,null,0]
[0,312,null,null,"SD20 U           1036"," 2000-1042-25.4",null,"53m2","компл.",null,null,0]
[0,313,"Корпус с диффузором 1х250мм YDWF68L25P4-250   ","950х400х500","ZO11-SD10","330-300.7-20",null,null,"компл.",null,null,0]
[0,314,"Корпус с диффузором 1х300мм YDWF68L35P4-300-PA   ",null,"ZO11-SD11","385-347.7-20",null,null,"компл.",null,null,0]
[0,315,"Корпус с диффузором 1х350мм YDWF74L34P4-350-PA","500х500х500","ZO11-SD12","460-432.3-20",null,null,"компл.",null,null,0]
[0,316,"Корпус с диффузором 1х350мм YDWF74L34P4-350-PA","600х500х1000 H","ZO11-SD12","460-432.3-20",null,null,"компл.",null,null,0]
[0,317,"Корпус с диффузором 1х400мм YDWF74L47P4-400-PA","650х500х1200 H","ZO11-SD13","550-516.9-20",null,null,"компл.",null,null,0]
[0,318,"Корпус с диффузором 1х450мм YDWF74L60P4-450","850х550х1300 H","ZO11-SD22","756-509.8-20",null,null,"компл.",null,null,0]
[0,319,"Корпус с диффузором 1х500мм YDWF102L35P4-500","950х550х1300 H","ZO11-SD23      120","803-669.6-20",null,null,"компл."]
[0,320,"Корпус с диффузором 1х500мм YDWF102L70P4-500-PA",null,"ZO11-SD23","803-669.6-20",null,null,"компл.",null,null,0]
[0,321,null,null,"ZO11-SD14","780-770.7-20",null,null,"компл.",null,null,0]
[0,322,"Корпус с диффузором 2х400мм YDWF74L47P4-400-PA","1200х550х1300 H","ZO11-SD15","1074-516.9-32",null,null,"компл.",null,null,0]
[0,323,"Корпус с диффузором 2х450мм YDWF74L60P4-450","1400х550х1300 H","ZO11-SD16","1280-620.3-20",null,null,"компл.",null,null,0]
[0,324,"Корпус с диффузором 2х500мм YDWF102L70P4-500-PA","1500х550х1300 H","ZO11-SD17","1324-639.1-32",null,null,"компл.",null,null,0]
[0,325,"Корпус с диффузором 2х630мм YSWF102L70P4-630","1700х600х1500 H","ZO11-SD30","1544-810.6-20",null,null,"компл.",null,null,0]
[0,326,"Корпус с диффузором 2х630мм YSWF102L70P4-630","1700х900х1500 H","ZO11-SD30 U","1544-810.6-20",null,null,"компл.",null,null,0]
[0,327,"Корпус с диффузором 2х500мм YDWF102L70P4-500-PA","1800х600х1300","ZO11-SD18","1074-1212.5-32",null,null,"компл.",null,null,0]
[0,328,"Корпус с диффузором 2х630мм YSWF102L70P4-630","2100х600х1500 H","ZO11-SD32","1938-857.6-20",null,null,"компл.",null,null,0]
[{"$f":"J385","v":0},329,"Корпус с диффузором 2х630мм YSWF102L70P4-630","2100х900х1500 H","ZO11-SD32 U","1938-857.6-20",null,null,"компл.",null,null,0]
[0,330,"Корпус с диффузором 2х500мм YDWF102L70P4-500-PA","2000х600х1500 ","ZO11-SD19","1274-1362.9-32",null,null,"компл.",null,null,0]
[0,331,"Корпус с диффузором 2x800мм YSWF138L100P6-800-PA","2100х1100х1800 H","ZO11-SD20 U","2000-1058.3-32",null,null,"компл.",null,null,0]
[{"$f":"SUM(J388:J441)","v":0},"Конденсатор  (батарея)   в корпусе с вентиляторами ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A388","v":0},"№","Модели корпуса","Размер корпуса (мм).  A-B-C","Параметры батареи",null,null,"Площадь    ","Ед. изм.",null,null,0]
[{"$f":"A388","v":0},null,null,null,"Модель  батареи ","Размер батареи (мм).  A-B-C",null,null,null,null,null,{"$f":"J390*K390","v":0}]
[0,{"$f":"B387+1","v":332},"Корпус с диффузором 1х350мм YDWF74L34P4-350-PA","900х400х500"," 400х400-3R   95","400х400х100",null,"8.1m2 ","компл.",null,null,0]
[0,{"$f":"B391+1","v":333},"Корпус с диффузором 1х500мм YDWF102L70P4-500-PA",null," 700х700-5R   370","700х700х140",null,"45.2m2 ","компл.",null,null,0]
[0,{"$f":"B392+1","v":334},"Корпус с диффузором 4х450мм YDWF74L60P4-450","2200х650х1200"," 4R35T1250A   800","1350х1200х150",null,"109.2m2 ","компл.",null,null,0]
[0,{"$f":"B393+1","v":335},"Корпус с диффузором 2х630мм YSWF102L70P4-630","2350х650х1200"," 4R35T1530A   950","1600х1200х150",null,"129.0m2 ","компл.",null,null,0]
[0,336,"Корпус с диффузором 4х500мм YDWF102L70P4-500-PA","2350х650х1500"," 1400х1400-3R   950","1400х1400х100",null,"112.7m2 ","компл.",null,null,0]
[0,337,null,null," 1400х1400-4R   1075","1400х1400х120",null,"150.3m2 ","компл.",null,null,0]
[0,338,null,null," 1400х1400-5R   1400","1400х1400х140",null,"187.8m2 ","компл.",null,null,0]
[0,339,"Корпус с диффузором 1х350мм YDWF74L34P4-350-PA",null,"HFNH-2.5/8.0   75","480х160х435",null,"8.0m2 ","компл.",null,null,0]
[0,340,null,"900х450х500   560x450x880 H","HFNH-3.5/12   120","500х170х440",null,"12.0m2 ","компл.",null,null,0]
[0,{"$f":"B399+1","v":341},null,"950х450х540   610x450x1030 H","HFNH-4.6/15   155","560х200х485",null,"15.0m2 ","компл.",null,null,0]
[0,342,"Корпус с диффузором 1х400мм YDWF74L47P4-400-PA",null,"HFNH-5.4/18   177","640х210х540",null,"18.0m2 ","компл.",null,null,0]
[0,343,null,null,"HFNH-6.4/122  207","640х210х540",null,"22.0m2 ","компл.",null,null,0]
[0,344,"Корпус с диффузором 1х450мм YDWF74L60P4-450",null,"HFNH-6.4/122  207","640х210х540",null,"22.0m2 ","компл.",null,null,0]
[0,345,"Корпус с диффузором 1х450мм YDWF74L60P4-450","1100x730x400"," WD 17            150","560х690x100",null,"17m2 ","компл.",null,null,0]
[0,346,"Корпус с диффузором 1х500мм YDWF102L70P4-500-PA","1350х730х500"," WD 17            150","560х690x100",null,"17m2 ","компл.",null,null,0]
[0,347,null,null," WD 23                        175","660х690x100",null,"23m2 ","компл.",null,null,0]
[0,348,null,null," WD 25         215","560х690x101",null,"25m2 ","компл.",null,null,0]
[0,349,null,null," WD 35            240","660х690x100",null,"35m2 ","компл.",null,null,0]
[0,350,null,null," WD 34          262","560х690x101",null,"34m2 ","компл.",null,null,0]
[0,351,null,null," WD 46             316","660х690x100",null,"46m2 ","компл.",null,null,0]
[0,352,"Корпус с диффузором 2х500мм YDWF102L70P4-500-PA","1500х1500х550"," WD 45         351","660х1460x100",null,"44m2 ","компл.",null,null,0]
[0,353,null,null," WD 60             416","760х1460x100",null,"59m2 ","компл.",null,null,0]
[0,354,null,null," WD 65                     505","660х1460x140",null,"66m2 ","компл.",null,null,0]
[0,355,null,null," WD 90            600","760х1460x140",null,"89m2 ","компл.",null,null,0]
[0,356,null,null," WD 88            651","660х1460x150",null,"88m2 ","компл.",null,null,0]
[0,357,null,null," WD 120            772","760х1460x150",null,"118m2 ","компл.",null,null,0]
[0,358,"Корпус с диффузором 4х500мм YDWF102L70P4-500-PA","2400х1500х550"," WD 85              680","1440х1460x100",null,"84m2 ","компл.",null,null,0]
[0,359,null,null," WD 100                     715",null,null,"99m2 ","компл.",null,null,0]
[0,360,null,null," WD 115            755",null,null,"115m2 ","компл.",null,null,0]
[0,361,null,null," WD 125         980","14400х1460x140",null,"126m2 ","компл.",null,null,0]
[0,362,null,null," WD 150              1037",null,null,"149m2 ","компл.",null,null,0]
[0,363,null,null," WD 175        1100",null,null,"173m2 ","компл.",null,null,0]
[0,364,null,null," WD 200       1365","1440х1460x150",null,"199m2 ","компл.",null,null,0]
[0,365,null,null," WD 230       1444",null,null,"231m2 ","компл.",null,null,0]
[0,366,null,null," WD 210              1575","1440х1460x180",null,"210m2 ","компл.",null,null,0]
[0,367,null,null," WD 250            1672",null,null,"248m2 ","компл.",null,null,0]
[0,368,null,null," WD 290                  1770",null,null,"288m2 ","компл.",null,null,0]
[0,369,"Корпус с диффузором 1х500мм YDWF102L70P4-500-PA","820х1200х740","KB 20                180","640х690x100",null,"19m2 ","компл.",null,null,0]
[0,370,null,null,"KB 30                 242","640х690x140",null,"29m2 ","компл.",null,null,0]
[0,371,null,null,"KB 40               306","640х690x150",null,"39m2 ","компл.",null,null,0]
[0,372,"Корпус с диффузором 2х500мм YDWF102L70P4-500-PA                       (расположение вентиляторов сверху)","1440х1200х740","KB 40                       312","1320х690x100",null,"39m2 ","компл.",null,null,0]
[0,373,null,null,"KB 60                       433","1320х690x140",null,"59m2 ","компл.",null,null,0]
[0,374,null,null,"KB 70                    540","1320х690x150",null,"69m2 ","компл.",null,null,0]
[0,375,null,null,"KB 80                       572","1320х690x160",null,"82m2 ","компл.",null,null,0]
[0,376,null,null,"KB 100                 695","1320х690x180",null,"102m2 ","компл.",null,null,0]
[0,377,"Корпус с диффузором 2х630мм YSWF102L70P4-630     (расположение вентиляторов сверху)","20000х1200х980","KB 120             833","1860х920x140",null,"118m2 ","компл.",null,null,0]
[0,378,null,null,"KB 200           1310","1860х920x180",null,"197m2 ","компл.",null,null,0]
[0,379,"Корпус с диффузором 3х630мм YSWF102L70P4-630     (расположение вентиляторов сверху)","27000х1200х980","KB 165                1122","2600х920x140",null,"166m2 ","компл.",null,null,0]
[0,380,null,null,"KB 250                1720","2600х920x180",null,"253m2 ","компл.",null,null,0]
[0,381,"Корпус с диффузором 2x800мм YSWF138L100P6-800-PA    (расположение вентиляторов сверху) ","25000х2000х1400","KBV 260                2850","2400х1000x1400",null,"260m2 ","компл.",null,null,0]
[0,382,null,null,"KBV 300                        3000","2400х1000x1400",null,"300m2 ","компл.",null,null,0]
[{"$f":"SUM(J442:J444)","v":0},"Емкость-молокоохладителя  Fic  Италия",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A442","v":0},"№","Модель",null,"Емкость  литр","Холодопроизводительность       кВт, t -5 +50°C  R404-507",null,"Кол-во в упаковке","Ед. изм",null,null,0]
[{"$f":"J444","v":0},{"$f":"B441+1","v":383},"Молокоохладитель-танк",null,500,"2.7 kw",null,1,"шт.",null,null,0]
[{"$f":"SUM(J445:J449)","v":0},"Барабан льдогенератора    ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A445","v":0},"№","Модель",null,"Производительность   кг./сут",null,"Холодопроизводительность  кВт, t -25 +40°C","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B444+1","v":384},"LRD-1T",null,"1000кг ",null," 5.5 kw",1,"шт.",null,null,0]
[0,{"$f":"B447+1","v":385},"LRD-3T",null,"3000кг ",null," 20.5 kw",null,"шт.",null,null,{"$f":"J448*K448","v":0}]
[0,{"$f":"B448+1","v":386},"LRD-5T",null,"5000кг ",null," 29 kw",null,"шт.",null,null,0]
[{"$f":"SUM(J450:J454)","v":0},"Испарители  потолочные плоские с вентиляторами, с тэнами E1 KARYER",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A450","v":0},"№","Модель  (6mm)   ","Мощность        W R404-507            -8 +40C sc2","Мощность          W R404-507                     -25 +40C  sc3","Ø вент-ра","Тены W   (E1) ","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B449+1","v":387},"EG-A 125AE6",907,728,"1 х 250",400,null,"шт",null,null,0]
[0,{"$f":"B452+1","v":388},"EG-A 225AC6",1208,944,"2 х 250",680,null,"шт",null,null,0]
[0,389,"EG-A 225AD6",1458,1221,"2 х 250",680,null,"шт",null,null,0]
[{"$f":"SUM(J455:J466)","v":0},"Испарители  без вентиляторов, с тэнами E2 KARYER",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A455","v":0},"№","Модель  (7mm)   ","Мощность        kw R404-507            -8 +40C sc2","Мощность  kw R404-507                     -25 +40C  sc3","Ø вент-ра","Тены kw      (E2) ","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B454+1","v":390},"HEA-150AC7-C03     ",8.18,6.45,"1 х 500",4.8499999999999996,1,"шт",null,null,0]
[0,{"$f":"B457+1","v":391},"HEA-150AE7-C03     ",10.71,8.2899999999999991,"1 х 500",7.76,null,"шт",null,null,0]
[0,392,"HEA-150AG7-C03    ",11.96,9.2899999999999991,"1 х 500",7.76,null,"шт",null,null,0]
[0,393,"HEA-250AC7-C03     ",16.399999999999999,12.97,"2 х 500",9.25,null,"шт",null,null,0]
[0,394,"HEA-250AE7-C03    ",21.89,17.07,"2 х 500",14.8,null,"шт",null,null,0]
[0,395,"HEA-250AG7-C03    ",26.05,20.38,"2 х 500",14.8,null,"шт",null,null,0]
[0,396,"HEA-350AE7-C03    ",31.8,25.1,"3 х 500",21.6,null,"шт",null,null,0]
[0,397,"HEA-350AG7-C03    ",38.11,29.91,"3 х 500",21.6,null,"шт",null,null,0]
[0,{"$f":"B464+1","v":398},"HEA-450AE7-C03    ",43.82,"34.22","4 х 500",28,null,"шт",null,null,0]
[0,399,"HEA-450AG7-C03     ","48.85",38.56,"4 х 500",28,null,"шт",null,null,0]
[{"$f":"SUM(J467:J478)","v":0}," Испарители глубокой заморозки и хранения, без вентиляторов, с тэнами E2  KARYER",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A467","v":0},"№","Модель  (10mm)","Мощность       kw R404-507            -8 +40C sc2","Мощность  kw R404-507                    -25 +40C  sc3","Ø вент-ра","Тены kw      (E2) ","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B466+1","v":400},"HEA-150AC10-C03   ",6.6,5.26,"1 х 500",4.8499999999999996,1,"шт",null,null,0]
[0,401,"HEA-150AE10-C03   ",9,7.22,"1 х 500",7.76,null,"шт",null,null,0]
[0,402,"HEA-150AG10-C03   ",10.9,8.68,"1 х 500",7.76,null,"шт",null,null,0]
[0,{"$f":"B471+1","v":403},"HEA-250AC10-C03   ",13.7,10.91,"2 х 500",9.25,null,"шт",null,null,0]
[0,404,"HEA-250AE10-C03   ",18,14.51,"2 х 500",14.8,null,"шт",null,null,0]
[0,{"$f":"B473+1","v":405},"HEA-250AG10-C03   ",22.2,17.850000000000001,"2 х 500",14.8,null,"шт",null,null,0]
[0,406,"HEA-350AE10-C03   ",27.3,21.87,"3 х 500",21.6,null,"шт",null,null,0]
[0,407,"HEA-350AG10-C03   ",33,26.61,"3 х 500",21.6,null,"шт",null,null,0]
[0,{"$f":"B476+1","v":408},"HEA-450AE10-C03   ",36.5,29.31,"4 х 500",28,null,"шт",null,null,0]
[0,409,"HEA-450AG10-C03   ",44,35.270000000000003,"4 х 500",28,null,"шт",null,null,0]
[{"$f":"SUM(J479:J482)","v":0}," Испарители Шоковой заморозки без вентиляторов, с комплектами тэнов. Тэн дренажный. Тэны оттайки батареи. Дополнительно запасная группа тэнов оттайки батареи. KARYER",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A479","v":0},"№","Модель","A-B-C                cm","Мощность  kw R404-507   -31 +40c (dt=6K)","Ø вент-ра","Тены kw      (E2) ","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B478+1","v":410},"HEK-T-263BG10-B08   (30hp)","246-120-115",32,"2 х 630",25,1,"шт",null,null,0]
[0,{"$f":"B481+1","v":411},"EK-T-363BE10-B08   (40hp)","346-120-115",37,"3 х 630",35.54,null,"шт",null,null,0]
[{"$f":"SUM(J483:J523)","v":0},"Испарители  без вентиляторов, с тэнами   (E2) ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A483","v":0},"№","МОДЕЛЬ  6мм","R404 kw -8c ","R404 kw -25c ","вент-ры мм"," A*B*C mm","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B482+1","v":412},"HDE-0.45/2.5  +FAN  E1"," 0.70"," 0.50","1*250","435*390*150",1,"шт",null,null,0]
[0,{"$f":"B485+1","v":413},"HDE-0.9/5.0  +FAN   E1"," 1.26"," 0.90","2*250","745*390*150",null,"шт",null,null,0]
[0,414,"HDE-1.35/7.5  +FAN  E1"," 2.1"," 1.5","3*250","1055*390*150",null,"шт",null,null,0]
[0,415,"HDE-1.8/10.0  +FAN  E1"," 2.70"," 1.90","4*250","1365*390*150",null,"шт",null,null,0]
[0,416,"HDE-2.2/12.5  +FAN  E1"," 3.50"," 2.40","5*250","1700*390*150",null,"шт",null,null,0]
[0,{"$f":"B489+1","v":417},"HDD-3/7"," 2.8",null,"1*300",null,null,"шт",null,null,0]
[0,418,"HDD-4.5/12"," 4.2",null,"2*300",null,null,"шт",null,null,0]
[0,419,"HDD-5.4/15"," 5.0",null,"2*300",null,null,"шт",null,null,0]
[0,420,"HDD-9.4/22"," 8.7",null,"2*350",null,null,"шт",null,null,0]
[0,421,"HDD-1.4/7"," 1.2"," 1.0","1*300","730*390*460",null,"шт",null,null,0]
[0,422,"HDD-2.35/12"," 2.8"," 2.1","2*300","980*390*460",null,"шт",null,null,0]
[0,423,"HDD-3.0/15"," 3.0"," 2.3","2*300","1130*390*460",null,"шт",null,null,0]
[0,424,"HDD-4.0/22"," 4.5"," 3.3","2*350","1310*460*460",null,"шт",null,null,0]
[0,425,"HDD-5.0/25"," 7.0"," 5.3","2*400","1260*400*600",null,"шт",null,null,0]
[0,426,"HDD-6.0/30"," 8.0"," 6.0","2*400","1510*490*550",null,"шт",null,null,0]
[0,427,"HDD-8.0/40","10.0"," 7.5","2*400","1510*490*550",null,"шт",null,null,0]
[0,428,"HDD-9.0/46"," 11.0"," 9.0","1*500","1130*520*760",null,"шт",null,null,0]
[0,429,"HDD-9.6/48"," 12.5",10,"2*450","1530*440*670",null,"шт",null,null,0]
[{"$f":"J503","v":0},430,"HDD-12.0/60"," 14.5"," 11.5","2*500","1810*670*660",null,"шт",null,null,0]
[0,431,"HDD-15.9/80","18.0","14.0","2*500","1810*670*660",null,"шт",null,null,0]
[0,432,"HDD-20.0/100"," 24.0"," 18.0","3*500","2290*670*660",null,"шт",null,null,0]
[0,433,"HDD-24.0/120","27.0"," 21.0","3*500","2710*670*660",null,"шт",null,null,0]
[0,434,"HDD-28.0/140","33.0","25.0","4*500","3110*670*660",null,"шт",null,null,0]
[0,435,"HDD-32.1/160","36.0","28.0","4*500","3510*670*660",null,"шт",null,null,0]
[0,{"$f":"B508+1","v":436},"YDDE-50 2-0808085   (7mm)"," 12.8"," 9.7","2*500","1990*850*880",null,"шт",null,null,{"$f":"J509*K509","v":0}]
[0,437,"YDDE-50 2-1008085   (7mm)"," 17.5"," 11.6","2*500","1990*850*880",null,"шт",null,null,0]
[0,438,"YDDE-63 2-1212100   (7mm)"," 28.6"," 23.2","2*630","2290*1000*1030",null,"шт",null,null,0]
[0,439,"DJ-1.2/7"," 1.9"," 1.5","2*300","980*390*460",null,"шт",null,null,0]
[0,440,"DJ-1.32/10"," 2.5"," 2.0","2*300","1130*390*460",null,"шт",null,null,0]
[0,441,"DJ-2.3/15"," 3.5"," 2.5","2*350","1310*460*460",null,"шт",null,null,0]
[0,442,"DJ-4.0/20"," 6.3"," 5.0","2*400","1510*490*550",null,"шт",null,null,0]
[0,443,"DJ-5.1/30"," 8.0"," 6.0","2*400","1510*490*550",null,"шт",null,null,0]
[0,444,"DJ-7.8/40"," 10.5"," 8.5","2*500","1810*670*660",null,"шт",null,null,0]
[0,445,"DJ-9.5/55"," 12.5"," 10.0","2*500","1810*670*660",null,"шт",null,null,0]
[0,446,"DJ-12.8/70"," 19.0"," 15.0","3*500","2290*670*660",null,"шт",null,null,0]
[0,447,"DJ-15.7/85"," 22.0"," 17.0","3*500","2710*670*660",null,"шт",null,null,0]
[0,448,"DJ-18.5/100"," 25.0"," 20.0","4*500","3110*670*660",null,"шт",null,null,0]
[0,449,"DJ-21.6/115"," 28.0"," 22.0","4*500","3510*670*660",null,"шт",null,null,0]
[0,450,"DJ-23.8/140",38,30,"2*630",null,null,"шт",null,null,0]
[{"$f":"SUM(J524:J531)","v":0},"Испарители  без вентиляторов, с тэнами   (E1)  потолочные двухпоточные",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A524","v":0},"№","МОДЕЛЬ  6мм","R404 kw -8c ","R404 kw -25c ","вент-ры мм","Тены kw E1","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B523+1","v":451},"SEDD-15",3.5,2.8,"2*300"," 2.7",1,"шт",null,null,0]
[0,{"$f":"B526+1","v":452},"SEDD-22",5.0999999999999996,4.0999999999999996,"2*300"," 2.8",null,"шт",null,null,0]
[0,{"$f":"B527+1","v":453},"SEDD-15",6.2,4.8,"3*300"," 2.7",null,"шт",null,null,0]
[0,{"$f":"B528+1","v":454},"SEDD-22",9,6.9,"3*300"," 2.8",null,"шт",null,null,0]
[0,{"$f":"B529+1","v":455},"SEDD-30",11.4,9,"2*350"," 3.5",null,"шт",null,null,0]
[0,{"$f":"B530+1","v":456},"SEDD-40",15.8,12.9,"3*350"," 4.8",null,"шт",null,null,0]
[{"$f":"SUM(J532:J565)","v":0},"Конденсаторы  без вентиляторов",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A532","v":0},"№","МОДЕЛЬ","вент-ры мм","трубы мм","L-K-H mm",null,"Кол-во в упаковке","Ед. изм",null,null,0]
[{"$f":"A532","v":0},null,null,null,null,null,null,null,null,null,null,0]
[0,{"$f":"B531+1","v":457},"HFNH-0.6/2","1*200","10x10","320x130x250",null,null,"шт",null,null,0]
[0,{"$f":"B535+1","v":458},"HFNH-0.9/3","1*200","10x10","320x130x250",null,null,"шт",null,null,0]
[0,{"$f":"B536+1","v":459},"HFNH-1.2/4","1*250","10x10","340x120x300",null,null,"шт",null,null,0]
[0,460,"HFNH-1.7/6.0","1*300","10x10","460x160x385",null,1,"шт",null,null,0]
[0,461,"HFNH-2.5/8.0","1*350","16x16","480x160x435",null,null,"шт",null,null,0]
[0,{"$f":"B539+1","v":462},"HFNH-3.5/12","1*350","16x16","500x170x440",null,null,"шт",null,null,0]
[0,463,"HFNH-4.6/15","1*350","19x16","560x200x485",null,null,"шт",null,null,0]
[0,464,"HFNH-5.4/18","1*400","19x16","640x210x540",null,null,"шт",null,null,0]
[0,465,"HFNH-6.4/22","1*400","19x16","640x210x540",null,null,"шт",null,null,0]
[0,{"$f":"B543+1","v":466},"HFNH-6.4/22","1*450","19x16","640x210x540",null,null,"шт",null,null,0]
[0,{"$f":"B544+1","v":467},"HFNH-6.4/22B","2*350","19x16","940x210x440",null,null,"шт",null,null,0]
[0,{"$f":"B545+1","v":468},"HFNH-7.3/28","2*350","19x16","940x210x490",null,null,"шт",null,null,0]
[0,469,"HFNH-9.7/33","2*400","19x16","1010x210x540",null,null,"шт",null,null,0]
[0,470,"HFNH-12.0/41","2*400","19x16","1010x210x540",null,null,"шт",null,null,0]
[0,471,"HFNH-13.8/50","2*400","22x16","1010x230x640",null,null,"шт",null,null,0]
[0,472,"HFNH-16.2/60","2*400","22x16","1010x230x640",null,null,"шт",null,null,0]
[0,473,"HFNH-20.7/70","4*350","25x19","1170x230x940",null,null,"шт",null,null,0]
[0,474,"HFNH-23.0/80","4*400","25x19","1170x230x1040",null,null,"шт",null,null,0]
[0,475,"HFNH-27.6/100","4*400","28x22","1170x230x1040",null,null,"шт",null,null,0]
[0,476,"HFNH-33.3/120","4*400","32x22","1200x230x1240",null,null,"шт",null,null,0]
[0,477,"HFNH-39.8/140","4*500","32x22","1280x250x1240",null,null,"шт",null,null,0]
[0,478,"HFNH-45.6/160","4*500","32x22","1340x250x1340",null,null,"шт",null,null,0]
[0,{"$f":"B556+1","v":479},"HFNH-49.9/180","4*500","32x22","1460x250x1340",null,null,"шт",null,null,0]
[0,480,"HFNH-72.5/260","6*500","32x25",null,null,null,"шт",null,null,0]
[0,{"$f":"B558+1","v":481},"HFNH-89.6/320","6*500","38x28","2740x300x1340",null,null,"шт",null,null,0]
[0,{"$f":"B559+1","v":482},"HFNHC-25-3","1*450","19x16","630x220x540",null,null,"шт",null,null,0]
[0,483,"HFNHC-35-4","1*500","19x16","730x230x590",null,null,"шт",null,null,0]
[0,484,"HFNHC-41-5","1*500","19x16","810x230x690",null,null,"шт",null,null,0]
[0,485,"HFNHC-55-8","1*630","22x19","900x230x840",null,null,"шт",null,null,0]
[0,486,"HFNHC-80-10","2*500","25x19","1175x250x940",null,null,"шт",null,null,0]
[0,487,"HFNHC-100-15","2*500","28x22","1360x270x890",null,null,"шт",null,null,0]
[{"$f":"SUM(J566:J580)","v":0},"Мотор вентиляторы ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A566","v":0},"№","Наименование","Мощность ватт",null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B565+1","v":488},"FAN radyan ","180мм 0.32A  (левый)                  УПК 20 шт ",null,null,null,20,"шт",null,null,0]
[0,{"$f":"B568+1","v":489},"XD1238A2HSL","Черный вентилятор   40 вт 0.14A  УПК 40 шт",null,null,null,40,"шт",null,null,0]
[0,{"$f":"B569+1","v":490},"YZF45L13P4-5","29 вт 0.20A 1300об/мин     УПК 24 шт  ",null,null,null,24,"шт",null,null,0]
[0,491,"YZF45L20P4-10","36 вт 0.25A  1300об/мин    УПК 24 шт  ",null,null,null,null,"шт",null,null,0]
[0,492,"YZF45L25P4-16","60 вт 0.45A  1300об/мин    УПК 12 шт ",null,null,null,12,"шт",null,null,0]
[{"$f":"J573","v":0},493,"YZF45L40P4-25","90 вт 0.70A   1300об/мин    УПК 12 шт  ",null,null,null,null,"шт",null,null,0]
[0,494,"YZF45L45P4-34","110 вт 0.85A 1300об/мин   УПК 12 шт  ",null,null,null,null,"шт",null,null,0]
[0,495,"Лопасти алюм","200 мм  (всасывание)      ",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B575+1","v":496},"Лопасти алюм","250 мм  (всасывание)      ",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B576+1","v":497},"Лопасти алюм","300 мм  (всасывание)           ",null,null,null,null,"шт",null,null,0]
[0,498," Диффузор  ","200 мм             УПК 24 шт",null,null,null,null,"шт",null,null,{"$f":"J578*K578","v":0}]
[0,499," Диффузор  ","250 мм           УПК 20 шт",null,null,null,null,"шт",null,null,0]
[0,500," Диффузор  ","300 мм             УПК 20 шт",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J581:J627)","v":0},"Вентиляторы  MАER Micro-motor   ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A581","v":0},"№","Модель","Диаметр мм","Мощность Ватт","об/мин.","Произв.   м3/час","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B580+1","v":501},"YDWF68L15P4-200",200,27,1399,400,1,"шт",null,null,0]
[0,{"$f":"B583+1","v":502},"YDWF68L25P4-250",250,45,1357,1100,null,"шт",null,null,0]
[0,{"$f":"B584+1","v":503},"YDWF67L25P2-250",null,114,2579,1500,null,"шт",null,null,0]
[0,{"$f":"B585+1","v":504},"YDWF68L35P4-300",300,89,1354,1800,1,"шт",null,null,0]
[0,{"$f":"B586+1","v":505},"YDWF67L35P2-300",null,168,2592,2400,null,"шт",null,null,0]
[0,506,"YDWF68L35P6-300-PA ",null,49,924,1200,null,"шт",null,null,0]
[0,507,"YDWF68L35P4-300-PA ",null,86,1340,1800,null,"шт",null,null,0]
[0,508,"YDWF68L35P4-300B нагнетание",null,89,1354,1800,null,"шт",null,null,0]
[0,509,"YDWF74L47P4-350",350,192,1381,3000,1,"шт",null,null,0]
[0,510,"YDWF74L34P4-350",null,147,1353,2800,null,"шт",null,null,0]
[0,511,"YDWF74L34P6-350",null,77,903,2000,null,"шт",null,null,0]
[0,512,"YDWF74L34P4-350-PA",null,162,1329,3000,null,"шт",null,null,0]
[0,513,"YDWF74L34P4-350B нагнетание",null,147,1353,2800,null,"шт",null,null,0]
[0,514,"YDWF74L47P4-400",400,219,1352,4000,1,"шт",null,null,0]
[0,515,"YDWF74L47P4-400-PA",null,207,1377,4000,null,"шт",null,null,0]
[0,516,"YDWF74L47P6-400-PA",null,120,915,3000,null,"шт",null,null,0]
[0,517,"YDWF74L47P4-400B нагнетание",null,219,1352,4000,null,"шт",null,null,0]
[0,518,"YDWF74L60P4-450",450,249,1339,5000,1,"шт",null,null,0]
[0,519,"YDWF74L60P6-450-PA ",null,176,888,4000,null,"шт",null,null,0]
[0,520,"YDWF102L45P4-450-7",null,499,1387,6000,null,"шт",null,null,0]
[0,521,"YDWF102L35P4-500",500,424,1323,7000,1,"шт",null,null,0]
[0,522,"YDWF102L35P6-500",null,217,849,5000,null,"шт",null,null,0]
[0,523,"YDWF102L50P4-500-7",null,661,1356,8000,null,"шт",null,null,0]
[0,524,"YSWF102L70P4-500-7       3F",null,795,1396,9000,null,"шт",null,null,0]
[0,525,"YDWF102L45P6-500PA",null,270,869,6000,null,"шт",null,null,0]
[0,526,"YDWF102L70P4-500PA",null,838,1355,8600,null,"шт",null,null,0]
[0,{"$f":"B608+1","v":527},"YDWF102L35P4-500B нагнетание",null,424,1300,7000,null,"шт",null,null,0]
[0,{"$f":"B609+1","v":528},"YSWF102L70P6-630-PA",630,603,899,9877,1,"шт",null,null,0]
[0,{"$f":"B610+1","v":529},"YSWF102L70P4-630",null,937,1378,12000,null,"шт",null,null,0]
[0,530,"YSWF127L80P4-630-7  ШОК",null,2331,1395,18000,null,"шт",null,null,0]
[0,531,"YSWF127L80P4-630 S  ШОК",null,2266,1401,16834,null,"шт",null,null,0]
[0,532,"YSWF127L50P6-710","710   3-F",923,923,12000,1,"шт",null,null,0]
[0,533,"YSWF127L65P6-800","800   3-F",1126,906,16000,1,"шт",null,null,0]
[0,534,"YSWF127L80P6-800-7",null,1477,919,18000,null,"шт",null,null,0]
[0,535,"YSWF138L100P6-800-PA",null,1923,925,24000,null,"шт",null,null,0]
[0,536,"YSWF127L80P6-900","900   3-F",1738,901,22000,1,"шт",null,null,0]
[0,537," Диффузор  200мм","Панель  31х31 см",null,null,null,null,"шт",null,null,0]
[0,538," Диффузор  250мм","Панель  31х31 см",null,null,null,null,"шт",null,null,0]
[0,539," Диффузор  300мм","Панель  43х43 см",null,null,null,null,"шт",null,null,0]
[0,540," Диффузор  350мм","Панель  42.5х42.5 см",null,null,null,null,"шт",null,null,0]
[0,541," Диффузор  400мм","Панель  48х48 см",null,null,null,null,"шт",null,null,0]
[0,542," Диффузор  450мм","Панель  57,5х57,5см",null,null,null,null,"шт",null,null,0]
[0,543," Диффузор  500мм ","Панель  66х66см",null,null,null,null,"шт",null,null,0]
[0,544," Диффузор  630мм","Панель  80х80см",null,null,null,null,"шт",null,null,0]
[0,545," Диффузор  800мм ","Панель  97х97см",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J628:J633)","v":0},"Вентиляторы ZIEHL-ABEGG ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A628","v":0},"№","Модель","Диаметр мм","Напряж. Вольт","Мощность Ватт","Произв.  м3/час","Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B627+1","v":546},"FN050-4EK.4I.V7P1",500,220,720,9000,1,"шт",null,null,0]
[0,{"$f":"B630+1","v":547},"FN050-VDK.4I.V7P1",500,380,840,9500,null,"шт",null,null,0]
[0,{"$f":"B631+1","v":548},"FN050-6EK.4F.V7P1",500,220,300,6300,null,"шт",null,null,0]
[0,{"$f":"B632+1","v":549},"FN080-SDQ.6N.V7  ",800,380,1800,25000,null,"шт",null,null,0]
[{"$f":"SUM(J634:J661)","v":0},"Тэны для ВОПа  230v ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A634","v":0},"№","Тэны Длина ",null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B633+1","v":550},"450-мм      ",null,null,"300-Вт",null,null,"шт",null,null,0]
[{"$f":"J637","v":0},{"$f":"B636+1","v":551},"550-мм      ",null,null,"300-Вт",null,null,"шт",null,null,0]
[0,552,"670-мм      ",null,null,"400-Вт",null,null,"шт",null,null,0]
[0,553,"830-мм      ",null,null,"500-Вт",null,null,"шт",null,null,0]
[0,554,"950-мм      ",null,null,"500-Вт",null,null,"шт",null,null,0]
[0,555,"1200-мм      ",null,null,"600-Вт",null,null,"шт",null,null,0]
[0,556,"1320-мм      ",null,null,"600-Вт",null,null,"шт",null,null,0]
[0,557,"1400-мм      ",null,null,"700-Вт",null,null,"шт",null,null,0]
[0,558,"1620-мм      ",null,null,"800-Вт",null,null,"шт",null,null,0]
[0,559,"1800-мм      ",null,null,"800-Вт",null,null,"шт",null,null,0]
[0,560,"2000-мм      ",null,null,"900-Вт",null,null,"шт",null,null,0]
[0,561,"2200-мм      ",null,null,"1000-Вт",null,null,"шт",null,null,0]
[0,562,"2450-мм      ",null,null,"1000-Вт",null,null,"шт",null,null,0]
[0,563,"2900-мм      ",null,null,"1100-Вт",null,null,"шт",null,null,0]
[0,564,"3310-мм      ",null,null,"1200-Вт",null,null,"шт",null,null,0]
[0,565,"3550-мм      ",null,null,"1200-Вт",null,null,"шт",null,null,0]
[0,{"$f":"B651+1","v":566},"400-мм       ",null,null,"200-Вт",null,null,"шт",null,null,0]
[0,{"$f":"B652+1","v":567},"500-мм       ",null,null,"300-Вт",null,null,"шт",null,null,0]
[0,568,"700-мм       ",null,null,"300-Вт",null,null,"шт",null,null,0]
[0,569,"800-мм       ",null,null,"400-Вт",null,null,"шт",null,null,0]
[0,570,"900-мм       ",null,null,"400-Вт",null,null,"шт",null,null,{"$f":"J656*K656","v":0}]
[0,{"$f":"B656+1","v":571},"1300-мм       ",null,null,"600-Вт",null,null,"шт",null,null,0]
[0,572,"2500-мм       ",null,null,"1200-Вт",null,null,"шт",null,null,0]
[0,573,"2700-мм       ",null,null,"1300-Вт",null,null,"шт",null,null,0]
[0,{"$f":"B659+1","v":574},"3500-мм       ",null,null,"1700-Вт",null,null,"шт",null,null,0]
[0,575,"4000-мм       ",null,null,"2000-Вт",null,null,"шт",null,null,0]
[{"$f":"SUM(J662:J674)","v":0},"Гибкие Тэны для дренажной оттайки ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A662","v":0},"№","Наименование","Длина мм",null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B661+1","v":576},"Гибкий тэн","1 мт   40w",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B664+1","v":577},"Гибкий тэн","1,5 мт   60w",null,null,null,null,"шт",null,null,0]
[0,578,"Гибкий тэн","2 мт   80w",null,null,null,null,"шт",null,null,0]
[0,579,"Гибкий тэн","3 мт   120w",null,null,null,null,"шт",null,null,0]
[0,580,"Гибкий тэн","4 мт   160w",null,null,null,null,"шт",null,null,0]
[0,581,"Гибкий тэн","5 мт   200w",null,null,null,null,"шт",null,null,0]
[0,582,"Гибкий тэн","6 мт   240w",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B670+1","v":583},"Гибкий тэн","7 мт   280w",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B671+1","v":584},"Гибкий тэн  AKO-5234","1-мт 40w (50-м в -рулоне)  ",null,"УПК 1 рул",null,null,"рул",null,null,0]
[0,{"$f":"B672+1","v":585},"Гибкий тэн лента","для 500мм вентилятора",null,null,null,null,"шт",null,null,0]
[0,586,"Гибкий тэн лента","для 630мм вентилятора",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J675:J710)","v":0},"Теплообменники для охлаждения жидкости - кожухотрубные ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A675","v":0},"№","Модель             ","R404-507  (-10 / +40с)",null,"R407C  (+2 / +50c)",null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[{"$f":"A675","v":0},null,null," KW  ","m3/h","KW  ","m3/h",null,null,null,null,0]
[0,{"$f":"B674+1","v":587},"HRS-20-R",6.65,1.2,19.899999999999999,3.4,1,"шт",null,null,0]
[0,{"$f":"B678+1","v":588},"HRS-33-R",10.45,2,24.51,4.2,null,"шт",null,null,0]
[0,{"$f":"B679+1","v":589},"BE-40",17.75,3.3,38.5,6.6,null,"шт",null,null,0]
[0,590,"BE-50",23.2,4.4000000000000004,47.7,8.1999999999999993,null,"шт",null,null,0]
[0,591,"HRS-60-R",28.5,5.3,62.5,10.3,null,"шт",null,null,0]
[0,592,"HRS-85-R",46,8.6,83.3,14.6,null,"шт",null,null,0]
[0,593,"BE-100",49.2,9.1999999999999993,93.7,16.100000000000001,null,"шт",null,null,0]
[0,594,"HRS-125-R",null,null,122.1,21.5,null,"шт",null,null,0]
[0,595,"HRS-144-R",87.5,16.399999999999999,142.4,24.7,null,"шт",null,null,0]
[0,596,"HRS-168-R",null,null,161.69999999999999,28.7,null,"шт",null,null,0]
[0,597,"HRS-200-R",null,null,203.2,34.299999999999997,null,"шт",null,null,0]
[0,598,"RCS-205",128.5,24.1,243.4,41.8,null,"шт",null,null,0]
[0,{"$f":"B689+1","v":599},"BE-205",128.5,24.1,243.4,41.8,null,"шт",null,null,0]
[0,600,"BE-245",150,28.1,272,46.7,null,"шт",null,null,0]
[0,601,"BE-290",188.5,35.4,336.3,57.7,null,"шт",null,null,0]
[0,602,"HRS-396-R",254.6,47.7,417.9,68,null,"шт",null,null,0]
[0,603,"BED-100",49.2,9.1999999999999993,93.7,16.100000000000001,null,"шт",null,null,0]
[{"$f":"J695","v":0},604,"HRD-125-R",null,null,122.1,21.5,null,"шт",null,null,0]
[0,605,"HRD-144-R",87.5,16.399999999999999,142.4,24.7,null,"шт",null,null,0]
[0,606,"HRD-168-R",102,19.100000000000001,161.69999999999999,28.7,null,"шт",null,null,0]
[0,607,"HRD-200-R",128.5,24.1,243.4,41.8,null,"шт",null,null,0]
[0,608,"HRD-250-R",150,28.1,247.8,42.9,null,"шт",null,null,0]
[0,609,"HRD-296-R",150,28.1,294.5,50.8,null,"шт",null,null,0]
[0,610,"HRD-345-R",216.4,40.6,353.8,59.2,null,"шт",null,null,0]
[0,611,"HRD-396-R",254.6,47.7,417.9,68,null,"шт",null,null,0]
[0,612,"HRD-452-R",283,53.1,449.4,77.599999999999994,null,"шт",null,null,0]
[0,613,"BED-500",330.5,62,566.4,97.2,null,"шт",null,null,0]
[0,614,"HRD-505-R",330.5,62,475.7,86.7,null,"шт",null,null,0]
[0,{"$f":"B705+1","v":615},"HRD-580-R",370.6,69.5,568.4,99.9,null,"шт",null,null,0]
[0,{"$f":"B706+1","v":616},"BED-590",370.6,69.5,622,106.8,null,"шт",null,null,0]
[0,617,"HRD-670-R",380,71.3,635,115,null,"шт",null,null,0]
[0,618,"BED-660",380,71.3,722,123.9,null,"шт",null,null,0]
[0,619,"HRD-777-R",null,null,725.2,133.4,null,"шт",null,null,0]
[{"$f":"SUM(J711:J742)","v":0},"Теплообменники для охлаждения жидкости - пластинчатые ",null,null,null,null,null,null,null,null,null,{"$f":"J711*K711","v":0}]
[{"$f":"A711","v":0},"№","Модель             ","KW R407C  +7 +12C  ",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B710+1","v":620},"HU50-10",5,null,null,null,1,"шт",null,null,0]
[0,{"$f":"B713+1","v":621},"HU50-14",7,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B714+1","v":622},"MB-08-20",11,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B715+1","v":623},"HU50-20",11,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B716+1","v":624},"HU50-24",14,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B717+1","v":625},"HU50-30",18,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B718+1","v":626},"HU50-40",23,null,null,null,null,"шт",null,null,0]
[0,627,"HU50-50",29,null,null,null,null,"шт",null,null,0]
[0,628,"HU50-60",33,null,null,null,null,"шт",null,null,0]
[0,629,"HU50-70",38,null,null,null,null,"шт",null,null,0]
[0,630,"HU50-80",42,null,null,null,null,"шт",null,null,0]
[0,631,"MB-08-90",45,null,null,null,null,"шт",null,null,0]
[0,632,"HU50-90",45,null,null,null,null,"шт",null,null,0]
[0,633,"HU50-100",48,null,null,null,null,"шт",null,null,0]
[0,634,"MB-08-100",48,null,null,null,null,"шт",null,null,0]
[0,635,"HU95-30",28,null,null,null,1,"шт",null,null,0]
[0,636,"HU95-40",38,null,null,null,null,"шт",null,null,0]
[0,637,"HU95-50",48,null,null,null,null,"шт",null,null,0]
[0,638,"HU95-60",58,null,null,null,null,"шт",null,null,0]
[0,639,"HU95-70",68,null,null,null,null,"шт",null,null,0]
[0,640,"HU95-80",78,null,null,null,null,"шт",null,null,0]
[0,641,"HU95-100",97,null,null,null,null,"шт",null,null,0]
[0,642,"HU95-120",116,null,null,null,null,"шт",null,null,0]
[0,643,"HU100-80",82,null,null,null,null,"шт",null,null,0]
[0,644,"HU100-100",104,null,null,null,null,"шт",null,null,0]
[0,645,"HU100-120",125,null,null,null,null,"шт",null,null,0]
[0,646,"HU100-41+41 ",82,null,null,null,null,"шт",null,null,0]
[0,647,"HU100-51+51",106,null,null,null,null,"шт",null,null,0]
[0,648,"HU100-61+61",126,null,null,null,null,"шт",null,null,0]
[0,649,"Реле протока жидкости MGS1001    10А                                               ",null,null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J743:J840)","v":0},"Терморегулирующие вентили  ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"SUM(J744:J824)","v":0},"№","Модель","tº - режим","R404 / 507            ","артикул","MOP","Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B742+1","v":650},"ERSE-2-Z ton"," -17 -40c","7.0-kw  10*12*6мм               ","P-169220","  -10C",1,"шт",null,null,0]
[0,{"$f":"B745+1","v":651},"ERSE-3-C ton"," +10 -23c","10.5-kw  12*22*6мм     ","P-169260"," +15C",null,"шт",null,null,0]
[0,{"$f":"B746+1","v":652},"SSE-3-C ton"," +10 -23c","10.5-kw   12*22*6мм               ","P-128934"," +15C",null,"шт",null,null,0]
[0,{"$f":"B747+1","v":653},"SSE-3-Z ton"," -17 -40c","10.5-kw   12*22*6мм               ","P-128944","  -10C",null,"шт",null,null,0]
[0,654,"ERSE-4-C ton"," +10 -23c","14.0-kw  12*22*6мм     ","P-169278"," +15C",null,"шт",null,null,0]
[0,655,"ERSE-4-Z ton"," -17 -40c","14.0-kw  12*22*6мм        ","P-169280","  -10C",null,"шт",null,null,0]
[0,656,"SSE-4-C ton"," +10 -23c","14.0-kw  12*22*6мм        ","P-128936"," +15C",null,"шт",null,null,0]
[0,657,"SSE-4-Z ton"," -17 -40c","14.0-kw  12*22*6мм       ","P-128945","  -10C",null,"шт",null,null,0]
[0,658,"ERSE-6-C ton"," +10 -23c","21.0-kw  16*22*6мм      ","P-169287"," +15C",null,"шт",null,null,0]
[0,659,"ERSE-6-Z ton"," -17 -40c","21.0-kw   16*22*6мм       ","P-169288","  -10C",null,"шт",null,null,0]
[0,660,"SSE-6-C ton"," +10 -23c","21.0-kw  16*22*6мм       ","P-128937"," +15C",null,"шт",null,null,0]
[{"$f":"J756","v":0},661,"SSE-6-Z ton"," -17 -40c","21.0-kw   16*22*6мм      ","P-128946","  -10C",null,"шт",null,null,0]
[0,662,"SSE-7-C ton"," +10 -23c","24.6-kw  16*22*6мм       ","P-128938"," +15C",null,"шт",null,null,0]
[0,663,"SSE-7-Z ton"," -17 -40c","24.6-kw   16*22*6мм       ","P-128947","  -10C",null,"шт",null,null,0]
[0,664,"OSE-9-Z ton"," -17 -40c","31.5-kw  22*28*6мм      ","P-124216",null,null,"шт",null,null,0]
[0,665,"SSE-10-C ton"," +10 -23c","35-kw   22*28*6мм       ","P-128226"," +15C",null,"шт",null,null,0]
[0,666,"SSE-10-Z ton"," -17 -40c","35-kw  22*28*6мм       ","P-128235","  -10C",null,"шт",null,null,0]
[0,667,"OSE-12-C ton"," +10 -23c","42-kw   22*28*6мм    ","P-124129"," +15C",null,"шт",null,null,0]
[0,668,"OSE-12-Z ton"," -17 -40c","42-kw      22*28*6мм       ","P-124332","  -10C",null,"шт",null,null,0]
[0,669,"OSE-21-C ton"," +10 -23c","74-kw   28*35*6мм             ","P-124215"," +15C",null,"шт",null,null,0]
[0,{"$f":"B764+1","v":670},"OSE-30-C ton"," +10 -23c","105-kw 28*35*6мм      ","P-124819"," +15C",null,"шт",null,null,0]
[0,{"$f":"B765+1","v":671},"OSE-35-C ton"," +10 -23c","125-kw   28*35*6мм       ","P-124156",null,null,"шт",null,null,0]
[0,672,"OSE-45-C ton"," +10 -23c","160-kw   28*35*6мм       ","P-124127",null,null,"шт",null,null,0]
[0,{"$f":"B767+1","v":673},"SSE-7-ZР ton  ШОК"," -25 -40c","24.6-kw   16*22*6мм       ","P-128957",null,null,"шт",null,null,0]
[0,674,"OSE-9-ZР ton  ШОК"," -25 -40c","31.5-kw  22*28*6мм        ","P-124224",null,null,"шт",null,null,0]
[0,675,"SSE-10-ZР ton  ШОК"," -25 -40c","35-kw   16*22*6мм        ","P-128221",null,null,"шт",null,null,0]
[0,676,"ERVE-3-GA ton","R22 / R407C","10.6kw      12*16*6мм        ","P-168749"," +15C",1,"шт",null,null,{"$f":"J771*K771","v":0}]
[0,677,"ERVE-4-GA ton",null," 14.0kw      12*16*6мм        ","P-168754",null,null,"шт",null,null,0]
[0,678,"ERVE-5-GA ton",null," 17.6kw      12*16*6мм       ","P-168760",null,null,"шт",null,null,0]
[0,679,"ERVE-6-GA ton",null," 21.0kw      12*16*6мм       ","P-168768",null,null,"шт",null,null,0]
[0,680,"ERVE-8-GA ton",null," 28kw      16*22*6мм       ","P-168773",null,null,"шт",null,null,0]
[0,681,"ERVE-10-GA ton",null," 35kw      16*22*6мм      ","P-168777",null,null,"шт",null,null,0]
[0,682,"ERVE-12-GA ton",null," 42kw       16*22*6мм        ","P-168781",null,null,"шт",null,null,0]
[0,683,"SVE-15- ton",null," 53kw       22*28*6мм         ","P-129409",null,null,"шт",null,null,0]
[0,684,"EBSVE-20- ton",null," 70kw       22*28*6мм        ","P-163697",null,null,"шт",null,null,0]
[0,685,"OVE-30- ton",null," 105kw       28*35*6мм        ","P-124310",null,null,"шт",null,null,0]
[0,686,"OVE-40- ton",null,"140kw       28*35*6мм        ","P-124317",null,null,"шт",null,null,0]
[0,687,"OVE-55- ton",null,"193kw       28*35*6мм        ","P-124331",null,null,"шт",null,null,0]
[0,{"$f":"B782+1","v":688},"OVE-70- ton",null," 246kw       28*35*6мм        ","P-124345",null,null,"шт",null,null,0]
[0,{"$f":"B783+1","v":689},"RFGD03E-2.0-1500 1","RFGD03E R404 / R507               -8С/+40С      sc2"," 5.7kw       3/8*5/8*1/4  ODF",10205411602," +15C",1,"шт",null,null,0]
[0,690,"RFGD03E-2.5-1502 2",null," 7.7kw       1/2*7/8*1/4  ODF",10205411902,null,null,"шт",null,null,0]
[0,691,"RFGD03E-4.0-1504 3",null," 11.3kw       1/2*7/8*1/4   ODF",10205411802,null,null,"шт",null,null,0]
[0,692,"RFGD03E-5.0-1506 4",null," 15.1kw       5/8*7/8*1/4   ODF",10205411702,null,null,"шт",null,null,0]
[0,693,"RFGD03E-6.0-1508 5",null," 17.7kw       5/8*7/8*1/4   ODF",10205412002,null,null,"шт",null,null,0]
[0,694,"RFGD03E-7.5-1510 6",null," 22.4kw       5/8*7/8*1/4   ODF",10205412102,null,null,"шт",null,null,0]
[0,695,"RFGD03E-9.0-628 7",null,"26.9kw       5/8*1-1/8*1/4   ODF",10205061702,null,null,"шт",null,null,0]
[0,696,"RFGD03E-11.0-632 8",null," 33.7kw       7/8*1-1/8*1/4   ODF",10205062102,null,null,"шт",null,null,0]
[0,697,"RFGD03E-13.0-636 9",null," 40.3kw       7/8*1-3/8*1/4   ODF",10205062502,null,null,"шт",null,null,0]
[0,698,"RFGD03E-2.0-1514 1","RFGD03E R404 / R507       -25С/+40С      sc3"," 3.7kw       3/8*5/8*1/4  ODF",10205412202," -10C",1,"шт",null,null,0]
[0,699,"RFGD03E-2.5-1516 2",null," 4.9kw       1/2*7/8*1/4  ODF",10205412302,null,null,"шт",null,null,0]
[0,700,"RFGD03E-4.0-1518 3",null," 7.2kw       1/2*7/8*1/4  ODF",10205412402,null,null,"шт",null,null,0]
[0,701,"RFGD03E-5.0-1520 4",null," 9.7kw       5/8*7/8*1/4  ODF",10205412502,null,null,"шт",null,null,0]
[0,702,"RFGD03E-6.0-1522 5",null," 11.4kw       5/8*7/8*1/4  ODF",10205412602,null,null,"шт",null,null,0]
[0,703,"RFGD03E-7.5-1524 6",null," 14.5kw       5/8*7/8*1/4  ODF",10205412702,null,null,"шт",null,null,0]
[0,704,"RFGD03E-9.0-328 7",null," 16.7kw       5/8*1-1/8*1/4  ODF",10205413002,null,null,"шт",null,null,0]
[0,705,"RFGD03E-11.0-332 8",null," 20.6kw       7/8*1-1/8*1/4  ODF",10205410902,null,null,"шт",null,null,0]
[0,706,"RFGD03E-13.0-336 9",null," 25.1kw       7/8*1-3/8*1/4  ODF",10205411002,null,null,"шт",null,null,0]
[0,707,"RFGD02E-5.0-1312 3","RFGD02E    R22 / R407C   +2С/+50С      "," 17.1kw       1/2*7/8*1/4  ODF",10205404502," +15C",1,"шт",null,null,0]
[0,708,"RFGD02E-7.0-1316 4",null," 22.6kw       5/8*7/8*1/4  ODF",10205372802,null,null,"шт",null,null,0]
[0,709,"RFGD02E-8.5-1302 5",null," 27.4kw       5/8*7/8*1/4  ODF",10205217802,null,null,"шт",null,null,0]
[0,710,"RFGD02E-10.0-1303 6",null," 34.1kw       5/8*7/8*1/4  ODF",10205218902,null,null,"шт",null,null,0]
[0,711,"RFGD02E-12.0-638 7",null," 41.1kw       5/8*1-1/8*1/4  ODF",10205062702,null,null,"шт",null,null,0]
[0,712,"RFGD02E-15.0-642 8",null," 51.2kw       7/8*1-1/8*1/4  ODF",10205063102,null,null,"шт",null,null,0]
[0,713,"RFGD02E-18.0-646 9",null," 60.8kw       7/8*1-3/8*1/4  ODF",10205063502,null,null,"шт",null,null,0]
[0,714,"RFGD05E-4.5-1902 2","RFGD05E R410A     +2С/+50С    "," 15.7kw       1/2*7/8*1/4  ODF",10205347102," +15C",1,"шт",null,null,0]
[0,715,"RFGD05E-6.5-1909 3",null," 22.7kw       1/2*7/8*1/4  ODF",10205346902,null,null,"шт",null,null,0]
[0,716,"RFGD05E-9.0-1905 4",null," 30.0kw       5/8*7/8*1/4  ODF",10205347002,null,null,"шт",null,null,0]
[0,717,"RFGD05E-11.0-1906 5",null," 35.1kw       5/8*7/8*1/4  ODF",10205359402,null,null,"шт",null,null,0]
[0,718,"RFGD05E-13.0-1907 6",null," 44.7kw       5/8*7/8*1/4  ODF",10205315402,null,null,"шт",null,null,0]
[0,719,"RFGD05E-15.0-648 7",null," 52.8kw       5/8*1-1/8*1/4  ODF",10205063702,null,null,"шт",null,null,0]
[0,720,"RFGD05E-19.0-652 8",null," 66.0kw       7/8*1-1/8*1/4  ODF",10205064102,null,null,"шт",null,null,0]
[0,721,"RFGD05E-23.0-656 9",null," 78.1kw       7/8*1-3/8*1/4  ODF",10205064502,null,null,"шт",null,null,0]
[{"$f":"J817","v":0},722,"RFKH03E-4.8-311","R404 / R507","      3/8*1/2*1/4    резьба  ",10201009102," -10C",1,"шт",null,null,0]
[0,723,"RFKH03E-4.8-310",null,"      3/8*1/2*1/4    пайка",10201005802,null,null,"шт",null,null,0]
[0,724,"RFKH03E-4.8-217",null,"      3/8*1/2*1/4    резьба  ",10201008502," +15C",null,"шт",null,null,0]
[0,725,"RFKH03E-4.8-216",null,"      3/8*1/2*1/4    пайка",10201008602,null,null,"шт",null,null,0]
[0,726,"RFKH02E-6.3-208","R22 / R407C","      3/8*1/2*1/4    резьба  ",10201007502," +15C",1,"шт",null,null,0]
[0,727,"RFKH05E-7.6-226","R410A","      3/8*1/2*1/4    пайка",10201010002," +15C",null,"шт",null,null,0]
[0,728,"RFK-A04-038011",null,"      3/8 переходник под пайку  ",20201002502,null,1,"шт",null,null,0]
[0,729,"RFK-A04-038012",null,"      1/4 переходник под пайку  ",20201002602,null,null,"шт",null,null,0]
[{"$f":"SUM(J825:J840)","v":0},730,"Модель","R404-507               -8С/+40С sc2","R404-507                             -25С/+40С sc3","R407C                  +2С/+50С","R410A                   +2С/+50С",null,null,null,null,0]
[0,731,"RFKH-023-0X","0,71 kw","0,6 kw"," 1,0 kw"," 1,2 kw",10,"шт",null,null,0]
[0,732,"RFKH-023-00","1,3 kw","0,95 kw"," 2,0 kw"," 2,3 kw",null,"шт",null,null,0]
[0,733,"RFKH-023-01","2,5 kw","1,5 kw"," 3,8 kw"," 4,3 kw",null,"шт",null,null,0]
[0,734,"RFKH-023-02","3,3 kw","1,8 kw"," 5,1 kw"," 5,3 kw",null,"шт",null,null,0]
[0,735,"RFKH-023-03","5,7 kw","3,1 kw"," 8,9 kw"," 9,6 kw",null,"шт",null,null,0]
[0,736,"RFKH-023-04","8,4 kw","4,5 kw"," 13,2 kw"," 14,5 kw",null,"шт",null,null,0]
[0,737,"RFKH-023-05","10,9 kw","5,8 kw"," 17,2 kw"," 18,2 kw",null,"шт",null,null,0]
[0,738,"RFKH-023-06","13,7 kw","7,2 kw"," 21,8 kw"," 22,8 kw",null,"шт",null,null,{"$f":"J833*K833","v":0}]
[0,739,"SEK 45-01","        5/8*5/8  ODF",null,"Комплект ЭРВ в составе: контроллер серии SEK, электронный расширительный клапан, датчик давления с кабелем  Packard, датчик температуры",null,null,"шт",null,null,0]
[0,{"$f":"B834+1","v":740},"SEK 52-01","        5/8*5/8  ODF",null,null,null,null,"шт",null,null,0]
[0,741,"SEK 55-01","        5/8*5/8  ODF",null,null,null,null,"шт",null,null,0]
[0,742,"SEK 62-01","        5/8*5/8  ODF",null,null,null,null,"шт",null,null,0]
[0,743,"VPF 100 H01","        1-1/8*1-1/8  ODF",null,"Электронный расширительный вентиль серии  VPF",null,null,"шт",null,null,0]
[0,744,"VPF 150 H01","        1-1/8*1-3/8  ODF",null,null,null,null,"шт",null,null,0]
[0,745,"Y 08 A","8 м","Соединительный кабель для ЭРВ серии VPF",null,null,null,"шт",null,null,0]
[{"$f":"SUM(J841:J858)","v":0},"№","Модель","Электронные Терморегулирующие вентили",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B840+1","v":746},"SER-20 -ton","Электронное ТРВ R22, 134, 404, 407, 507       5/8 - 7/8         SPORLAN",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B842+1","v":747},"SEI-30 -ton","Электронное ТРВ R22, 134, 404, 407, 507       1 1/8 - 1 3/8     SPORLAN",null,null,null,null,"шт",null,null,0]
[0,748,"SEI-50 -ton","Электронное ТРВ R22, 134, 404, 407, 507       1 1/8 - 1 3/8     SPORLAN",null,null,null,null,"шт",null,null,0]
[0,749,"ETS 12C  ","034G7502   ШОК Электронное ТРВ с приводом без смотрового стекла    Danfoss              ",null,null,null,null,"шт",null,null,0]
[0,750,"E3V45SSR00   CAREL","E3V-45 SMART со смотровым стеклом,  диам.трубы: 18-22mm  (404a -5 / 50C 20-квт   407C +2 / 50C  35-квт)            ",null,null,null,null,"шт",null,null,0]
[0,751,"E3V55SSS00   CAREL","E3V-55 SMART со смотровым стеклом,  диам.трубы: 22-28mm  (404a -5 / 50C 35-квт   407C +2 / 50C  50-квт)            ",null,null,null,null,"шт",null,null,0]
[0,752,"E4V95BST00   CAREL","E4V-95 INTEGRAL SCREW со смотровым стеклом,  диам.трубы: 28-35mm  (404a  -5 / 50C  90-квт  407C  +2 / 50C 160-квт)              ",null,null,null,null,"шт",null,null,0]
[0,753,"E5VA2AST00   CAREL","E5VA2   INTEGRAL SCREW со смотровым стеклом,  диам.трубы: 28-35mm  (407C  +2 / 50C 200-квт)              ",null,null,null,null,"шт",null,null,0]
[0,754,"E5VA5AST00   CAREL","E5VA5   INTEGRAL SCREW со смотровым стеклом,  диам.трубы: 28-35mm  (407C  +2 / 50C 250-270-квт)              ",null,null,null,null,"шт",null,null,0]
[0,755,"EVD0000E20   CAREL","Контроллер   EVOLUTION UNIVERSAL",null,null,"комп-лект",1,"шт",null,null,0]
[0,756,"EVD0000UC0   CAREL","Контроллер для аварийного закрытия   ULTRACAR",null,null,null,null,"шт",null,null,0]
[0,757,"TRADRFE240   CAREL","Трансформатор  230 / 24v",null,null,null,null,"шт",null,null,0]
[0,758,"E2VCABS300   CAREL","Кабель экранированный",null,null,null,null,"шт",null,null,0]
[0,759,"SPKTOO13P1   CAREL","Датчик давления  1-9.3 bar",null,null,null,null,"шт",null,null,0]
[0,760,"NTC060HF01   CAREL","Датчик  температуры IP67 -50T90 чувствительный элемент",null,null,null,null,"шт",null,null,0]
[0,761,"SPKC002311K   CAREL","Кабель датчика давления   AWG 3 WIRES",null,null,null,null,"шт",null,null,0]
[0,762,"EVDIS00RU0   CAREL","Дисплей Контроллера для электронного ТРВ ",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J859:J862)","v":0},"№","Модель","Термостатические элементы   Danfoss",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B858+1","v":763},"TEZ 20","067B3371   R407C   MOP +15C",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B860+1","v":764},"TEZ 55","067G3240   R407C   MOP +15C",null,null,null,null,"шт",null,null,0]
[0,765,"TES 20","   067B3352   R404 - 507      MOP +15C",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J863:J871)","v":0},"№","Модель","Клапанные узлы  Danfoss ",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B862+1","v":766},"TE 5 01  /  067B2789     ","  R404-507   -8 +40c 12,73квт  / -25 +40с 8,77квт / -40+40c 5,77квт    (+2 +50c 19,0квт  R407c)     ",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B864+1","v":767},"TE 5 03  /  067B2791     ","  R404-507    -8 +40с 22,46квт / -25 +40c 15,41квт / -40 +40c 10,1квт    (+2 +50c 33,32квт R407c)   ",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B865+1","v":768},"TE 12 05  /  067B2708     ","  R404-507    -8 +40с 40,74квт / -25 +40c 26,29квт / -40 +40c 16,7квт    (+2 +50c 49,35квт R407c)",null,null,null,null,"шт",null,null,0]
[0,769,"TE 12 06  /  067B2709    ","  R404-507    -8 +40с 50,81квт / -25 +40c 32,05квт / -40 +40c 19,85квт    (+2 +50c 65,2квт R407c)",null,null,null,null,"шт",null,null,0]
[0,770,"TE 55 10  /  067G2701  ","  R404-507    -8 +40с 98,91квт / -25 +40c 60,42квт / -40 +40c 35,56квт    (+2 +50c 142,6квт R407c)",null,null,null,null,"шт",null,null,0]
[0,771,"TE 55 11  /  067G2704  ","  R404-507    -8 +40с 107,1квт / -25 +40c 65,59квт / -40 +40c 38,66квт    (+2 +50c 154,0квт R407c)",null,null,null,null,"шт",null,null,0]
[0,772,"TE 55 12  /  067G2707  ","  R404-507    -8 +40с 115,6квт / -25 +40c 69,91квт / -40 +40c 40,97квт    (+2 +50c 165,2квт R407c)",null,null,null,null,"шт",null,null,0]
[0,773,"TE 55 13  /  067G2710  ","  R404-507    -8 +40с 138,8квт / -25 +40c 83,23квт / -40 +40c 48,27квт    (+2 +50c 197,2квт R407c)",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J872:J876)","v":0},"№","Модель","Корпуса клапана   Danfoss",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B871+1","v":774},"TE 5 ","   067B4012   16x22мм  угловой",null,null,null,1,"шт",null,null,0]
[0,775,"TE 12 ","   067B4017   22x28мм  угловой",null,null,null,null,"шт",null,null,0]
[0,776,"TE 20 ","   067B4023   22x28мм  угловой",null,null,null,null,"шт",null,null,0]
[0,777,"TE 55 ","   067G4004   28x35мм  угловой",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J877:J886)","v":0},"Терморегулирующие вентили",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A877","v":0},"№","Модель",null,"Параметры",null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[{"$f":"J879","v":0},{"$f":"B876+1","v":778},"ТРВ  TES2   R404  R507 ",null,"068Z3403","  -40 -10","MOP +15",1,"шт",null,null,0]
[0,{"$f":"B879+1","v":779},"Узел №0     ","R404a  N   -8 +40c  1,22kw   /   -25 +40c  0,91kw  (+2 +50c  1,81квт R407)",null,null,null,25,"шт",null,null,0]
[0,780,"Узел №1","R404a  N   -8 +40c  2,27kw   /   -25 +40c  1,45kw  (+2 +50с 3,5квт R407)  ",null,null,null,null,"шт",null,null,0]
[0,781,"Узел №2","R404a  N   -8 +40c  2,93kw   /   -25 +40c  1,7kw  (+2 +50с 4,63квт R407)  ",null,null,null,null,"шт",null,null,0]
[0,782,"Узел №3","R404a  N   -8 +40c  5,0kw   /   -25 +40c  2,87kw   (+2 +50с 7,95квт R407)  ",null,null,null,null,"шт",null,null,0]
[0,783,"Узел №4","R404a  N   -8 +40c  7,6kw   /   -25 +40c  4,22kw   (+2 +50с 12,0квт R407)",null,null,null,null,"шт",null,null,0]
[0,784,"Узел №5","R404a  N   -8 +40c  10,0kw   /   -25 +40c  5,54kw   (+2 +50с  16,0квт R407)  ",null,null,null,null,"шт",null,null,0]
[0,785,"Узел №6","R404a  N   -8 +40c  12,0kw   /   -25 +40c  6,55kw  (+2 +50с  19,2квт R407)  ",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J887:J900)","v":0},"Соленоидные клапаны CASTEL под пайку.    Комплект с катушкой (220 вольт)",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A887","v":0},"№","Модель",null,"Параметры",null,"м3/ч","Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B886+1","v":786},"С-1068/4A6       ",null,"1/2   12мм",null,"0.8",null,"шт",null,null,0]
[0,{"$f":"B889+1","v":787},"С-1078/5A6       ",null,"5/8   16мм",null," 2.61",null,"шт",null,null,{"$f":"J890*K890","v":0}]
[0,{"$f":"B890+1","v":788},"С-1079/7A6      ",null,"7/8   22мм",null," 2.61",null,"шт",null,null,0]
[0,789,"С-1099/9A6      ",null,"1 1/8    28мм",null," 5.7",null,"шт",null,null,0]
[0,790,"С-1079/M42       ",null,"1 5/8    42мм",null,16,null,"шт",null,null,0]
[0,791,"C-9300/RA6     ",null,"Катушка   220V  ",null,null,null,"шт",null,null,0]
[0,792,"SV1028/2",null,"  1/4    6мм",null,"0.15",null,"шт",null,null,0]
[0,793,"SV1078/5",null,"  5/8    16мм",null," 2.61",null,"шт",null,null,0]
[0,{"$f":"B896+1","v":794},"SV1079/7",null,"  7/8    22мм",null," 2.61",null,"шт",null,null,0]
[0,795,"SV1098/7",null,"  7/8    22мм",null," 5.7",null,"шт",null,null,0]
[0,796,"SV1099/9",null,"  1 1/8    28мм",null," 5.7",null,"шт",null,null,0]
[0,797,"BLR/QSV 208 b",null,"Катушка   208-230V  ",null,null,null,"шт",null,null,0]
[{"$f":"SUM(J901:J921)","v":0},"Соленоидные клапаны SANHUA   под пайку.  Без катушки (катушка приобретается отдельно)",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A901","v":0},"№","Модель",null,"артикул","Параметры","Кол-во в коробка","Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B900+1","v":798},"KDF3H01",null,10101001802,"   1/4    6мм",30,1,"шт",null,null,0]
[0,{"$f":"B903+1","v":799},"KDF3H03",null,10101002002,"   3/8    10мм",null,null,"шт",null,null,0]
[0,800,"KDF4H01",null,10101000202,"   3/8    10мм",null,null,"шт",null,null,0]
[0,801,"KDF6H01",null,10101000102,"   3/8    10мм",null,null,"шт",null,null,0]
[0,802,"KDF6H03",null,10101000902,"   1/2    12мм",null,null,"шт",null,null,0]
[0,803,"KDF10H01",null,10101000502,"   1/2    12мм",21,null,"шт",null,null,0]
[0,804,"KDF10H02",null,10101001302,"   5/8    16мм",null,null,"шт",null,null,0]
[0,805,"KDF15H01",null,10101000402,"   5/8    16мм",null,null,"шт",null,null,0]
[0,806,"KDF15H02",null,10101001502,"   7/8    22мм",null,null,"шт",null,null,0]
[0,807,"KDF15H03",null,10101001602,"   3/4    19мм",null,null,"шт",null,null,0]
[0,808,"HQ1G11     (KDF)",null,10780000402,"Катушка   220-240V  ",36,null,"шт",null,null,0]
[0,809,"MDF-A03-22H001",null,10125011802,"   7/8    22мм",10,1,"шт",null,null,0]
[0,810,"MDF-A03-22H009",null,10125006202,"   1-1/8    28мм",null,null,"шт",null,null,0]
[0,811,"MDF-B03-25H003",null,10125006902,"   1-1/8    28мм",4,null,"шт",null,null,0]
[0,812,"MDF-B03-25H004",null,10125006802,"   1-3/8    35мм",null,null,"шт",null,null,0]
[0,813,"MDF-B03-32H001",null,10125009102,"   1-3/8    35мм",null,null,"шт",null,null,0]
[0,814,"MDF-B03-40H002",null,10125004302,"   1-5/8    42мм",3,null,"шт",null,null,0]
[0,815,"MDF-B03-40H004",null,10125007702,"   2-1/8    54мм",null,null,"шт",null,null,0]
[0,816,"MQ-A0322G-000001     (MDF)",null,10820010002,"Катушка   220-240V  ",36,null,"шт",null,null,0]
[{"$f":"SUM(J922:J932)","v":0},"ALCO CONTROL",null,null,null,null,null,null,null,null,null,0]
[0,{"$f":"B921+1","v":817},"Игла  TIO-005  ",null,"Игла для ТРВ №5    ( R134a  -10c  8-9kw )        ( R407C +5c 15-18kw )",null,null,1,"шт",null,null,0]
[0,{"$f":"B923+1","v":818},"Игла  TIO-006   ",null,"Игла для ТРВ №6    ( R134a  -10c  10-11kw )        ( R407C +5c 19-20kw )",null,null,null,"шт",null,null,0]
[0,{"$f":"B924+1","v":819},"ТРВ  TISE-MW (12mm) R134   ",null,"пайка медь","  -45…+20","MOP",null,"шт",null,null,0]
[0,820,"X 22440-B3B     (Дюза для TCLE)",null,"R134 - 6.1квт","R22 - 7.9квт","R404 - 5.6квт",null,"шт",null,null,0]
[0,821,"X 22440-B3.5B     (Дюза для TCLE)",null,"R134 - 9.3квт","R22 - 11.9квт","R404 - 8.4квт",null,"шт",null,null,0]
[0,822,"X 22440-B4B     (Дюза для TCLE)",null,"R134 - 13.5квт","R22 - 17.3квт","R404 - 12.2квт",null,"шт",null,null,0]
[0,823,"X 22440-B5B     (Дюза для TCLE)",null,"R134 - 17.3квт","R22 - 22.2квт","R404 - 15.7квт",null,"шт",null,null,0]
[0,824,"ASC 24 v DC   ",null,"Катушка для Alco",null,null,null,"шт",null,null,0]
[0,825,"PRE-11A   ",null,"KVP  Pегулятор давления в испарителе 16мм",null,null,null,"шт",null,null,0]
[0,{"$f":"B931+1","v":826},"PRE-11B   ",null,"KVP  Pегулятор давления в испарителе 22мм",null,null,null,"шт",null,null,0]
[{"$f":"SUM(J933:J948)","v":0},"Реле Давления, прессостаты ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A933","v":0},"№","Модель",null,"артикул","Параметры",null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B932+1","v":827},"KP-1    060-110366     Danfoss",null,"Реле низкого давления 0.2-7.5 бар.,   (ручное) ",null,null,null,"шт",null,null,0]
[{"$f":"J936","v":0},{"$f":"B935+1","v":828},"KP-5    060-117366     Danfoss",null,"  Реле высокого давления 8-32 бар.,   (ручное) ",null,null,null,"шт",null,null,0]
[0,{"$f":"B936+1","v":829},"KVR 15    034L0097     Danfoss",null,"Клапан регулятор давления",null,null,null,"шт",null,null,0]
[0,830,"KVD 15    034L0177     Danfoss",null,"Клапан регулятор давления",null,null,null,"шт",null,null,0]
[0,831,"ICS 50    027H5023     Danfoss",null,"Клапан регулятор давления",null,null,null,"шт",null,null,0]
[0,832,"ICS 65    027H6025     Danfoss",null,"Клапан регулятор давления",null,null,null,"шт",null,null,0]
[0,833,"CVP-M    027B0921     Danfoss",null,"Пилотн клапан пост давлления",null,null,null,"шт",null,null,0]
[0,834,"SCA-X 50    148B5703     Danfoss",null,"Клапан обратный запорный",null,null,null,"шт",null,null,0]
[0,835,"SCA-X 65    148B5802     Danfoss",null,"Клапан обратный запорный",null,null,null,"шт",null,null,0]
[0,836,"MGP300","Реле высокого давления  5A  18 / 13 бар. (автомат        ",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B944+1","v":837},"MGP300","FAN-CONTROL      6A      13-18 бар                              ",null,null,null,null,"шт",null,null,0]
[0,838,"MGP506 с гайкой","     Реле низокого давления  8A 0.5-6 бар., (автомат)                                                          ",null,null,null,null,"шт",null,null,0]
[0,839,"MGP830HME с гайками","   Реле комбинированного давления  0.5…7  -  6…31 бар  8A   (L-H ручное)                ",null,null,null,null,"шт",null,null,{"$f":"J947*K947","v":0}]
[0,{"$f":"B947+1","v":840},"MGD35   (MP54) с гайками","Реле перепада давления  масла   8A",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J949:J962)","v":0},"Реле Давления, прессостаты  SANHUA",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A949","v":0},"№","Модель","низкое давлений бар","высокое давлений бар","Присоеди-  нение","Кол-во в коробка","Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B948+1","v":841},"PS01AL"," -0.5 - 7",null,"резьба",30,1,"шт",null,null,0]
[0,{"$f":"B951+1","v":842},"PS01ML",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B952+1","v":843},"PS01AH",null,null,"пайка",36,null,"шт",null,null,0]
[0,{"$f":"B953+1","v":844},"PS01MH",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B954+1","v":845},"PS50AL",null," 6 - 32","резьба",30,1,"шт",null,null,0]
[0,846,"PS50ML",null,null,null,null,null,"шт",null,null,0]
[0,847,"PS50AH",null,null,"пайка",36,null,"шт",null,null,0]
[0,848,"PS50MH",null,null,null,null,null,"шт",null,null,0]
[0,849,"PS15AAL"," -0.5 - 7"," 6 - 32","резьба",18,1,"шт",null,null,0]
[0,850,"PS15AML",null,null,null,null,null,"шт",null,null,0]
[0,851,"PS15AAH",null,null,"пайка",21,null,"шт",null,null,0]
[0,852,"PS15AMH",null,null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J963:J969)","v":0},"Манометры глицериновые ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A963","v":0},"№","Модель",null,null,null," 1/4  6мм","Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B962+1","v":853},"RW-FRG-250A-R низкого давления (выход штуцера снизу)   ",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B965+1","v":854},"RW-FRG-500A-R высокого давления (выход штуцер снизу)   ",null,null,null,null,null,"шт",null,null,0]
[0,855,"RW-FRG-250A-A низкого давления (выход штуцера сзади)   ",null,null,null,null,null,"шт",null,null,0]
[0,856,"RW-FRG-500A-A высокого давления (выход штуцер сзади)   ",null,null,null,null,null,"шт",null,null,0]
[0,857,"500B-GF высокого давления (выход штуцер снизу)  3 ",null,null,"для заправочного манометра",null,null,"шт",null,null,0]
[{"$f":"SUM(J970:J987)","v":0},"Капилярные шланги для пресостата  Cold-flex  (Турция)",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A970","v":0},"№","Код","Параметры",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B969+1","v":858},"403   (красный)","2мм * 5.6мм     Капиллярный шланг                    ",null,null,null,50,"м",null,null,0]
[0,{"$f":"B972+1","v":859},"404   (синий)",null,null,null,null,null,"м",null,null,0]
[0,{"$f":"B973+1","v":860},"405   (оранжевый)",null,null,null,null,null,"м",null,null,0]
[0,{"$f":"B974+1","v":861},101,"6мм  1/4\"   Прес гайка                                               ",null,null,null,50,"шт",null,null,0]
[0,{"$f":"B975+1","v":862},121,"6мм 1/4\"   90°С    Прес гайка                            ",null,null,null,null,"шт",null,null,0]
[0,863,141,"   Tройник                                                      ",null,null,null,25,"шт",null,null,0]
[0,864,501,"Пассатижи для капиллярного шланга",null,null,null,1,"шт",null,null,0]
[0,865,"RW-TPH02 ID 2.0mm  (черный)","2мм * 5.6мм     Капиллярный шланг                    ",null,null,null,100,"м",null,null,0]
[0,866,"RW-TPH02 ID 2.0mm  (красный)",null,null,null,null,null,"м",null,null,0]
[0,867,"RW-TPH02 ID 2.0mm  (синий)",null,null,null,null,null,"м",null,null,0]
[0,868,"RW-TPH-S02 (B)","6мм  1/4\" прямая  Прес гайка           ",null,null,null,50,"шт",null,null,0]
[0,869,"RW-TPH-E02 (B)","6мм 1/4\"   90°С    Прес гайка             ",null,null,null,null,"шт",null,null,0]
[0,870,"RW-TPH-T02 (B)","   Tройник            ",null,null,null,25,"шт",null,null,0]
[0,871,"CTN-100","Трубка капилярная для прессостата 1/4 - 100см       ",null,null,null,10,"шт",null,null,0]
[0,872,"CTN-150","Трубка капилярная для прессостата 1/4 - 150см       ",null,null,null,10,"шт",null,null,0]
[0,873," HT-04A                     ","  Золотник с трубкой    0.7мм -1/4\" длина 60мм            ",null,null,null,50,"шт",null,null,0]
[{"$f":"SUM(J988:J1000)","v":0},"Вибропоглотители  ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A988","v":0},"№","Наименование","Размер ф мм",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B987+1","v":874},"COLDTHERM-67","67 мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B990+1","v":875},"BLR/VA-012m  1/2   D2","12 мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B991+1","v":876},"BLR/VA-058m  5/8   D3","16 мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B992+1","v":877},"BLR/VA-034m  3/4   D4","19 мм",null,null,null,null,"шт",null,null,0]
[{"$f":"J994","v":0},878,"BLR/VA-078m  7/8   D5","22 мм",null,null,null,null,"шт",null,null,0]
[0,879,"BLR/VA-118m  1-1/8   D6","  28 мм",null,null,null,null,"шт",null,null,0]
[0,880,"BLR/VA-138m  1-3/8   D7","35 мм",null,null,null,null,"шт",null,null,0]
[0,881,"BLR/VA-158m  1-5/8   D8","42 мм",null,null,null,null,"шт",null,null,0]
[0,882,"BLR/VA-218m  2-1/8   D9","54 мм",null,null,null,null,"шт",null,null,0]
[0,883,"BLR/VA-258m  2-5/8   D10","67 мм",null,null,null,null,"шт",null,null,0]
[0,884,"BLR/VA-318m  3-1/8   D11","80 мм",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1001:J1020)","v":0},"Обратные клапана ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1001","v":0},"№","Модель ","Диаметр мм",null,"м3/ч",null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1000+1","v":885},"33000-TS-04-D   OLAB","5/8   16мм  ",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1003+1","v":886},"33100-TS-10-D   OLAB","1 5/8   42мм  ",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1004+1","v":887},"33100-TS-12-D   OLAB","2 1/8   54мм  ",null,null,null,null,"шт",null,null,0]
[0,888,"C-3122/M42    CASTEL","1 5/8   42мм  ",null,null,null,null,"шт",null,null,0]
[0,889,"BLR/MCV-6"," 3/8   10мм",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1007+1","v":890},"BLR/MCV-10","    5/8   16мм",null,null,null,null,"шт",null,null,{"$f":"J1008*K1008","v":0}]
[0,{"$f":"B1008+1","v":891},"BLR/NRV-10S","3/8   10мм  ",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1009+1","v":892},"BLR-3142/7","7/8   22мм   ",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1010+1","v":893},"BLR-3142/13","1 5/8   42мм   ",null,null,null,null,"шт",null,null,0]
[0,894,"YCVSH8   33GSHC-1","3/8   10мм   ",null," 1.6","прямой",1,"шт",null,null,0]
[0,895,"YCVSH10   33GSHC-1","1/2   12мм   ",null," 2.64",null,null,"шт",null,null,0]
[0,896,"YCVSH13   55GSHC-1","5/8   16мм   ",null,"  4.0",null,null,"шт",null,null,0]
[0,897,"YCVSH17   66GSHC-1","3/4   19мм   ",null," 6.8",null,null,"шт",null,null,0]
[0,898,"YCVSH17   77GSHC-1","7/8   22мм   ",null," 6.8",null,null,"шт",null,null,0]
[0,899,"YCVSH20   77GSHC-1","7/8   22мм   ",null," 13.09","угловвой",1,"шт",null,null,0]
[0,900,"YCVSH26   88GSHC-1","1-1/8   28мм   ",null," 18.86",null,null,"шт",null,null,0]
[0,901,"YCVSH31   BBGSHC-1","1-3/8   35мм   ",null," 28.86",null,null,"шт",null,null,0]
[0,902,"YCVSH31   DDGSHC-2","1-5/8   42мм   ",null," 28.86",null,null,"шт",null,null,0]
[{"$f":"SUM(J1021:J1060)","v":0},"Маслоотделители GVN ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1021","v":0},"№","Модель","Диаметр мм",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1020+1","v":903},"OS.33b.22.1","22 мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1023+1","v":904},"OS.33b.28.1","28 мм  ",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1024+1","v":905},"OS.33b.35.1","35 мм  ",null,null,null,null,"шт",null,null,0]
[0,906,"OS.33b.42.2","42 мм  ",null,null,null,null,"шт",null,null,0]
[0,907,"OS.33b.54.2","54 мм  ",null,null,null,null,"шт",null,null,0]
[0,908,"OS.HF.33b.80.1","80 мм  ",null,null,null,null,"шт",null,null,0]
[0,909,"BLR/A-W 55855","5/8  16 мм   BLUE ",null,null,null,1,"шт",null,null,0]
[0,910,"BLR/A-W 55877","7/8  22 мм   BLUE  ",null,null,null,null,"шт",null,null,0]
[0,911,"BLR/A-W 55889","1 1/8  28 мм   BLUE  ",null,null,null,null,"шт",null,null,0]
[0,912,"BLR/A-W 569011","1 3/8  35 мм   BLUE  ",null,null,null,null,"шт",null,null,0]
[0,913,"BLR/A-W 569213","1 5/8  42 мм   BLUE  ",null,null,null,null,"шт",null,null,0]
[0,914,"BLR/A-F 579417","2 1/8  54 мм   BLUE  ",null,null,null,null,"шт",null,null,0]
[0,915,"BLR/OSR-3258","2 5/8  66 мм ODS   BLUE  ",null,null,null,null,"шт",null,null,0]
[0,916,"BLR/OSR-3318","3 1/8  80 мм ODS   BLUE  ",null,null,null,null,"шт",null,null,0]
[0,917,"BLR/VOR-04038","Маслянный рессивер  3/8   4 LT ",null,null,null,null,"шт",null,null,0]
[0,918,"BLR/VOR-06038","Маслянный рессивер  3/8   6 LT ",null,null,null,null,"шт",null,null,0]
[0,919,"BLR/VOR-10038","Маслянный рессивер  3/8   10 LT ",null,null,null,null,"шт",null,null,0]
[0,920,"BLR/VOR-18012","Маслянный рессивер  1/2   18 LT ",null,null,null,null,"шт",null,null,0]
[0,921,"BLR/ODCV-20   3/8 SAE","Обратный клапан маслянной линии 1.5 бар",null,null,null,null,"шт",null,null,0]
[0,922,"OS.D.33B.180S.C6.1HTI.G3","Маслоотделитель для винтового компрессора 54 мм 40L ",null,null,null,1,"шт",null,null,0]
[0,923,"OS.D.33b.400.E1.E1.C8.G5 12","Маслоотделитель для винтового компрессора 54 мм 50L ",null,null,null,null,"шт",null,null,0]
[0,924,"OR.33b.10","Маслянный рессивер     10 LT ",null,null,null,1,"шт",null,null,0]
[0,925,"OR.33b.18","Маслянный рессивер     18 LT ",null,null,null,null,"шт",null,null,0]
[0,926,"OR.33b.21","Маслянный рессивер     21 LT ",null,null,null,null,"шт",null,null,0]
[0,927,"33002-FM-02-D-2   СV-3/8","Обратный клапан маслянной линии 1.5 бар",null,null,null,null,"шт",null,null,0]
[0,928,"BLR/OFD-083","3/8   Маслянный фильтр",null,null,null,null,"шт",null,null,0]
[0,929,"COM1-230/000","Электронный регулятор уровня масла DEKA   ",null,null,null,null,"шт",null,null,0]
[{"$f":"J1050","v":0},930,"Адаптер  CE","Присоеденительный адаптер для Электронного регулятора уровня масла   INVOTECH",null,null,null,null,"шт",null,null,0]
[0,931,"412  Маслянный шланг   5мм * 8мм (Cold-flex)  (оранжевый)                                УПК 25 мт",null,null,null,null,25,"м",null,null,0]
[0,932,"282  10мм  TEE под запрессовку для масляного шланга (Cold-flex)  в коробке     УПК 25 шт",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1052+1","v":933},"242  10мм 3/8 Пресс гайка под запрессовку для масляного шланга (Cold-flex)      УПК 25 шт",null,null,null,null,null,"шт",null,null,0]
[0,934,"262  90С  10мм 3/8 Пресс гайка под запрессовку для масляного шланга (Cold-flex)   УПК 25 шт",null,null,null,null,null,"шт",null,null,0]
[0,935,"202  6мм 1/4 Пресс гайка под запрессовку   для масляного шланга (Cold-flex)       УПК 25 шт",null,null,null,null,null,"шт",null,null,0]
[0,936,"222  90С 6мм 1/4 Пресс гайка под запрессовку для масляного шланга (Cold-flex)       УПК 25 шт",null,null,null,null,null,"шт",null,null,0]
[0,937,"RW-TPH04 ID 4.0mm  Маслянный шланг  (черный)          УПК 25 мт",null,null,null,null,25,"м",null,null,0]
[0,938,"RW-TPH-S04 (B) прямая  6мм 1/4 Пресс гайка под запрессовку   для масляного шланга        УПК 25 шт",null,null,null,null,null,"шт",null,null,0]
[0,939,"RW-TPH-E04  (B)  90С 6мм 1/4 Пресс гайка под запрессовку для масляного шланга       УПК 25 шт",null,null,null,null,null,"шт",null,null,0]
[0,940,"TPC-CY (DN4) Пассатиж для масляного шланга     ",null,null,null,null,1,"шт",null,null,0]
[{"$f":"SUM(J1061:J1080)","v":0},"Отделители  жидкости ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1061","v":0},"№","Модель","Диаметр мм",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1060+1","v":941},"Коллектор для Централь","SLAE CLTR.HL.33b.90.2xB17.B21.H30Y2               3 компрессор          54*67*54*67*54=273мм",null,null,null,null,"шт",null,null,{"$f":"J1063*K1063","v":0}]
[0,{"$f":"B1063+1","v":942},null,"SLAE CLTR.HL.33b.90.5xB14.Y1.Y2.H30               3 компрессор          80*80*80*80*80=273мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1064+1","v":943},"SLA.A.33B.80.32.F4     GVN   ","3 1/8      80 мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1065+1","v":944},"BLR/SLA-205","  16мм",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1066+1","v":945},"BLR/SLA-206","   19мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1067+1","v":946},"BLR/SLA-207","   22мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1068+1","v":947},"BLR/SLA-211","   28мм",null,null,null,null,"шт",null,null,0]
[0,948,"BLR/SLA-213","   35мм",null,null,null,null,"шт",null,null,0]
[0,949,"BLR/SLA-215","   42мм",null,null,null,null,"шт",null,null,0]
[0,950,"BLR/HSA-2404","   Cо встроенным теплообменником  12 х 10мм",null,null,null,1,"шт",null,null,0]
[0,951,"BLR/HSA-2405","   Cо встроенным теплообменником  16 х 10мм",null,null,null,null,"шт",null,null,0]
[0,952,"BLR/HSA-2406","Cо встроенным теплообменником  19 х 12мм",null,null,null,null,"шт",null,null,0]
[0,953,"BLR/HSA-2407","   Cо встроенным теплообменником  22 х 12мм",null,null,null,null,"шт",null,null,0]
[0,954,"BLR/HSA-2411","   Cо встроенным теплообменником  28 х 16мм",null,null,null,null,"шт",null,null,0]
[0,955,"BLR/HSA-2413","Cо встроенным теплообменником  35 х 19мм",null,null,null,null,"шт",null,null,0]
[0,956,"BLR/HSA-2415","Cо встроенным теплообменником  42 х 22мм",null,null,null,null,"шт",null,null,0]
[0,957,"BLR/HSA-2417","Cо встроенным теплообменником  54 х 28мм",null,null,null,null,"шт",null,null,0]
[0,958,"BLR/HSA-2421","Cо встроенным теплообменником  66 х 28мм",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1081:J1103)","v":0},"Ресиверы ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1081","v":0},"№","Модель ","Диаметр мм",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1080+1","v":959},"VLR.A.33b.21.B6.C6.F4","21-лт   22мм   GVN",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1083+1","v":960},"V7A.33b.25.B6.C6.F4","25-лт   22мм   GVN",null,"   BLR/RV-7/8   (1 1/4)   22мм",null,null,"шт",null,null,0]
[0,{"$f":"B1084+1","v":961},"V8A.33b.30.B7.C7.F4","30-лт   28мм   GVN",null,"   BLR/RV-1 1/8   (1 3/4)   28мм",null,null,"шт",null,null,0]
[0,962,"V9A.33b.40.B7.C7.F4","40-лт   28мм   GVN",null,"   BLR/RV-1 1/8   (1 3/4)   28мм",null,null,"шт",null,null,0]
[0,963,"V9A.33b.50.B7.C7.F4","50-лт   28мм   GVN",null,null,null,null,"шт",null,null,0]
[0,964,"V9A.33b.60.B7.C7.F4","60-лт   28мм   GVN",null,null,null,null,"шт",null,null,0]
[0,965,"V9A.33b.80.B8.C8.F4","80-лт   35мм   GVN",null," 35мм 2-шт",null,null,"шт",null,null,0]
[0,966,"V10A.33b.100.B9.C9.F4","100-лт   42мм   GVN",null,null,null,null,"шт",null,null,0]
[0,967,"V10A.33b.150.B9.C9.F4.H4","150-лт   42мм   GVN",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1091+1","v":968},"40095-K4N4-0-280   OLAB","1/2 NPT 5/8 SAE   Предохранительный клапан для рессивера  30 бар",null,null,null,null,"шт",null,null,0]
[0,969,"BLR/VLR-01","  1-лт     6мм",null,null,null,1,"шт",null,null,0]
[0,970,"BLR/VLR-02","  2-лт     10мм",null,null,null,null,"шт",null,null,0]
[0,971,"BLR/VLR-03","  3-лт     10мм",null,null,null,null,"шт",null,null,0]
[0,972,"BLR/VLR-04"," 4-лт   10мм",null,null,null,null,"шт",null,null,0]
[0,973,"BLR/VLR-05"," 5-лт   10мм",null,null,null,null,"шт",null,null,0]
[0,974,"BLR/VLR-06"," 6-лт    12мм",null,null,null,null,"шт",null,null,0]
[0,975,"BLR/VLR-09"," 9-лт    12мм",null,null,null,null,"шт",null,null,0]
[0,976,"BLR/VLR-10","  10-лт    16мм",null,null,null,null,"шт",null,null,0]
[0,977,"BLR/VLR-14","  14-лт    16мм",null,null,null,null,"шт",null,null,0]
[0,978,"BLR/VLR-18","  18-лт    16мм",null,null,null,null,"шт",null,null,0]
[0,979,"BLR/VLR-21","  21-лт    22мм",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1104:J1111)","v":0},"Фильтры-осушители  DENA",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1104","v":0},"№","Модель","Диаметр трубы",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1103+1","v":980},"13.5 гр","      6.5-2.5мм      ",null,null,null,500,"шт",null,null,0]
[0,{"$f":"B1106+1","v":981},"15 гр","      6.5-2.5мм      ",null,null,null,null,"шт",null,null,0]
[0,982,"20 гр","      6.5-2.5мм      ",null,null,null,350,"шт",null,null,0]
[0,983,"30 гр","      6.5-2.5мм      ",null,null,null,250,"шт",null,null,0]
[0,{"$f":"B1109+1","v":984},"40 гр","        6.5-6.5мм  ",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1110+1","v":985},"50 гр","         6.5-6.5мм  ",null,null,null,200,"шт",null,null,0]
[{"$f":"SUM(J1112:J1151)","v":0},"Фильтры-осушители  BLUE",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1112","v":0},"№","Модель",null,"Диаметр трубы",null,"Объем см3","Кол-во в упаковке","Ед.изм.",null,null,0]
[{"$f":"J1114","v":0},{"$f":"B1111+1","v":986},"BLR/EK-052  резьба",null,"6 мм 1/4\"",null,80,25,"шт",null,null,0]
[0,{"$f":"B1114+1","v":987},"BLR/EK-053  резьба",null,"10 мм 3/8\"",null,80,null,"шт",null,null,0]
[0,{"$f":"B1115+1","v":988},"BLR/EK-083  резьба",null,"10 мм 3/8\"",null,130,null,"шт",null,null,0]
[0,{"$f":"B1116+1","v":989},"BLR/EK-163  резьба",null,"10 мм 3/8\"",null,250,null,"шт",null,null,0]
[0,990,"BLR/EK-164  резьба",null,"12 мм 1/2\"",null,250,null,"шт",null,null,0]
[0,991,"BLR/EK-165  резьба",null,"16 мм 5/8\"",null,250,null,"шт",null,null,0]
[0,992,"BLR/EK-304  резьба",null,"12 мм 1/2\"",null,500,12,"шт",null,null,0]
[0,993,"BLR/EK-305  резьба",null,"16 мм 5/8\"",null,500,9,"шт",null,null,0]
[0,994,"BLR/EK-052s  пайка",null,"6 мм 1/4\"",null,80,25,"шт",null,null,0]
[0,995,"BLR/EK-083s  пайка",null,"10 мм 3/8\"",null,130,null,"шт",null,null,0]
[0,996,"BLR/EK-163s  пайка",null,"10 мм 3/8\"",null,250,null,"шт",null,null,0]
[0,997,"BLR/EK-164s  пайка",null,"12 мм 1/2\"",null,250,null,"шт",null,null,0]
[0,998,"BLR/EK-165s  пайка",null,"16 мм 5/8\"",null,250,null,"шт",null,null,{"$f":"J1126*K1126","v":0}]
[0,{"$f":"B1126+1","v":999},"BLR/EK-304s  пайка",null,"12 мм 1/2\"",null,500,12,"шт",null,null,0]
[0,1000,"BLR/EK-305s  пайка",null,"16 мм 5/8\"",null,500,9,"шт",null,null,0]
[0,1001,"BLR/EK-307s   пайка",null,"22 мм 7/8\"",null,670,null,"шт",null,null,0]
[0,1002,"BLR/EK-309s   пайка",null,"28 мм 1 1/8\"",null,670,null,"шт",null,null,0]
[0,1003,"BLR/SSR-287T   пайка      (всас)",null,"22 мм 7/8\"",null,670,null,"шт",null,null,0]
[0,1004,"BLR/SSR-289T   пайка      (всас)",null,"28 мм 1 1/8\"",null,670,null,"шт",null,null,0]
[0,1005,"BLR/STAS-485T     ",null,"5/8     16 мм",null,"Н-48  ",null,"шт",null,null,0]
[0,1006,"BLR/STAS-487T",null,"7/8   22 мм",null,null,null,"шт",null,null,0]
[0,1007,"BLR/STAS-489T",null,"1 1/8     28 мм",null,null,null,"шт",null,null,0]
[0,1008,"BLR/STAS-4811T",null,"1 3/8     35 мм",null,null,null,"шт",null,null,0]
[0,1009,"BLR/STAS-4813T",null,"1 5/8     42 мм",null,null,null,"шт",null,null,0]
[0,1010,"BLR/STAS-4817T",null,"2 1/8     54 мм",null,null,null,"шт",null,null,0]
[0,1011,"BLR/STAS-4821T",null,"2 5/8     67 мм",null,null,null,"шт",null,null,0]
[0,1012,"BLR/STAS-4825ST",null,"3 1/8     80 мм",null,null,null,"шт",null,null,0]
[0,1013,"BLR/STAS-967T",null,"7/8     22 мм",null,"Н-48  2шт",null,"шт",null,null,0]
[0,1014,"BLR/STAS-969T",null,"1 1/8     28 мм",null,null,null,"шт",null,null,0]
[0,1015,"BLR/STAS-9611T",null,"1 3/8     35 мм",null,null,null,"шт",null,null,0]
[0,1016,"BLR/STAS-9613T",null,"1 5/8     42 мм",null,null,null,"шт",null,null,0]
[0,1017,"BLR/STAS-14413T",null,"1 5/8     42 мм",null,"Н-48  3шт",null,"шт",null,null,0]
[0,1018,"BLR/STAS-14417T",null,"2 1/8     54 мм",null,null,null,"шт",null,null,0]
[0,1019,"BLR/ADKS-10021",null,"2-5/8     67 мм",null,"Н-100  1шт",null,"шт",null,null,0]
[0,1020,"BLR/ADKS-10025",null,"3-1/8     80 мм",null,null,null,"шт",null,null,0]
[0,1021,"                      Картридж фильтра линии всасывания     бумага            ",null,null,null,"F-100",6,"шт",null,null,0]
[0,1022,"                      Картридж фильтра линии всасывания     бумага             ",null,null,null,"F-48",12,"шт",null,null,0]
[0,1023,"                      Сердечник для фильтра                 камень         ",null,null,null,"BLR/H-48",null,"шт",null,null,0]
[{"$f":"SUM(J1152:J1160)","v":0},"Разборные фильтры  GVN ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1152","v":0},"№","Модель",null,"Диаметр трубы",null,"Объем ","Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1151+1","v":1024},"H48.33b.28.1",null,"28 мм",null,null,null,"шт",null,null,0]
[0,{"$f":"B1154+1","v":1025},"H48.33b.66.1         ",null,"66 мм",null,null,null,"шт",null,null,0]
[0,{"$f":"B1155+1","v":1026},"H48.33b.35.2",null,"35 мм",null,null,null,"шт",null,null,0]
[0,1027,"H48.33b.42.2",null,"42 мм",null,null,null,"шт",null,null,0]
[0,1028,"                      Сердечник для фильтра  DENA  камень          УПК 12 шт",null,null,null,"CD - H 48   ",12,"шт",null,null,0]
[0,{"$f":"B1158+1","v":1029},"                   Сердечник для фильтра  DENA антикислотный  камень   УПК 12 шт",null,null,null,"CD - H 48 А ",null,"шт",null,null,0]
[0,{"$f":"B1159+1","v":1030},"                      Картридж фильтра линии всасывания  CASTEL   бумага  H100",null,null,null,"C-4496/C",1,"шт",null,null,0]
[{"$f":"SUM(J1161:J1171)","v":0},"Индикаторы  влажности  под пайку  ODF  ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1161","v":0},"№","Размер ","Диаметр трубы","артикул",null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1160+1","v":1031},"SYJ19H11"," 3/4 - 19мм",10285007602,null,null,null,"шт",null,null,0]
[0,{"$f":"B1163+1","v":1032},"SYJ22H11"," 7/8 - 22мм",10285007702,null,null,null,"шт",null,null,0]
[null,1033,"BLR/SG-014S   "," 1/4 - 6мм",null,null,null,null,"шт.",null,null,0]
[0,1034,"BLR/SG-038S   "," 3/8 - 10мм",null,null,null,null,"шт",null,null,0]
[0,1035,"BLR/SG-012S    "," 1/2 - 12мм",null,null,null,null,"шт",null,null,0]
[{"$f":"J1168","v":0},1036,"BLR/SG-058S    "," 5/8 - 16мм",null,null,null,null,"шт",null,null,0]
[0,1037,"BLR/SG-078S   "," 7/8 - 22мм",null,null,null,null,"шт",null,null,0]
[0,1038,"BLR/SGN-G3/4",null,null,null,null,null,"шт",null,null,0]
[0,1039,"BLR/SR-05","адаптер для BLR/SGN-G3/4",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1172:J1177)","v":0},null,"Модель",null,"артикул","Вентили шаровые CASTEL",null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1171+1","v":1040}," С-6570/5    5/8    ","16мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1173+1","v":1041}," С-6570/7    7/8   ","22мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1174+1","v":1042}," С-6570/9    1 1/8    ","28мм",null,null,null,null,"шт",null,null,0]
[0,1043," С-6590/M42    1 5/8    ","42мм",null,null,null,null,"шт",null,null,0]
[0,1044," С-6570/17    2 1/8   ","54мм",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1178:J1197)","v":0},null,"Модель",null,"артикул","Вентили шаровые ",null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1177+1","v":1045},"HT-08  1/2","12мм",null,"Кран под резьбу с гайкой  ",null,1,"шт",null,null,0]
[0,{"$f":"B1179+1","v":1046},"BLR/GBC-16    ","16мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1180+1","v":1047},"BLR/GBC-22   ","22мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1181+1","v":1048},"BLR/GBC-28   ","28мм",null,null,null,null,"шт",null,null,{"$f":"J1182*K1182","v":0}]
[0,1049,"BLR/GBC-35   ","35мм",null,null,null,null,"шт",null,null,0]
[0,1050,"BLR/GBC-42   ","42мм",null,null,null,null,"шт",null,null,0]
[0,1051,"BLR/GBC-54  ","54мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1185+1","v":1052},"BLR/GBC-67","67мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1186+1","v":1053},"BLR/GBC-79    BV-016","80мм",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1187+1","v":1054},"SBV6  02-019 ","6мм",10150091902,null,null,null,"шт",null,null,0]
[0,1055,"SBV10  03-020 ","10мм",10150092102,null,null,null,"шт",null,null,0]
[0,1056,"SBV12  04-020 ","12мм",10150092202,null,null,null,"шт",null,null,0]
[0,1057,"SBV16   JA5YSY","16мм",10150053402,"с клапаном шредера",null,null,"шт",null,null,0]
[0,1058,"SBV19   JA6YSY","19мм",10150054202,null,null,null,"шт",null,null,0]
[0,1059,"SBV22   JA7YSY","22мм",10150053602,null,null,null,"шт",null,null,0]
[0,1060,"SBV28   JA9YSY","28мм",10150055202,null,null,null,"шт",null,null,0]
[0,1061,"SBV35   JA11YSY","35мм",10150054902,null,null,null,"шт",null,null,0]
[0,1062,"SBV42   JA13YSY ","42мм",10150057802,null,null,null,"шт",null,null,0]
[0,1063,"SBV54   JA17YSY ","54мм",10150055802,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1198:J1206)","v":0},"Гайки    ",null,null,null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1197+1","v":1064},"31007-01","Штуцер компрессора резьбовой  1/4-1/4 (6х10мм) OLAB Италия   ",null,null,null,25,"шт",null,null,0]
[0,{"$f":"B1199+1","v":1065},"31008-01   ","Штуцер компрессора резьбовой  1/4-1/8 (6х6мм)  OLAB Италия  ",null,null,null,null,"шт",null,null,0]
[0,1066,"MC-04x02","Штуцер компрессора резьбовой  1/4-1/8  ",null,null,null,null,"шт",null,null,0]
[0,1067,"MC-04x04","Штуцер компрессора резьбовой  1/4-1/4  ",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1202+1","v":1068},"BLR/RA-1/4      "," 6-мм        ","  BLUE            ",null,null,400,"шт",null,null,0]
[0,1069,"BLR/RA-3/8    "," 10-мм        ",null,null,null,160,"шт",null,null,0]
[0,1070,"BLR/RA-1/2"," 12-мм        ",null,null,null,120,"шт",null,null,0]
[0,1071,"BLR/RA-5/8"," 16-мм        ",null,null,null,80,"шт",null,null,0]
[{"$f":"SUM(J1207:J1214)","v":0},"Электроды   (припой)",null,null,null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1206+1","v":1072},"Медно-фосфорный 6% FORTEBRAZE   1 кг     1.2x3.5x500mm   ",null,null,null,null,null,"кг",null,null,0]
[0,{"$f":"B1208+1","v":1073},"припой HP-02  0%        1.2x3.5x500mm    Упаковка 0.454-кг 30 шт  ",null,null,null,null,null,"уп",null,null,0]
[0,1074,"припой CP302  BLOCKADE    Упаковка 0.454-кг 28 шт   ",null,null,null,null,null,"уп",null,null,0]
[0,1075," Серебро15 %  2х500мм  SENTESBIR  (без флюса)    (1 кг-76шт)  1-шт= 3,5 usd   ",null,null,null,null,null,"кг",null,null,0]
[0,1076," Серебро30 %  2х500мм  SENTESBIR  (без флюса)    (1 кг-76шт)  1-шт= 6,7 usd   ",null,null,null,null,null,"кг",null,null,0]
[0,1077," Серебро30 %  2х500мм  SENTESBIR  (с флюсом)    (1 кг-71шт)  1-шт= 7,3 usd   ",null,null,null,null,null,"кг",null,null,0]
[0,1078," FORTEBRAZE   флюс    (100-гр)                                                                               ",null,null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1215:J1270)","v":0},"Медные трубы",null,null,null,null,null,null,null,null,null,0]
[{"$f":"SUM(J1216:J1246)","v":0},"№","Размер (Ф мм).","В рулоне","В рулоне",null,null,"Кол-во в упаковке","Ед.изм",null,null,0]
[null,null,null,"метр","кг",null,null,null,null,null,null,0]
[0,{"$f":"B1214+1","v":1079},"6,35*0,51*15000mm  1/4\" ",15,1.2509999999999999,null,null,10,"рул",null,null,0]
[0,{"$f":"B1218+1","v":1080},"6,35*0,51*50000mm  1/4\" ",50,4.17,null,null,5,"рул",null,null,0]
[0,{"$f":"B1219+1","v":1081},"6,35*0,60*15000mm  1/4\" ",15,1.45,null,null,10,"рул",null,null,0]
[0,{"$f":"B1220+1","v":1082},"6,35*0,60*50000mm  1/4\" ",50,4.8,"ЦЕНЫ НА РУЛОННУЮ ТРУБУ УТОЧНЯЙТЕ У МЕНЕДЖЕРОВ",null,5,"рул",null,null,0]
[0,1083,"6,35*0,71*15000mm  1/4\" ",15,1.65,null,null,10,"рул",null,null,0]
[0,1084,"6,35*0,71*50000mm  1/4\" ",50,5.59,null,null,5,"рул",null,null,0]
[0,1085,"7,94*0,65*15000mm  5/16\" ",15,1.99,null,null,12,"рул",null,null,0]
[0,1086,"9,52*0,50*15000mm  3/8\" ",15,1.8939999999999999,null,null,10,"рул",null,null,0]
[0,1087,"9,52*0,50*50000mm  3/8\" ",50,6.3140000000000001,null,null,3,"рул",null,null,0]
[0,1088,"9,52*0,60*15000mm  3/8\" ",15,2.2250000000000001,null,null,10,"рул",null,null,0]
[0,1089,"9,52*0,60*50000mm  3/8\" ",50,7.42,null,null,3,"рул",null,null,0]
[0,1090,"9,52*0,70*15000mm  3/8\" ",15,2.54,null,null,10,"рул",null,null,0]
[{"$f":"J1230","v":0},1091,"9,52*0,70*50000mm  3/8\" ",50,8.64,null,null,3,"рул",null,null,0]
[0,1092,"9,52*0,80*50000mm  3/8\" ",50,9.65,null,null,3,"рул",null,null,0]
[0,1093,"12,7*0,60*15000mm  1/2\" ",15,3.05,null,null,5,"рул",null,null,0]
[0,1094,"12,7*0,60*50000mm  1/2\" ",50,10.164,null,null,5,"рул",null,null,0]
[0,1095,"12,7*0,70*15000mm  1/2\" ",15,3.5150000000000001,null,null,5,"рул",null,null,0]
[0,1096,"12,7*0,70*50000mm  1/2\" ",50,11.76,null,null,3,"рул",null,null,0]
[0,1097,"12,7*0,90*50000mm  1/2\" ",50,14.868,null,null,3,"рул",null,null,0]
[0,1098,"15,88*0,64*15000mm  5/8\" ",15,4.0940000000000003,null,null,5,"рул",null,null,0]
[0,1099,"15,88*0,70*15000mm  5/8\" ",15,4.3899999999999997,null,null,4,"рул",null,null,0]
[0,1100,"15,88*0,70*50000mm  5/8\" ",50,14.63,null,null,2,"рул",null,null,0]
[0,1101,"15,88*1,00*50000mm  5/8\" ",50,20.75,null,null,2,"рул",null,null,0]
[0,1102,"19,05*0,68*15000mm  3/4\" ",15,5.25,null,null,3,"рул",null,null,0]
[0,1103,"19,05*0,71*15000mm  3/4\" ",15,5.4690000000000003,null,null,3,"рул",null,null,0]
[0,1104,"19,05*0,70*50000mm  3/4\" ",50,17.760000000000002,null,null,2,"рул",null,null,0]
[0,1105,"19,05*1,00*50000mm  3/4\" ",50,25.2,null,null,2,"рул",null,null,0]
[0,{"$f":"B1244+1","v":1106},"2,2*1,00mm ","30-м",null,"Капиллярные трубы",null,null,"рул",null,null,0]
[0,1107,"2,4*1,20mm ",null,null,null,null,null,"рул",null,null,0]
[{"$f":"SUM(J1247:J1270)","v":0},"№","Размер (Ф мм).","ШТ","кг - шт",null,null,"Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1246+1","v":1108},"8*0,80*5000mm ","5-м",0.81299999999999994,null,null,20,"шт  ",null,null,0]
[0,{"$f":"B1248+1","v":1109},"10*0,70*5000mm ",null,0,null,null,null,"шт  ",null,null,0]
[0,1110,"10*0,80*5000mm ",null,0.96,null,null,null,"шт",null,null,{"$f":"J1250*K1250","v":0}]
[0,1111,"10*1,00*5000mm ",null,1.24,"ЦЕНЫ НА ПРЯМУЮ  ТРУБУ УТОЧНЯЙТЕ У МЕНЕДЖЕРОВ",null,null,"шт",null,null,0]
[0,1112,"12.7*0,60*5000mm ",null,1.01,null,null,null,"шт",null,null,0]
[0,1113,"12*0,97*5000mm ",null,1.49,null,null,null,"шт",null,null,0]
[0,1114,"15*0,80*5000mm ",null,1.56,null,null,null,"шт",null,null,0]
[0,1115,"16*1,00*5000mm ",null,2.09,null,null,null,"шт",null,null,0]
[0,1116,"18*0,75*5000mm ",null,1.8,null,null,null,"шт",null,null,0]
[0,1117,"19*0,89*5000mm ",null,2.2200000000000002,null,null,null,"шт",null,null,0]
[0,1118,"22*0,80*5000mm ",null,2.36,null,null,10,"шт",null,null,0]
[0,1119,"22*1,00*5000mm ",null,2.89,null,null,null,"шт",null,null,0]
[0,1120,"25*1,00*5000mm ",null,3.36,null,null,null,"шт",null,null,0]
[0,1121,"28*0,90*5000mm ",null,3.33,null,null,null,"шт",null,null,0]
[0,1122,"28*1,00*5000mm ",null,3.78,null,null,null,"шт",null,null,0]
[0,1123,"35-мм х 1,0 мм",null,4.75,null,null,5,"шт",null,null,0]
[0,1124,"42-мм х 1.0 мм",null,5.65,null,null,3,"шт",null,null,0]
[0,1125,"54-мм х 1 мм",null,7.32,null,null,2,"шт",null,null,0]
[0,1126,"54-мм х 1,5 мм",null,10.75,null,null,null,"шт",null,null,0]
[0,1127,"66.67-mm x 1.6 mm",null,14.4,null,null,1,"шт",null,null,0]
[0,1128,"66.67-mm x 2.0 mm",null,17.8,null,null,null,"шт",null,null,0]
[0,1129,"79.3-mm x 2.0 mm",null,21.16,null,null,null,"шт",null,null,0]
[0,1130,"104.78-mm x 2.5 mm",null,35.799999999999997,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1271:J1283)","v":0},null,"Размер ","Крепление для медных труб ",null,null,null,"Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1270+1","v":1131},"Ф 10 мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1272+1","v":1132},"Ф 12 мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1273+1","v":1133},"Ф 16 мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1274+1","v":1134},"Ф 19 мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1275+1","v":1135},"Ф 22 мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1276+1","v":1136},"Ф 28 мм",null,null,null,null,null,"шт",null,null,0]
[0,1137,"Ф 35 мм",null,null,null,null,null,"шт",null,null,0]
[0,1138,"Ф 42 мм",null,null,null,null,null,"шт",null,null,0]
[0,1139,"Ф 54 мм",null,null,null,null,null,"шт",null,null,0]
[0,1140,"Ф 67 мм",null,null,null,null,null,"шт",null,null,0]
[0,1141,"Ф 89 мм",null,null,null,null,null,"шт",null,null,0]
[0,1142,"Ф 102 мм",null,null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1284:J1287)","v":0},"Паук",null,null,null,null,null,"Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1283+1","v":1143},"FB-16x6.35/4",null,"Ф16   Ф6.35   4",null,null,null,"шт",null,null,0]
[0,{"$f":"B1285+1","v":1144},"FB-16x6.35/6",null,"Ф16   Ф6.35   6",null,null,null,"шт",null,null,0]
[0,{"$f":"B1286+1","v":1145},"FB-16x6.35/9",null,"Ф16   Ф6.35   9",null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1288:J1290)","v":0},"Рефнет  ",null,null,null,null,null,"Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1287+1","v":1146},"RMB-BY53E",null,"16/12 - 12/10 - 12/10мм",null,null,null,"компл",null,null,0]
[{"$f":"J1290","v":0},{"$f":"B1289+1","v":1147},"RMB-BY103E",null,"22/16 - 19/12 - 19/12мм",null,null,null,"компл",null,null,0]
[{"$f":"SUM(J1291:J1393)","v":0},"Медные фитинги ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"SUM(J1292:J1298)","v":0},"№","Модель","Толщина стенки мм.","Отводы 45° ELBOW CxC ",null,"Кол-во штук  в коробка","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1290+1","v":1148},"      7/8-22mm",0.84,null,null,null,50,"шт",null,null,0]
[0,{"$f":"B1293+1","v":1149},"       1-1/8-28mm",1.02,null,null,null,10,"шт",null,null,0]
[0,{"$f":"B1294+1","v":1150},"    1-3/8-35mm",1.1200000000000001,null,null,null,10,"шт",null,null,0]
[0,{"$f":"B1295+1","v":1151},"    1 5/8-42mm",1.3,null,null,null,5,"шт",null,null,0]
[0,{"$f":"B1296+1","v":1152},"      2 1/8-54mm",1.5,null,null,null,24,"шт",null,null,0]
[0,{"$f":"B1297+1","v":1153}," 2 5/8-67mm",1.7,null,null,null,12,"шт",null,null,0]
[{"$f":"SUM(J1299:J1313)","v":0},"№","Модель. Стандартный","Толщина стенки мм.","Отводы 90° ELBOW  CxC",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1298+1","v":1154},"    1/4-6.35mm",null,null,null,null,100,"шт",null,null,0]
[0,{"$f":"B1300+1","v":1155},"    3/8-10mm",null,null,null,null,200,"шт",null,null,0]
[0,{"$f":"B1301+1","v":1156},"      1/2-12mm",0.66,null,null,2000,100,"шт",null,null,0]
[0,{"$f":"B1302+1","v":1157},"    5/8-16mm",0.74,null,null,1000,100,"шт",null,null,0]
[0,{"$f":"B1303+1","v":1158},"       3/4-19mm",0.79,null,null,600,50,"шт",null,null,0]
[0,{"$f":"B1304+1","v":1159},"      7/8-22mm",0.84,null,null,400,25,"шт",null,null,0]
[0,{"$f":"B1305+1","v":1160},"1-25mm",null,null,null,null,10,"шт",null,null,0]
[0,{"$f":"B1306+1","v":1161},"       1 1/8-28mm",1.02,null,null,200,10,"шт",null,null,0]
[0,{"$f":"B1307+1","v":1162},"        1 3/8-35mm",1.1200000000000001,null,null,100,10,"шт",null,null,0]
[0,{"$f":"B1308+1","v":1163},"     1 5/8-42mm",1.3,null,null,70,5,"шт",null,null,0]
[0,{"$f":"B1309+1","v":1164},"        2 1/8-54mm",1.5,null,null,36,3,"шт",null,null,0]
[0,{"$f":"B1310+1","v":1165},"      2 5/8-67mm",1.7,null,null,20,2,"шт",null,null,0]
[0,{"$f":"B1311+1","v":1166},"   3 1/8-80mm",1.91,null,null,10,2,"шт",null,null,0]
[0,1167,"4 1/8    105mm",null,null,null,null,10,"шт",null,null,0]
[{"$f":"SUM(J1314:J1322)","v":0},"№","Модель. Удлиненный  FTGxC","Толщина стенки мм.","Отводы 90° STREET LONG ELBOW  наружн/внутр",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,{"$f":"J1314*K1314","v":0}]
[0,{"$f":"B1313+1","v":1168},"       5/8   16mm",0.74,null,null,null,50,"шт",null,null,0]
[0,{"$f":"B1315+1","v":1169},"       7/8   22mm",0.84,null,null,null,20,"шт",null,null,0]
[0,{"$f":"B1316+1","v":1170},"     1-1/8   28mm",1.02,null,null,null,10,"шт",null,null,0]
[0,1171,"    1-3/8   35mm",1.1200000000000001,null,null,null,5,"шт",null,null,0]
[0,1172,"      1-5/8   42mm",1.3,null,null,null,5,"шт",null,null,0]
[0,1173,"   2 1/8   54mm",1.5,null,null,null,14,"шт",null,null,0]
[0,1174,"    2 5/8   67mm",1.7,null,null,null,25,"шт",null,null,0]
[0,1175,"    3 1/8   80mm",1.91,null,null,null,15,"шт",null,null,0]
[{"$f":"SUM(J1323:J1332)","v":0},"№","Модель. Удлиненный","Толщина стенки мм.","Отводы 90° LONG ELBOW  CxC",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1322+1","v":1176},"       5/8-16mm",0.74,null,null,600,50,"шт",null,null,0]
[0,{"$f":"B1324+1","v":1177},"     3/4-19mm",0.79,null,null,400,50,"шт",null,null,0]
[0,{"$f":"B1325+1","v":1178},"       7/8-22mm",0.84,null,null,null,20,"шт",null,null,0]
[0,{"$f":"B1326+1","v":1179},"  1 1/8-28mm",1.02,null,null,null,10,"шт",null,null,0]
[0,1180,"   1 3/8-35mm",1.1200000000000001,null,null,null,5,"шт",null,null,0]
[0,1181," 1 5/8-42mm",1.3,null,null,null,5,"шт",null,null,0]
[0,1182,"          2 1/8-54mm",1.5,null,null,null,14,"шт",null,null,0]
[0,1183,"      2 5/8-67mm",1.7,null,null,12,2,"шт",null,null,0]
[0,1184,"      3 1/8-80mm",1.91,null,null,5,5,"шт",null,null,0]
[{"$f":"SUM(J1333:J1341)","v":0},"№","Модель. Возвратный изгиб","Толщина стенки мм.","Колено 180°  (Калач) CxC",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1332+1","v":1185},"     1/2-12mm",0.66,null,null,400,10,"шт",null,null,0]
[0,{"$f":"B1334+1","v":1186},"    5/8-16mm",0.74,null,null,200,10,"шт",null,null,0]
[0,1187,"     3/4-19mm",0.79,null,null,100,5,"шт",null,null,0]
[0,1188,"    7/8-22mm",0.84,null,null,80,5,"шт",null,null,0]
[0,1189,"    1 1/8-28mm",1.02,null,null,40,5,"шт",null,null,0]
[0,1190,"     1 3/8-35mm",1.1200000000000001,null,null,35,5,"шт",null,null,0]
[0,1191,"1 5/8-42mm",1.3,null,null,20,2,"шт",null,null,0]
[0,1192,"2 1/8-54mm",1.5,null,null,20,2,"шт",null,null,0]
[{"$f":"SUM(J1342:J1349)","v":0},"№","Модель. Mасленная петля","Толщина стенки мм.","P-TRAP  CxC",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1341+1","v":1193},"     5/8-16mm",0.74,null,null,100,10,"шт",null,null,0]
[0,{"$f":"B1343+1","v":1194}," 3/4-19mm",0.79,null,null,40,5,"шт",null,null,0]
[0,1195,"    7/8-22mm",0.84,null,null,25,5,"шт",null,null,0]
[0,1196,"    1 1/8-28mm",1.02,null,null,10,10,"шт",null,null,0]
[0,1197,"     1 3/8-35mm",1.1200000000000001,null,null,10,10,"шт",null,null,0]
[0,1198,"1 5/8-42mm",1.3,null,null,8,8,"шт",null,null,0]
[0,1199,"      2 1/8-54mm",1.5,null,null,3,3,"шт",null,null,0]
[{"$f":"SUM(J1350:J1362)","v":0},"№","Модель. Тройник","Толщина стенки мм.","TEE   CxCxC",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1349+1","v":1200},"1/4-6.35mm",null,null,null,null,100,"шт",null,null,0]
[0,{"$f":"B1351+1","v":1201},"3/8-10mm",null,null,null,null,100,"шт",null,null,0]
[0,{"$f":"B1352+1","v":1202},"     1/2-12mm",0.66,null,null,1000,100,"шт",null,null,0]
[{"$f":"J1354","v":0},1203,"             5/8-16mm",0.74,null,null,500,50,"шт",null,null,0]
[0,1204,"     7/8-22mm",0.84,null,null,200,25,"шт",null,null,0]
[0,1205,"    1 1/8-28mm",1.02,null,null,120,10,"шт",null,null,0]
[0,1206,"      1 3/8-35mm",1.1200000000000001,null,null,80,5,"шт",null,null,0]
[0,1207,"     1 5/8-42mm",1.3,null,null,40,5,"шт",null,null,0]
[0,1208,"          2 1/8   54mm",1.5,null,null,25,5,"шт",null,null,0]
[0,1209,"     2 5/8   67mm",1.7,null,null,12,2,"шт",null,null,0]
[0,1210,"     3 1/8   80mm",1.91,null,null,null,16,"шт",null,null,0]
[0,1211,"     4 1/8   105mm",null,null,null,null,8,"шт",null,null,0]
[{"$f":"SUM(J1363:J1375)","v":0},"№","Модель. Муфты","Толщина стенки мм.","COUPLINGSw/STOP  CxC  DIMPLE",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1362+1","v":1212}," 1/4-6,35mm",null,null,null,null,100,"шт",null,null,0]
[0,{"$f":"B1364+1","v":1213}," 3/8-10mm",null,null,null,null,100,"шт",null,null,0]
[0,{"$f":"B1365+1","v":1214},"       1/2-12mm",0.66,null,null,null,100,"шт",null,null,0]
[0,{"$f":"B1366+1","v":1215},"  5/8-16mm",0.74,null,null,null,100,"шт",null,null,0]
[0,1216,"       7/8-22mm",0.84,null,null,500,50,"шт",null,null,0]
[0,1217,"      1-1/8-28mm",1.02,null,null,250,25,"шт",null,null,0]
[0,1218,"    1-3/8-35mm",1.1200000000000001,null,null,null,25,"шт",null,null,0]
[0,1219,"     1-5/8-42mm",1.3,null,null,120,10,"шт",null,null,0]
[0,1220,"  2 1/8-54mm",1.5,null,null,70,10,"шт",null,null,0]
[0,1221,"       2-5/8-67mm",1.7,null,null,40,5,"шт",null,null,0]
[0,1222,"        3 1/8-80mm",1.91,null,null,null,48,"шт",null,null,0]
[0,1223,"        4-1/8-105mm",null,null,null,null,5,"шт",null,null,0]
[{"$f":"SUM(J1376:J1389)","v":0},"№","Модель. Муфты переходные","Толщина стенки мм.","REDUCING COULINGw/STOP  CxC",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1375+1","v":1224},"  7/8x5/8    22x16мм       ",0.84,null,null,null,50,"шт",null,null,0]
[0,{"$f":"B1377+1","v":1225},"1 1/8x7/8       28x22мм              ",1.02,null,null,null,20,"шт",null,null,{"$f":"J1378*K1378","v":0}]
[0,1226,"1 3/8x1 1/8     35x28мм          ",1.1200000000000001,null,null,null,10,"шт",null,null,0]
[0,1227,"   1 5/8x1 3/8     42х35мм ",1.1200000000000001,null,null,200,10,"шт",null,null,0]
[0,1228,"     2 1/8x1 3/8     54x35мм",1.3,null,null,null,5,"шт",null,null,0]
[0,1229,"     2 1/8x1 5/8     54x42мм",1.3,null,null,100,5,"шт",null,null,0]
[0,1230,"    2 5/8x1 3/8    67x35мм",1.7,null,null,null,2,"шт",null,null,0]
[0,1231,"     2 5/8x1 1/8    67x28мм",1.7,null,null,null,2,"шт",null,null,0]
[0,1232,"  2 5/8x2 1/8    67x54мм  ",1.7,null,null,null,5,"шт",null,null,0]
[0,1233,"     3 1/8x2 5/8     80x67мм",1.91,null,null,null,1,"шт",null,null,0]
[0,1234,"  4 1/8x2 1/8    105x54мм  ",null,null,null,null,1,"шт",null,null,0]
[0,1235,"  4 1/8x2 5/8    105x67мм  ",null,null,null,null,1,"шт",null,null,0]
[0,1236,"  4 1/8x3 1/8    105x80мм  ",null,null,null,null,1,"шт",null,null,0]
[{"$f":"SUM(J1390:J1393)","v":0},"№","Модель. Медные заглушки","Толщина стенки мм.","CAP",null,"Кол-во штук  в коробке","Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1389+1","v":1237},"HL-40CAP02    Q3/8-10mm",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1391+1","v":1238},"3 1/8   80mm",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1392+1","v":1239},"4 1/8   105mm",null,null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1394:J1452)","v":0},"Изоляции  трубные  ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1394","v":0},"№","Размер (Ф мм).","Кол-во в упаковке",null,null,null,"Кол-во в упаковке","Ед. Изм.",null,null,0]
[0,{"$f":"B1393+1","v":1240},"6х6       ",null,null,null,null,486,"м",null,null,0]
[0,{"$f":"B1396+1","v":1241},"6х10     ",null,null,null,null,378,"м",null,null,0]
[0,{"$f":"B1397+1","v":1242},"6х12        ",null,null,null,null,342,"м",null,null,0]
[0,{"$f":"B1398+1","v":1243},"6х15      ",null,null,null,null,270,"м",null,null,0]
[0,{"$f":"B1399+1","v":1244},"6х18         ",null,null,null,null,234,"м",null,null,0]
[0,{"$f":"B1400+1","v":1245},"6х22",null,null,null,null,198,"м",null,null,0]
[0,{"$f":"B1401+1","v":1246},"6х25",null,null,null,null,164,"м",null,null,0]
[0,1247,"6х28",null,null,null,null,132,"м",null,null,0]
[0,1248,"6х35",null,null,null,null,120,"м",null,null,0]
[0,1249,"6х42",null,null,null,null,108,"м",null,null,0]
[0,1250,"9х6",null,null,null,null,342,"м",null,null,0]
[0,1251,"9х10",null,null,null,null,270,"м",null,null,0]
[0,1252,"9х12",null,null,null,null,234,"м",null,null,0]
[0,1253,"9х15",null,null,null,null,198,"м",null,null,0]
[0,1254,"9х18",null,null,null,null,180,"м",null,null,0]
[0,1255,"9х22",null,null,null,null,162,"м",null,null,0]
[0,1256,"9х28      ",null,null,null,null,108,"м",null,null,0]
[0,1257,"9х35      ",null,null,null,null,96,"м",null,null,0]
[0,1258,"9х42",null,null,null,null,88,"м",null,null,0]
[0,1259,"9х60   ",70,null,null,null,56,"м",null,null,0]
[0,1260,"9х76 ",null,null,null,null,48,"м",null,null,0]
[{"$f":"J1417","v":0},1261,"9х89",null,null,null,null,42,"м",null,null,0]
[0,1262,"9х114",null,null,null,null,28,"м",null,null,0]
[0,1263,"13х12",null,null,null,null,162,"м",null,null,0]
[0,1264,"13х15",138,null,null,null,144,"м",null,null,0]
[0,1265,"13х18",null,null,null,null,126,"м",null,null,0]
[0,1266,"13х22",100,null,null,null,null,"м",null,null,0]
[0,1267,"13х28",80,null,null,null,84,"м",null,null,0]
[0,1268,"13х35",60,null,null,null,72,"м",null,null,0]
[0,1269,"13х42",50,null,null,null,56,"м",null,null,0]
[0,1270,"13х60      ",null,null,null,null,40,"м",null,null,0]
[0,1271,"13х76     (67mm)",40,null,null,null,null,"м",null,null,0]
[0,1272,"13х89     (80mm)",null,null,null,null,30,"м",null,null,0]
[0,1273,"13х114     (105mm)",null,null,null,null,24,"м",null,null,0]
[0,1274,"19х22",null,null,null,null,72,"м",null,null,0]
[0,1275,"19х28",null,null,null,null,60,"м",null,null,0]
[0,1276,"19х35",null,null,null,null,48,"м",null,null,0]
[0,1277,"19х42",null,null,null,null,40,"м",null,null,0]
[0,1278,"19х60     (54mm)",null,null,null,null,32,"м",null,null,0]
[0,1279,"19х76     (67mm)",32,null,null,null,null,"м",null,null,0]
[0,1280,"19х89     (80mm)",24,null,null,null,24,"м",null,null,0]
[0,1281,"19х114     (105mm)","24-18",null,null,null,16,"м",null,null,0]
[0,1282,"Клей  для листовой изоляции  3кг",null,null,null,null,6,"шт",null,null,0]
[0,1283,"Листовая изоляция  9мм х 1000мм   STD   ",null,null,"Кол-во в рулоне 20-м2",null,20,"рул",null,null,0]
[0,1284,"Листовая изоляция  13мм х 1000мм   STD   ",null,null,"Кол-во в рулоне 14-м2",null,14,"рул",null,null,0]
[0,1285,"Листовая изоляция  19мм х 1000мм   STD   ",null,null,"Кол-во в рулоне 10-м2",null,10,"рул",null,null,{"$f":"J1441*K1441","v":0}]
[0,1286,"Листовая изоляция  9мм х 1000мм   KY   самоклеющаяся   ",null,null,"Кол-во в рулоне 20-м2",null,20,"рул",null,null,0]
[0,1287,"Листовая изоляция  13мм х 1000мм   KY   самоклеющаяся   ",null,null,"Кол-во в рулоне 14-м2",null,14,"рул",null,null,0]
[0,1288,"Звукоизоляция  30мм   STD  не самоклеющаяся   ",null,null,"Кол-во    2-м2       ",null,1,"шт",null,null,0]
[0,1289,"Изоляционный бант 3мм* 50мм* 15мт самоклеющийся",null,null,"Кол-во в коробке 20-24-рулон",null,20,"рул",null,null,0]
[0,1290,"Бант PVC 0.15мм x 45мм x 15мт не самоклеющаяся (белый)",null,null,"Кол-во в коробке 100-рулон",null,100,"рул",null,null,0]
[0,1291,"Бант PVC 0.15мм x 45мм x 15мт не самоклеющаяся (бежевый)",null,null,null,null,null,"рул",null,null,0]
[0,1292,"Бант   PVC  0.15mm x 45mm x 15мт  самоклеющаяся  белый",null,null,null,null,null,"рул",null,null,0]
[0,1293,"Бант   PVC  0.15mm x 45mm x 15мт  самоклеющаяся  черный",null,null,null,null,null,"рул",null,null,0]
[0,1294,"Спиральный шланг 5/8\"  16мм",null,null,"в рулоне 50 м",null,50,"рул",null,null,0]
[0,1295,"Спиральный шланг 3/4\"  19мм",null,null,"в рулоне 50 м",null,null,"рул",null,null,0]
[0,1296,"Спиральный шланг 1\"  25мм",null,null,"в рулоне 50 м",null,null,"рул",null,null,0]
[{"$f":"SUM(J1453:J1465)","v":0},"Двери и комплектующие для холодильных дверей ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1453","v":0},"№","Наименование",null,null,null,null,"Кол-во в упаковке","Ед.изм",null,null,0]
[0,{"$f":"B1452+1","v":1297},"Шторы для дверей (прозрачные) 200 х 2-мм                                   ",null,null,null,null,null,"рул",null,null,0]
[0,{"$f":"B1455+1","v":1298},"Шторы для дверей (прозрачные) 300 х 2-мм                    ",null,null,null,null,null,"рул",null,null,0]
[0,{"$f":"B1456+1","v":1299},"Шторы для дверей (прозрачные) 300 х 3-мм          ",null,null,null,null,null,"рул",null,null,0]
[0,1300,"Планка для штор НЖ сталь L= 1м   (компл. 5 звеньев 200мм)                ",null,null,null,null,25,"компл",null,null,0]
[0,1301,"Вакуумный клапан для холодильной камеры    I-500      до 200mm         ",null,null,null,null,null,"шт",null,null,0]
[0,1302,"Замок для холодильной камеры    I-266-02      до 120mm          ",null,null,null,null,null,"шт",null,null,0]
[0,1303,"Дверь  Световой проем: 90*190*8см  Наружный размер по косяку    94*203 см  без подогрева  право",null,null,null,null,1,"шт",null,null,0]
[0,1304,"Дверь  Световой проем: 90*190*8см                         Наружный размер по косяку    94*203 см               без подогрева          лево",null,null,null,null,null,"шт",null,null,0]
[0,1305,"Дверь  Световой проем: 90*190*10см                      Наружный размер по косяку     94*203 см               с подогревом           право",null,null,null,null,null,"шт",null,null,0]
[0,1306,"Дверь  Световой проем: 90*190*10см                      Наружный размер по косяку     94*203 см               с подогревом           лево",null,null,null,null,null,"шт",null,null,0]
[0,1307,"Дверь откатная Световой проем: 210*250*8см        левое открывание     Наружный размер по косяку  220*255 см",null,null,null,null,null,"компл",null,null,0]
[{"$f":"SUM(J1466:J1535)","v":0},"Инструменты   ",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1466","v":0},"№","Модель",null,"Параметры",null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1465+1","v":1308},"AD-78",null,"переходник с 1/2 - 5/16 с нипелем",null,null,null,"шт",null,null,0]
[0,{"$f":"B1468+1","v":1309},"CT-351",null,"Расческа пластиковая",null,null,null,"шт",null,null,0]
[0,1310,"CT-352",null,"Расческа  металическая",null,null,null,"шт",null,null,0]
[0,1311,"N100M-09     35мм",null,"Насадка для труборасширителя",null,null,null,"шт",null,null,0]
[0,1312,"N100M-11     42мм",null,null,null,null,null,"шт",null,null,0]
[0,1313,"N100M-54мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1473+1","v":1314},"VE-115N",null,"Вакуумный насос  1.8м3/час",null,"масла 250-г",null,"шт",null,null,0]
[0,1315,"VE-125N",null,"Вакуумный насос  2.5м3/час",null,"масла 250-г",null,"шт",null,null,0]
[0,1316,"VE-135N",null,"Вакуумный насос  3.5м3/час",null,"масла 250-г",null,"шт",null,null,0]
[0,1317,"VE-160N",null,"Вакуумный насос  6.0м3/час",null,"масла 415-г",null,"шт",null,null,0]
[0,1318,"VE-225N",null,"Вакуумный насос  2.5м3/час",null,"масла 200-г",null,"шт",null,null,0]
[{"$f":"J1479","v":0},1319,"VE-245N",null,"Вакуумный насос  4.5м3/час",null,"масла 325-г",null,"шт",null,null,0]
[0,1320,"VE-260N",null,"Вакуумный насос  6.0м3/час",null,"масла 580-г",null,"шт",null,null,0]
[0,1321,"VE-280N",null,"Вакуумный насос  8.0м3/час",null,"масла 500-г",null,"шт",null,null,0]
[0,1322,"VE-2100N",null,"Вакуумный насос  10.0м3/час",null,"масла 590-г",null,"шт",null,null,0]
[0,1323,"PUMPS 68 - 500ML",null,"Вакуумные масла ERRECOM",null,null,null,"кан.",null,null,0]
[0,1324,"PUMPS 68 - 1L",null,null,null,null,null,"кан.",null,null,0]
[0,1325,"VRR12L-OS",null,"Станция откачки фреона   3/4 HP",null,"14.2 кг",null,"шт",null,null,0]
[0,1326,"VRR24L-OS",null,"Станция откачки фреона   1 HP",null,"14.7 кг",null,"шт",null,null,0]
[0,1327,"VMG-2-R32",null,"Манифолд со шлангом   3x120 см   R32                  ",null,null,null,"компл",null,null,0]
[0,1328,"VMG-2-R32-B-03",null,"Манифолд  3x120 см   R32, R407, R410, R134                  ",null,null,null,"компл",null,null,0]
[0,1329,"VMG-2-1234yf",null,"Манифолд со шлангом   3x150 см   1234yf                  ",null,null,null,"компл",null,null,0]
[0,1330,"VMG-2-R600-B",null,"Манифолд со шлангом   3x120 см   R600, R290 ",null,null,null,"компл",null,null,0]
[0,1331,"VMG-2-R600-B-03",null,"Манифолд  R600, R290 ",null,null,null,"компл",null,null,0]
[0,1332,"VMG-2-R22-B",null,"Манифолд со шлангом   3x120 см   R404, 407, 134, 22 ",null,null,null,"компл",null,null,0]
[0,1333,"VMG-2-R22-B-03",null,"Манифолд   R404, 407, 134, 22 ",null,null,null,"компл",null,null,0]
[0,1334,"VMG-2-R410A-B",null,"Манифолд со шлангом   3x120 см   R410, 407, 134, 22 ",null,null,null,"компл",null,null,0]
[0,1335,"VMG-2-R410A-B-03",null,"Манифолд   R410, 407, 134, 22 ",null,null,null,"компл",null,null,0]
[0,1336,"VMG-1-S-H",null,"Манифолд  ",null,null,null,"компл",null,null,0]
[0,1337,"VMG-1-S-L",null,"Манифолд  ",null,null,null,"компл",null,null,0]
[0,1338,"VDG-1",null,"Манифолд электронный  R32, 410, 22, 1234yf, 134",null,null,null,"компл",null,null,0]
[0,1339,"VDG-2-S1",null,"Манифолд электронный со шлангом  3х150 см   R22, 134, 1234yf, 290, 404, 407, 410, 32, 507",null,null,null,"компл",null,null,0]
[0,1340,"VHF-A",null,"Переходник для заправки автокондиционера",null,null,null,"шт",null,null,0]
[0,1341,"VHF-SY",null,"Переходник для заправки автокондиционера",null,null,null,"шт",null,null,0]
[0,1342,"R410A",null,"Шланг для манифолда  3х150 см   R410A",null,null,null,"компл",null,null,0]
[0,1343,"R22",null,"Шланг для манифолда  3х120 см   R22",null,null,null,"компл",null,null,{"$f":"J1503*K1503","v":0}]
[0,1344,"R22",null,"Шланг для манифолда  3х180 см   R22",null,null,null,"компл",null,null,0]
[0,1345,"CV01",null,"Кран заправочный прямой",null,null,null,"шт",null,null,0]
[0,1346,"CV02",null,"Кран заправочный угловой 45с",null,null,null,"шт",null,null,0]
[0,1347,"V07",null,"Переходник  1/4 - 5/16",null,null,null,"шт",null,null,0]
[0,1348,"V08",null,"Переходник  5/16 - 1/4",null,null,null,"шт",null,null,0]
[0,1349,"VES-50A",null,"Весы для хладагента  50кг",null,null,null,"шт",null,null,0]
[0,1350,"VES-50B",null,"Весы для хладагента  50кг",null,null,null,"шт",null,null,0]
[0,1351,"VFT-808-IN",null,"Развальцовка 1/4, 5/16, 3/8, 1/2, 5/8, 3/4",null,null,null,"шт",null,null,0]
[0,1352,"VFT-808-MI",null,"Развальцовка 1/4, 5/16, 3/8, 1/2, 5/8, 3/4   -  6, 8, 10, 12, 16, 19мм",null,null,null,"шт",null,null,0]
[0,1353,"VFT-808-MIS    (VTC-32)",null,"Развальцовка 1/4, 5/16, 3/8, 1/2, 5/8, 3/4   -  6, 8, 10, 12, 16, 19мм",null,null,null,"шт",null,null,0]
[0,1354,"WK-1012-M ",null,"Трубогиб 10-12mm   (180С)",null,null,null,"шт",null,null,0]
[0,1355,"VBT-2 1/2 12мм",null,"Трубогиб 1/2  12mm   (180С)",null,null,null,"шт",null,null,0]
[0,1356,"VBT-3 5/8 16мм",null,"Трубогиб 5/8  16mm   (180С)",null,null,null,"шт",null,null,0]
[0,1357,"VBT-4 3/4 19мм",null,"Трубогиб 3/4  19mm   (180С)",null,null,null,"шт",null,null,0]
[0,1358,"VBT-5 7/8 22мм",null,"Трубогиб 7/8  22mm   (180С)",null,null,null,"шт",null,null,0]
[0,1359,"WK-202-06",null,"Трубогиб  Пружинного типа  3/8",null,null,null,"шт",null,null,0]
[0,1360,"WK-202-08",null,"Трубогиб  Пружинного типа  1/2",null,null,null,"шт",null,null,0]
[0,1361,"WK-202-10",null,"Трубогиб  Пружинного типа  5/8",null,null,null,"шт",null,null,0]
[0,1362,"WK-202-12",null,"Трубогиб  Пружинного типа  3/4",null,null,null,"шт",null,null,0]
[0,1363,"VHE-29E",null,"Труборасширитель гидравлический  3/8, 1/2, 5/8, 3/4, 7/8, 1, 1-1/8",null,null,null,"шт",null,null,0]
[0,1364,"VHE-42E",null,"Труборасширитель гидравлический  3/8, 1/2, 5/8, 3/4, 7/8, 1, 1-1/8, 1-1/4, 1-3/8, 1-1/2, 1-5/8",null,null,null,"шт",null,null,0]
[0,1365,"VST-22B",null,"Труборасширитель  1/4, 5/16, 3/8, 1/2, 5/8, 3/4, 7/8 - 6, 8, 10, 12, 16, 19, 22мм",null,null,null,"шт",null,null,0]
[0,1366,"VTC-19  1/8-3/4,  3-19мм",null,"Труборез  3-19 мм",null,null,null,"шт",null,null,0]
[0,1367,"VTC-32  1/8-1-1/4,  4-32мм",null,"Труборез  4-32 мм",null,null,null,"шт",null,null,{"$f":"J1527*K1527","v":0}]
[0,1368,"VTC-42  1/4-1-5/4,  6-42мм",null,"Труборез  6-42 мм",null,null,null,"шт",null,null,0]
[0,1369,"VTT-5",null,"Гратосниматель ",null,null,null,"шт",null,null,{"$f":"J1529*K1529","v":0}]
[0,1370,"VRT-201",null,"Ключ трещоточный",null,null,null,"шт",null,null,0]
[0,1371,"VTB-5A",null,"Набор инструментов V-I115S-M, VFT-808-I, VTC-32, VTT-5, VMG-2-R410A, VST-22",null,null,null,"шт",null,null,0]
[0,{"$f":"B1531+1","v":1372},"VTB-5B-II",null,"Набор инструментов VFT-808-I, VTC-32, VTC-19, VMG-2-R410A, VTT-5, V01 V08",null,null,null,"шт",null,null,0]
[0,1373,"VMC-1",null,"Мультимерт измерительный прибор  (амперметр)",null,null,null,"шт",null,null,0]
[0,1374,"VIT-300S",null,"Термометр инфракрасный",null,null,null,"шт",null,null,0]
[0,1375,"VML-1",null,"Детектор утечки фреона",null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1536:J1566)","v":0},"Электронные цифровые  микропроцессоры   (Италия)",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1536","v":0},"№","Модель",null,"Параметры",null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1535+1","v":1376},"PJEZS0H000  CAREL   (цена без датчика)",null,"230v -58/+320°C  1-релейный",null,null,null,"шт",null,null,0]
[0,{"$f":"B1538+1","v":1377},"PJEZC0H000  CAREL  (цена без датчиков)",null,"230v -58/+320°С 3- релейный",null,null,null,"шт",null,null,0]
[0,{"$f":"B1539+1","v":1378},"WE00C2HN00  SMARTCELLA  CAREL",null,"230v -58/+320°С 4- релейный",null,null,null,"шт",null,null,0]
[0,1379,"IDPlus 961 RUS         Eliwell",null,"230v -58/+320°C  1-релейный",null,null,null,"шт",null,null,0]
[0,1380,"IDPlus 974 RUS         Eliwell",null,"230v -58/+320°С 3- релейный",null,null,null,"шт",null,null,0]
[{"$f":"J1543","v":0},1381,"PW3P000TE000  CAREL",null,"Блок диспетчеризации ",null,null,null,"шт",null,null,0]
[0,1382,"IROPZ48505  CAREL (RS485 адаптер)",null," Для систем мониторинга",null,null,null,"шт",null,null,0]
[0,1383,"NTC 015 HP00   CAREL",null," Датчик для микропроцессора ",null,"УПК 10 шт",null,"шт",null,null,0]
[0,1384,"ACU5  CAREL  24V                                           CABEL KIT PANEL 100CM",null,"U20R00MRK0280  Компьютер контроля управления централизованной системой.  (5 групп настройки).     Кабель UCHCONP010 PANEL для ACU5  ",null,null,null,"компл",null,null,0]
[0,1385,"ACUD5LN  CAREL  24V                                           CABEL KIT PANEL 100CM",null,"U20R00MRK0290  Компьютер контроля управления централизованной системой.  (6 групп настройки).     Кабель UCHCONP010 DIN для ACUD5LN",null,null,null,"компл",null,null,0]
[0,1386,"PRK300S3FO  CAREL",null,"Компьютер контроля управления централизованной системой.  (7 групп настройки). ",null,null,null,"шт",null,null,0]
[0,1387,"PRK300L3F0  CAREL",null,"Компьютер контроля управления централизованной системой.  (18 групп настройки). ",null,null,null,"шт",null,null,0]
[0,1388,"TRADRFE 240  CAREL",null,"Трансформатор 230/24  для Контроллера ",null,null,null,"шт",null,null,0]
[0,1389,"SPKT0033P1   0 - 34.5 бар  CAREL",null,"Датчик высокого давления для контроллера ",null,null,null,"шт",null,null,0]
[0,1390,"SPKT00E3P1   1 - 12.8 бар  CAREL",null,"Датчик низкого давления для контроллера ",null,null,null,"шт",null,null,0]
[0,1391,"SPKC002311  CAREL",null,"Соединительный провод для датчика ",null,null,null,"шт",null,null,0]
[0,1392,"ETC-961",null,"230v -58/+320°C  1-релейный",null,null,null,"шт",null,null,0]
[0,{"$f":"B1554+1","v":1393},"ETC-974",null,"230v -58/+320°С 3- релейный",null,null,null,"шт",null,null,0]
[0,1394,"NA704L       (от 1-40А)",null,"контроллер защиты по току(А) ",null,null,null,"шт",null,null,0]
[0,1395,"NA708L      (от 2-80А)",null,null,null,null,null,"шт",null,null,0]
[0,1396,"i-141-05  (лампа 16-А)              ",null," УПК 200 шт",null,null,null,"шт",null,null,0]
[0,1397,"i-141   (снежинка 16-А)            ",null,null,null,null,null,"шт",null,null,0]
[0,1398,"i-142   (0/1   16-А)                     ",null,null,null,null,null,"шт",null,null,{"$f":"J1560*K1560","v":0}]
[0,1399,"i-142-03   (вентилятор  16-А)    ",null,null,null,null,null,"шт",null,null,0]
[0,1400," I-478-02  (корпус два тумблера)",null,null,null,null,null,"шт",null,null,0]
[0,1401," I-478-05  (панель один тумблер)",null,null,null,null,null,"шт",null,null,0]
[0,1402," I-478-06  (панель два тумблера)",null,null,null,null,null,"шт",null,null,0]
[0,1403," I-481-01 (корпус для холодильной камеры)   ",null," УПК 30 шт",null,null,30,"шт",null,null,0]
[0,1404,"F2000   термостат -30 +30с             ",null," УПК 100 шт",null,null,100,"шт",null,null,0]
[{"$f":"SUM(J1567:J1594)","v":0}," Автоматы защиты двигателя Siemens",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1567","v":0},"№","Модель",null,"Параметры",null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1566+1","v":1405},"3RV2901-1A",null,"Дополнительный контакт автомата защиты двигателя NO/NC",null,null,2,"шт",null,null,0]
[0,{"$f":"B1569+1","v":1406},"3RV2011-1BA10",null," 1.4 - 2 A",null,null,1,"шт",null,null,0]
[0,{"$f":"B1570+1","v":1407},"3RV2011-1CA10",null," 1.8 - 2.5 A",null,null,null,"шт",null,null,0]
[0,{"$f":"B1571+1","v":1408},"3RV2011-1EA10",null," 2.8 - 4 A",null,null,null,"шт",null,null,0]
[0,1409,"3RV2011-1FA10",null," 3.5 - 5 A",null,null,null,"шт",null,null,0]
[0,1410,"3RV2011-1GA10",null," 4.5 - 6.3 A",null,null,null,"шт",null,null,0]
[0,1411,"3RV2011-1HA10",null," 5.5 - 8 A",null,null,null,"шт",null,null,0]
[0,1412,"3RV2011-1JA10",null," 7 - 10 A",null,null,null,"шт",null,null,0]
[0,1413,"3RV2011-1KA10",null," 9 - 12.5 A",null,null,null,"шт",null,null,0]
[0,1414,"3RV2011-4AA10",null," 10 - 16 A",null,null,null,"шт",null,null,0]
[0,1415,"3RV2021-4BA10",null," 13 - 20 A",null,null,null,"шт",null,null,0]
[0,1416,"3RV2021-4CA10",null," 16 - 22 A",null,null,null,"шт",null,null,0]
[0,1417,"3RV2021-4DA10",null," 18 - 25 A",null,null,null,"шт",null,null,0]
[0,1418,"3RV2021-4NA10",null," 23 - 28 A",null,null,null,"шт",null,null,0]
[0,1419,"3RV2021-4EA10",null," 27 - 32 A",null,null,null,"шт",null,null,0]
[0,1420,"3RV2021-4PA10",null," 30 - 36 A",null,null,null,"шт",null,null,0]
[0,1421,"3RV2031-4UA10",null," 32 - 40 A",null,null,null,"шт",null,null,0]
[0,1422,"3RV2031-4VA10",null," 35 - 45 A",null,null,null,"шт",null,null,0]
[0,1423,"3RV2031-4WA10",null," 42 - 52 A",null,null,null,"шт",null,null,0]
[0,1424,"3RV2031-4XA10",null," 49 - 59 A",null,null,null,"шт",null,null,0]
[0,1425,"3RV2031-4JA10",null," 54 - 65 A",null,null,null,"шт",null,null,0]
[0,1426,"3RV2031-4RA10",null," 70 - 80 A",null,null,null,"шт",null,null,0]
[0,1427,"3RV2041-4JA10",null," 45 - 63 A",null,null,null,"шт",null,null,0]
[0,1428,"3RV2041-4RA10",null," 65 - 84 A",null,null,null,"шт",null,null,0]
[0,1429,"3RV2041-4MA10",null," 80 - 100 A",null,null,null,"шт",null,null,0]
[0,1430,"3UA59 00-2P",null,"50-63A",null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1595:J1606)","v":0},"Автоматы защиты двигателя  CHINT",null,null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1594+1","v":1431}," NS2-25X",null,"1,6-2,5A",null,null,1,"шт",null,null,0]
[0,{"$f":"B1596+1","v":1432}," NS2-25X",null,"2,5-4A",null,null,null,"шт",null,null,0]
[0,{"$f":"B1597+1","v":1433}," NS2-25X",null,"4-6,3A",null,null,null,"шт",null,null,0]
[0,1434," NS2-25X",null,"6-10A",null,null,null,"шт",null,null,0]
[0,1435," NS2-25X",null,"9-14A",null,null,null,"шт",null,null,0]
[0,1436," NS2-25X",null,"13-18A",null,null,null,"шт",null,null,0]
[0,1437," NS2-25X",null,"17-23A",null,null,null,"шт",null,null,0]
[0,1438," NS2-25X",null,"20-25A",null,null,null,"шт",null,null,0]
[0,1439," NS2-80B",null,"16-25A",null,null,null,"шт",null,null,0]
[0,1440," NS2-80B",null,"25-40A",null,null,null,"шт",null,null,0]
[{"$f":"J1606","v":0},1441," NS2-80B",null,"40-63A",null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1607:J1633)","v":0},"Автоматы Siemens",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1607","v":0},"№","Модель","Параметры (1 F)",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1606+1","v":1442},"5SL6106-7YA","C 1x6 A",null,null,null,12,"шт",null,null,0]
[0,{"$f":"B1609+1","v":1443},"5SL6110-7YA","C 1x10 A",null,null,null,null,"шт",null,null,0]
[0,1444,"5SL6116-7YA","C 1x16 A",null,null,null,null,"шт",null,null,0]
[0,1445,"5SL6120-7YA","C 1x20 A",null,null,null,null,"шт",null,null,0]
[0,1446," 5SL6125-7YA","  C 1x25 A",null,null,null,null,"шт",null,null,0]
[0,1447,"5SL6132-6YA","C 1x32 A",null,null,null,null,"шт",null,null,0]
[0,1448,"5SL6140-7YA","C 1x40 A",null,null,null,null,"шт",null,null,{"$f":"J1615*K1615","v":0}]
[0,1449,"5SL6150-7","C 1x50 A",null,null,null,null,"шт",null,null,0]
[0,1450,"5SL6163-7","C 1x63 A",null,null,null,null,"шт",null,null,0]
[0,1451,"5SP4180-7","C 1x80 A",null,null,null,6,"шт",null,null,0]
[0,1452,"5SP4191-7","C 1x100 A",null,null,null,null,"шт",null,null,0]
[0,1453,"5SP4192-7","C 1x125 A",null,null,null,null,"шт",null,null,0]
[0,1454,"5SL6310-7YA","C 3x10 A",null,null,null,4,"шт",null,null,0]
[0,1455,"5SL6316-7YA","C 3x16 A",null,null,null,null,"шт",null,null,0]
[0,1456,"5SL6320-7YA","C 3x20 A",null,null,null,null,"шт",null,null,0]
[0,1457,"5SL6325-7YA","C 3x25 A",null,null,null,null,"шт",null,null,0]
[0,1458,"5SL6332-7YA","C 3x32 A",null,null,null,null,"шт",null,null,0]
[0,1459,"5SL6340-7YA","C 3x40 A",null,null,null,null,"шт",null,null,0]
[0,1460,"5SL6350-7","C 3x50 A",null,null,null,null,"шт",null,null,0]
[0,1461,"5SL6363-7","C 3x63 A",null,null,null,null,"шт",null,null,0]
[0,1462,"3VM1080-3ED32-0AA0","C 3x80 A",null,null,null,1,"шт",null,null,0]
[0,1463,"3VM1010-3ED32-0AA0","C 3x100 A",null,null,null,null,"шт",null,null,0]
[0,1464,"5SP4392-7","C 3x125 A",null,null,null,null,"шт",null,null,0]
[0,1465,"3VM1116-3ED32-0AA0","C 3x160 A",null,null,null,null,"шт",null,null,0]
[0,1466,"3VM1220-3ED32-0AA0","C 3x200 A",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1634:J1661)","v":0},"Автоматы         CHINT",null,null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1633+1","v":1467},"DZ47-60  1P     4.5KA","C 1х6 А",null,null,null,12,"шт",null,null,0]
[0,{"$f":"B1635+1","v":1468},null,"C 1х10 А",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1636+1","v":1469},null,"C 1х16 А",null,null,null,null,"шт",null,null,0]
[0,1470,null,"C 1х20 А",null,null,null,null,"шт",null,null,0]
[0,1471,null,"C 1х25 А",null,null,null,null,"шт",null,null,0]
[0,1472,null,"C 1х32 А",null,null,null,null,"шт",null,null,0]
[0,1473,null,"C 1х40 А",null,null,null,null,"шт",null,null,0]
[0,1474,null,"C 1х50 А",null,null,null,null,"шт",null,null,0]
[0,1475,null,"C 1х63 А",null,null,null,null,"шт",null,null,0]
[0,1476,"NXB-125   1P       10KA","C 1х63 А",null,null,null,null,"шт",null,null,0]
[0,1477,null,"C 1х80 А",null,null,null,null,"шт",null,null,0]
[0,1478,null,"C 1х100 А",null,null,null,null,"шт",null,null,0]
[0,1479,"NXB-63S   3P    4.5KA","C 3х10 А",null,null,null,4,"шт",null,null,0]
[0,1480,null,"C 3х16 А",null,null,null,null,"шт",null,null,0]
[0,1481,null,"C 3х20 А",null,null,null,null,"шт",null,null,0]
[0,1482,null,"C 3х25 А",null,null,null,null,"шт",null,null,0]
[0,1483,null,"C 3х32 А",null,null,null,null,"шт",null,null,0]
[0,1484,null,"C 3х40 А",null,null,null,null,"шт",null,null,0]
[0,1485,null,"C 3х50 А",null,null,null,null,"шт",null,null,0]
[0,1486,null,"C 3х63 А",null,null,null,null,"шт",null,null,0]
[0,1487,"NXB-125G   3P    10KA","C 3х63 А",null,null,null,null,"шт",null,null,0]
[0,1488,"DZ158 3P     10KA","C 3х80 А",null,null,null,null,"шт",null,null,0]
[0,1489,null,"C 3х100 А",null,null,null,null,"шт",null,null,0]
[0,1490,null,"C 3х125 А",null,null,null,null,"шт",null,null,0]
[0,1491,"IM1-250S/3300   3P   25KA","C 3х160 А",null,null,null,1,"шт",null,null,0]
[0,1492,null,"C 3х200 А",null,null,null,null,"шт",null,null,0]
[0,1493,null,"C 3х250 А",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1662:J1676)","v":0},"Магнитные пускатели (Siemens)",null,null,null,null,null,null,null,null,null,0]
[{"$f":"A1662","v":0},"№","Модель","Параметры",null,null,null,"Кол-во в упаковке","Ед.изм.",null,null,0]
[0,{"$f":"B1661+1","v":1494},"3RT2015-1AP02","3-кВт   7-А    1-NO",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1664+1","v":1495},"3RT2016-1AP02","4-кВт    9-А      1-NO",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1665+1","v":1496},"3RT2017-1AP02","5.5-кВт    12-А     1-NO",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1666+1","v":1497},"3RT2018-1AP02","7.5-кВт   16-А    1-NO",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1667+1","v":1498},"3RT2026-1AP00","11-кВт   25-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[0,1499,"3RT2027-1AP00","15-кВт   32-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[{"$f":"J1670","v":0},1500,"3RT2028-1AP00","18.5-кВт   38-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[0,1501,"3RT2036-1AP00","22-кВт   51-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1671+1","v":1502},"3RT2037-1AP00","30-кВт   65-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[0,1503,"3RT2038-1AP00","37-кВт   80-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[0,1504,"3RT2046-1AP00","45-кВт   90-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[0,1505,"3RT2047-1AP00","55-кВт   110-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[0,1506,"3RT1055-6AP36","75-кВт   140-А   1NO+1NC",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1677:J1687)","v":0},"Контакторы магнитные   3P   CHINT",null,null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1676+1","v":1507},"NCH8-20/20","   1Р - 20А  2NO  ",null,null,null,8,"шт",null,null,0]
[0,{"$f":"B1678+1","v":1508},"NXC-12","   5.5kw    12A        1NO + 1NC ",null,null,null,1,"шт",null,null,{"$f":"J1679*K1679","v":0}]
[0,{"$f":"B1679+1","v":1509},"NXC-18","   7.5kw    18A        1NO + 1NC ",null,null,null,null,"шт",null,null,0]
[0,1510,"NXC-25","   11kw    25A        1NO + 1NC ",null,null,null,null,"шт",null,null,0]
[0,1511,"NXC-32","   15kw    32A        1NO + 1NC",null,null,null,null,"шт",null,null,0]
[0,1512,"NXC-50"," 22kw    50A        1NO + 1NC",null,null,null,null,"шт",null,null,0]
[0,1513,"NXC-65"," 30kw    65A        1NO + 1NC",null,null,null,null,"шт",null,null,0]
[0,1514,"NXC-85"," 37kw    85A        1NO + 1NC",null,null,null,null,"шт",null,null,0]
[0,1515,"NXC-100"," 45kw    100A        1NO + 1NC",null,null,null,null,"шт",null,null,0]
[0,1516,"NXC-120"," 55kw    120A        2NO + 2NC",null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1688:J1696)","v":0},"Устройства защиты",null,null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1687+1","v":1517},"NJYB3-8 AC380V    CHINT","Реле защиты фаз (диапазон посекундно и процентам)",null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1689+1","v":1518},"NTE8-10B     CHINT","Реле времени посекундное  (диапазон от 0.1 - до 10 сек)",null,null,null,12,"шт",null,null,0]
[0,1519,"NTE8-1HO     CHINT","Реле времени посекундное  (диапазон от 0.5 - до 5 сек)",null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1691+1","v":1520},"NTE8-480B     CHINT","Реле времени поминутное (диапазон от 0.5- до 8 мин)",null,null,null,null,"шт",null,null,0]
[0,1521,"МКC-05      ENTES","Реле защиты фаз (диапазон посекундно и процентам)",null,null,null,16,"шт",null,null,0]
[0,1522,"KRK-SKAD 04",null,null,null,null,10,"шт",null,null,0]
[0,1523,"Klemsan     P1-SA","Реле защиты фаз (диапазон  процентам)",null,null,null,null,"шт",null,null,0]
[0,1524,"MCB-7        ENTES","Реле времени посекундное  (диапазон 0.1-30 сек)",null,null,null,28,"шт",null,null,0]
[{"$f":"SUM(J1697:J1702)","v":0},"Корпуса электрощита",null,null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1696+1","v":1525},"        ЩИТ 400х300х180мм",null,null,null,null,1,"шт",null,null,0]
[0,{"$f":"B1698+1","v":1526},"        ЩИТ 600х400х200мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1699+1","v":1527},"        ЩИТ 800х600х200мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1700+1","v":1528},"        ЩИТ 1000х600х200мм",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1701+1","v":1529},"        ЩИТ 1200х800х250мм",null,null,null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1703:J1705)","v":0},"Виброопоры для агрегата",null,null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1702+1","v":1530},"WTG112-A       ",null,null,null,null,4,"шт",null,null,0]
[0,{"$f":"B1704+1","v":1531},"WTG006-C       ",null,null,null,null,4,"шт",null,null,0]
[{"$f":"SUM(J1706:J1707)","v":0},"Водяная помпа для кондиционера",null,null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1705+1","v":1532},"PC-24B",null,"Высота max. 10м.  V= до 24 л/час.",null,null,null,"шт",null,null,0]
[{"$f":"SUM(J1708:J1719)","v":0},"Стартовый конденсатор для ротационного компрессора",null,null,null,null,null,"Кол-во в упаковке","Ед. изм",null,null,0]
[0,{"$f":"B1707+1","v":1533},"20 μF",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1709+1","v":1534},"25 μF",null,null,null,null,null,"шт",null,null,0]
[0,{"$f":"B1710+1","v":1535},"30 μF",null,null,null,null,null,"шт",null,null,0]
[0,1536,"35 μF",null,null,null,null,null,"шт",null,null,0]
[0,1537,"40 μF",null,null,null,null,null,"шт",null,null,0]
[0,1538,"45 μF",null,null,null,null,null,"шт",null,null,0]
[0,1539,"50 μF",null,null,null,null,null,"шт",null,null,0]
[0,1540,"55 μF",null,null,null,null,null,"шт",null,null,0]
[0,1541,"60 μF",null,null,null,null,null,"шт",null,null,0]
[0,1542,"65 μF",null,null,null,null,null,"шт",null,null,0]
[0,1543,"70 μF",null,null,null,null,null,"шт",null,null,0]
[]
[null,null,"ИТОГО",null,null,null,null,null,null,null,null,{"$f":"SUM(L12:L1720)","v":0}]